 -- Copyright (C) 1991-2011 Altera Corporation
 -- Your use of Altera Corporation's design tools, logic functions 
 -- and other software and tools, and its AMPP partner logic 
 -- functions, and any output files from any of the foregoing 
 -- (including device programming or simulation files), and any 
 -- associated documentation or information are expressly subject 
 -- to the terms and conditions of the Altera Program License 
 -- Subscription Agreement, Altera MegaCore Function License 
 -- Agreement, or other applicable license agreement, including, 
 -- without limitation, that your use is for the sole purpose of 
 -- programming logic devices manufactured by Altera and sold by 
 -- Altera or its authorized distributors.  Please refer to the 
 -- applicable agreement for further details.
 -- 
 -- This is a Quartus II output file. It is for reporting purposes only, and is
 -- not intended for use as a Quartus II input file. This file cannot be used
 -- to make Quartus II pin assignments - for instructions on how to make pin
 -- assignments, please see Quartus II help.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- NC            : No Connect. This pin has no internal connection to the device.
 -- DNU           : Do Not Use. This pin MUST NOT be connected.
 -- VCCINT        : Dedicated power pin, which MUST be connected to VCC  (1.2V).
 -- VCCIO         : Dedicated power pin, which MUST be connected to VCC
 --                 of its bank.
 --					Bank 1:		3.3V
 --					Bank 2:		3.3V
 --					Bank 3:		3.3V
 --					Bank 4:		3.3V
 --					Bank 5:		3.3V
 --					Bank 6:		3.3V
 --					Bank 7:		3.3V
 --					Bank 8:		3.3V
 -- GND           : Dedicated ground pin. Dedicated GND pins MUST be connected to GND.
 --					It can also be used to report unused dedicated pins. The connection
 --					on the board for unused dedicated pins depends on whether this will
 --					be used in a future design. One example is device migration. When
 --					using device migration, refer to the device pin-tables. If it is a
 --					GND pin in the pin table or if it will not be used in a future design
 --					for another purpose the it MUST be connected to GND. If it is an unused
 --					dedicated pin, then it can be connected to a valid signal on the board
 --					(low, high, or toggling) if that signal is required for a different
 --					revision of the design.
 -- GND+          : Unused input pin. It can also be used to report unused dual-purpose pins.
 --					This pin should be connected to GND. It may also be connected  to a
 --					valid signal  on the board  (low, high, or toggling)  if that signal
 --					is required for a different revision of the design.
 -- GND*          : Unused  I/O  pin. Connect each pin marked GND* directly to GND
 --           	    or leave it unconnected.
 -- RESERVED      : Unused I/O pin, which MUST be left unconnected.
 -- RESERVED_INPUT    : Pin is tri-stated and should be connected to the board.
 -- RESERVED_INPUT_WITH_WEAK_PULLUP    : Pin is tri-stated with internal weak pull-up resistor.
 -- RESERVED_INPUT_WITH_BUS_HOLD       : Pin is tri-stated with bus-hold circuitry.
 -- RESERVED_OUTPUT_DRIVEN_HIGH        : Pin is output driven high.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- Pin directions (input, output or bidir) are based on device operating in user mode.
 ---------------------------------------------------------------------------------

Quartus II Version 11.0 Build 157 04/27/2011 SJ Full Version
CHIP  "LED_hello_world"  ASSIGNED TO AN: EP4CE10F17C8

Pin Name/Usage               : Location  : Dir.   : I/O Standard      : Voltage : I/O Bank  : User Assignment
-------------------------------------------------------------------------------------------------------------
VCCIO8                       : A1        : power  :                   : 3.3V    : 8         :                
RESERVED_INPUT               : A2        :        :                   :         : 8         :                
RESERVED_INPUT               : A3        :        :                   :         : 8         :                
RESERVED_INPUT               : A4        :        :                   :         : 8         :                
RESERVED_INPUT               : A5        :        :                   :         : 8         :                
RESERVED_INPUT               : A6        :        :                   :         : 8         :                
RESERVED_INPUT               : A7        :        :                   :         : 8         :                
RESERVED_INPUT               : A8        :        :                   :         : 8         :                
SS_n_from_the_spi_touch      : A9        : output : 3.3-V LVTTL       :         : 7         : N              
RESERVED_INPUT               : A10       :        :                   :         : 7         :                
RESERVED_INPUT               : A11       :        :                   :         : 7         :                
RESERVED_INPUT               : A12       :        :                   :         : 7         :                
RESERVED_INPUT               : A13       :        :                   :         : 7         :                
RESERVED_INPUT               : A14       :        :                   :         : 7         :                
RESERVED_INPUT               : A15       :        :                   :         : 7         :                
VCCIO7                       : A16       : power  :                   : 3.3V    : 7         :                
RESERVED_INPUT               : B1        :        :                   :         : 1         :                
GND                          : B2        : gnd    :                   :         :           :                
RESERVED_INPUT               : B3        :        :                   :         : 8         :                
RESERVED_INPUT               : B4        :        :                   :         : 8         :                
RESERVED_INPUT               : B5        :        :                   :         : 8         :                
RESERVED_INPUT               : B6        :        :                   :         : 8         :                
RESERVED_INPUT               : B7        :        :                   :         : 8         :                
RESERVED_INPUT               : B8        :        :                   :         : 8         :                
RESERVED_INPUT               : B9        :        :                   :         : 7         :                
RESERVED_INPUT               : B10       :        :                   :         : 7         :                
RESERVED_INPUT               : B11       :        :                   :         : 7         :                
RESERVED_INPUT               : B12       :        :                   :         : 7         :                
RESERVED_INPUT               : B13       :        :                   :         : 7         :                
RESERVED_INPUT               : B14       :        :                   :         : 7         :                
GND                          : B15       : gnd    :                   :         :           :                
RESET                        : B16       : input  : 3.3-V LVTTL       :         : 6         : Y              
EPCS_SDO                     : C1        : output : 3.3-V LVTTL       :         : 1         : N              
RESERVED_INPUT               : C2        :        :                   :         : 1         :                
RESERVED_INPUT               : C3        :        :                   :         : 8         :                
VCCIO8                       : C4        : power  :                   : 3.3V    : 8         :                
GND                          : C5        : gnd    :                   :         :           :                
RESERVED_INPUT               : C6        :        :                   :         : 8         :                
VCCIO8                       : C7        : power  :                   : 3.3V    : 8         :                
RESERVED_INPUT               : C8        :        :                   :         : 8         :                
RESERVED_INPUT               : C9        :        :                   :         : 7         :                
VCCIO7                       : C10       : power  :                   : 3.3V    : 7         :                
RESERVED_INPUT               : C11       :        :                   :         : 7         :                
GND                          : C12       : gnd    :                   :         :           :                
VCCIO7                       : C13       : power  :                   : 3.3V    : 7         :                
RESERVED_INPUT               : C14       :        :                   :         : 7         :                
RESERVED_INPUT               : C15       :        :                   :         : 6         :                
RESERVED_INPUT               : C16       :        :                   :         : 6         :                
RESERVED_INPUT               : D1        :        :                   :         : 1         :                
EPCS_SCE                     : D2        : output : 3.3-V LVTTL       :         : 1         : N              
RESERVED_INPUT               : D3        :        :                   :         : 8         :                
RESERVED_INPUT               : D4        :        :                   :         : 1         :                
RESERVED_INPUT               : D5        :        :                   :         : 8         :                
RESERVED_INPUT               : D6        :        :                   :         : 8         :                
GND                          : D7        : gnd    :                   :         :           :                
RESERVED_INPUT               : D8        :        :                   :         : 8         :                
RESERVED_INPUT               : D9        :        :                   :         : 7         :                
GND                          : D10       : gnd    :                   :         :           :                
RESERVED_INPUT               : D11       :        :                   :         : 7         :                
RESERVED_INPUT               : D12       :        :                   :         : 7         :                
VCCD_PLL2                    : D13       : power  :                   : 1.2V    :           :                
RESERVED_INPUT               : D14       :        :                   :         : 7         :                
RESERVED_INPUT               : D15       :        :                   :         : 6         :                
RESERVED_INPUT               : D16       :        :                   :         : 6         :                
GND+                         : E1        :        :                   :         : 1         :                
GND                          : E2        : gnd    :                   :         :           :                
VCCIO1                       : E3        : power  :                   : 3.3V    : 1         :                
GND                          : E4        : gnd    :                   :         :           :                
RESERVED_INPUT               : E5        :        :                   :         : 1         :                
RESERVED_INPUT               : E6        :        :                   :         : 8         :                
RESERVED_INPUT               : E7        :        :                   :         : 8         :                
out_port_from_the_bl_n       : E8        : output : 3.3-V LVTTL       :         : 8         : N              
RESERVED_INPUT               : E9        :        :                   :         : 7         :                
RESERVED_INPUT               : E10       :        :                   :         : 7         :                
RESERVED_INPUT               : E11       :        :                   :         : 7         :                
GNDA2                        : E12       : gnd    :                   :         :           :                
GND                          : E13       : gnd    :                   :         :           :                
VCCIO6                       : E14       : power  :                   : 3.3V    : 6         :                
GND+                         : E15       :        :                   :         : 6         :                
CLK                          : E16       : input  : 3.3-V LVTTL       :         : 6         : Y              
RESERVED_INPUT               : F1        :        :                   :         : 1         :                
RESERVED_INPUT               : F2        :        :                   :         : 1         :                
RESERVED_INPUT               : F3        :        :                   :         : 1         :                
nSTATUS                      : F4        :        :                   :         : 1         :                
RESERVED_INPUT               : F5        :        :                   :         : 1         :                
RESERVED_INPUT               : F6        :        :                   :         : 8         :                
RESERVED_INPUT               : F7        :        :                   :         : 8         :                
RESERVED_INPUT               : F8        :        :                   :         : 8         :                
RESERVED_INPUT               : F9        :        :                   :         : 7         :                
RESERVED_INPUT               : F10       :        :                   :         : 7         :                
RESERVED_INPUT               : F11       :        :                   :         : 7         :                
VCCA2                        : F12       : power  :                   : 2.5V    :           :                
RESERVED_INPUT               : F13       :        :                   :         : 6         :                
RESERVED_INPUT               : F14       :        :                   :         : 6         :                
RESERVED_INPUT               : F15       :        :                   :         : 6         :                
RESERVED_INPUT               : F16       :        :                   :         : 6         :                
RESERVED_INPUT               : G1        :        :                   :         : 1         :                
RESERVED_INPUT               : G2        :        :                   :         : 1         :                
VCCIO1                       : G3        : power  :                   : 3.3V    : 1         :                
GND                          : G4        : gnd    :                   :         :           :                
RESERVED_INPUT               : G5        :        :                   :         : 1         :                
VCCINT                       : G6        : power  :                   : 1.2V    :           :                
VCCINT                       : G7        : power  :                   : 1.2V    :           :                
VCCINT                       : G8        : power  :                   : 1.2V    :           :                
VCCINT                       : G9        : power  :                   : 1.2V    :           :                
VCCINT                       : G10       : power  :                   : 1.2V    :           :                
RESERVED_INPUT               : G11       :        :                   :         : 6         :                
MSEL2                        : G12       :        :                   :         : 6         :                
GND                          : G13       : gnd    :                   :         :           :                
VCCIO6                       : G14       : power  :                   : 3.3V    : 6         :                
DQ[15]                       : G15       : bidir  : 3.3-V LVTTL       :         : 6         : Y              
RESERVED_INPUT               : G16       :        :                   :         : 6         :                
EPCS_CLK                     : H1        : output : 3.3-V LVTTL       :         : 1         : N              
EPCS_DATA0                   : H2        : input  : 3.3-V LVTTL       :         : 1         : N              
altera_reserved_tck          : H3        : input  : 3.3-V LVTTL       :         : 1         : N              
altera_reserved_tdi          : H4        : input  : 3.3-V LVTTL       :         : 1         : N              
nCONFIG                      : H5        :        :                   :         : 1         :                
VCCINT                       : H6        : power  :                   : 1.2V    :           :                
GND                          : H7        : gnd    :                   :         :           :                
GND                          : H8        : gnd    :                   :         :           :                
GND                          : H9        : gnd    :                   :         :           :                
GND                          : H10       : gnd    :                   :         :           :                
VCCINT                       : H11       : power  :                   : 1.2V    :           :                
MSEL1                        : H12       :        :                   :         : 6         :                
MSEL0                        : H13       :        :                   :         : 6         :                
CONF_DONE                    : H14       :        :                   :         : 6         :                
GND                          : H15       : gnd    :                   :         :           :                
GND                          : H16       : gnd    :                   :         :           :                
RESERVED_INPUT               : J1        :        :                   :         : 2         :                
RESERVED_INPUT               : J2        :        :                   :         : 2         :                
nCE                          : J3        :        :                   :         : 1         :                
altera_reserved_tdo          : J4        : output : 3.3-V LVTTL       :         : 1         : N              
altera_reserved_tms          : J5        : input  : 3.3-V LVTTL       :         : 1         : N              
RESERVED_INPUT               : J6        :        :                   :         : 2         :                
GND                          : J7        : gnd    :                   :         :           :                
GND                          : J8        : gnd    :                   :         :           :                
GND                          : J9        : gnd    :                   :         :           :                
GND                          : J10       : gnd    :                   :         :           :                
RESERVED_INPUT               : J11       :        :                   :         : 5         :                
RESERVED_INPUT               : J12       :        :                   :         : 5         :                
RESERVED_INPUT               : J13       :        :                   :         : 5         :                
RESERVED_INPUT               : J14       :        :                   :         : 5         :                
DQ[14]                       : J15       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
DQ[13]                       : J16       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
DQ[1]                        : K1        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
DQ[0]                        : K2        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
VCCIO2                       : K3        : power  :                   : 3.3V    : 2         :                
GND                          : K4        : gnd    :                   :         :           :                
RESERVED_INPUT               : K5        :        :                   :         : 2         :                
out_port_from_the_bl_p       : K6        : output : 3.3-V LVTTL       :         : 2         : N              
VCCINT                       : K7        : power  :                   : 1.2V    :           :                
RESERVED_INPUT               : K8        :        :                   :         : 3         :                
MOSI_from_the_spi_touch      : K9        : output : 3.3-V LVTTL       :         : 4         : Y              
RESERVED_INPUT               : K10       :        :                   :         : 4         :                
RESERVED_INPUT               : K11       :        :                   :         : 5         :                
RESERVED_INPUT               : K12       :        :                   :         : 5         :                
GND                          : K13       : gnd    :                   :         :           :                
VCCIO5                       : K14       : power  :                   : 3.3V    : 5         :                
DQ[12]                       : K15       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
DQ[11]                       : K16       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
DQ[3]                        : L1        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
DQ[2]                        : L2        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
RAS                          : L3        : output : 3.3-V LVTTL       :         : 2         : Y              
CAS                          : L4        : output : 3.3-V LVTTL       :         : 2         : Y              
VCCA1                        : L5        : power  :                   : 2.5V    :           :                
RA[2]                        : L6        : output : 3.3-V LVTTL       :         : 2         : Y              
RESERVED_INPUT               : L7        :        :                   :         : 3         :                
RESERVED_INPUT               : L8        :        :                   :         : 3         :                
MISO_to_the_spi_touch        : L9        : input  : 3.3-V LVTTL       :         : 4         : Y              
RESERVED_INPUT               : L10       :        :                   :         : 4         :                
RESERVED_INPUT               : L11       :        :                   :         : 4         :                
RESERVED_INPUT               : L12       :        :                   :         : 5         :                
RESERVED_INPUT               : L13       :        :                   :         : 5         :                
RESERVED_INPUT               : L14       :        :                   :         : 5         :                
DQ[10]                       : L15       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
DQ[9]                        : L16       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GND+                         : M1        :        :                   :         : 2         :                
GND+                         : M2        :        :                   :         : 2         :                
VCCIO2                       : M3        : power  :                   : 3.3V    : 2         :                
GND                          : M4        : gnd    :                   :         :           :                
GNDA1                        : M5        : gnd    :                   :         :           :                
RESERVED_INPUT               : M6        :        :                   :         : 3         :                
RESERVED_INPUT               : M7        :        :                   :         : 3         :                
RESERVED_INPUT               : M8        :        :                   :         : 3         :                
out_port_from_the_touch_cs   : M9        : output : 3.3-V LVTTL       :         : 4         : Y              
RESERVED_INPUT               : M10       :        :                   :         : 4         :                
RESERVED_INPUT               : M11       :        :                   :         : 4         :                
RESERVED_INPUT               : M12       :        :                   :         : 5         :                
GND                          : M13       : gnd    :                   :         :           :                
VCCIO5                       : M14       : power  :                   : 3.3V    : 5         :                
GND+                         : M15       :        :                   :         : 5         :                
GND+                         : M16       :        :                   :         : 5         :                
DQ[5]                        : N1        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
DQ[4]                        : N2        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
BA[0]                        : N3        : output : 3.3-V LVTTL       :         : 3         : Y              
VCCD_PLL1                    : N4        : power  :                   : 1.2V    :           :                
RA[10]                       : N5        : output : 3.3-V LVTTL       :         : 3         : Y              
BA[1]                        : N6        : output : 3.3-V LVTTL       :         : 3         : Y              
GND                          : N7        : gnd    :                   :         :           :                
RA[3]                        : N8        : output : 3.3-V LVTTL       :         : 3         : Y              
bidir_port_to_and_from_the_lcd32_data[5] : N9        : bidir  : 3.3-V LVTTL       :         : 4         : Y              
GND                          : N10       : gnd    :                   :         :           :                
bidir_port_to_and_from_the_lcd32_data[3] : N11       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
bidir_port_to_and_from_the_lcd32_data[1] : N12       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
RESERVED_INPUT               : N13       :        :                   :         : 5         :                
RESERVED_INPUT               : N14       :        :                   :         : 5         :                
DQ[8]                        : N15       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
S_DQM[1]                     : N16       : output : 3.3-V LVTTL       :         : 5         : Y              
DQ[7]                        : P1        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
DQ[6]                        : P2        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
CS                           : P3        : output : 3.3-V LVTTL       :         : 3         : Y              
VCCIO3                       : P4        : power  :                   : 3.3V    : 3         :                
GND                          : P5        : gnd    :                   :         :           :                
RA[1]                        : P6        : output : 3.3-V LVTTL       :         : 3         : Y              
VCCIO3                       : P7        : power  :                   : 3.3V    : 3         :                
RA[0]                        : P8        : output : 3.3-V LVTTL       :         : 3         : Y              
bidir_port_to_and_from_the_lcd32_data[4] : P9        : bidir  : 3.3-V LVTTL       :         : 4         : Y              
VCCIO4                       : P10       : power  :                   : 3.3V    : 4         :                
bidir_port_to_and_from_the_lcd32_data[2] : P11       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
GND                          : P12       : gnd    :                   :         :           :                
VCCIO4                       : P13       : power  :                   : 3.3V    : 4         :                
RESERVED_INPUT               : P14       :        :                   :         : 4         :                
S_CLK                        : P15       : output : 3.3-V LVTTL       :         : 5         : Y              
CKE                          : P16       : output : 3.3-V LVTTL       :         : 5         : Y              
WE                           : R1        : output : 3.3-V LVTTL       :         : 2         : Y              
GND                          : R2        : gnd    :                   :         :           :                
out_port_from_the_reset      : R3        : output : 3.3-V LVTTL       :         : 3         : Y              
out_port_from_the_lcd_wr     : R4        : output : 3.3-V LVTTL       :         : 3         : Y              
out_port_from_the_lcd_cs     : R5        : output : 3.3-V LVTTL       :         : 3         : Y              
bidir_port_to_and_from_the_lcd32_data[14] : R6        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
bidir_port_to_and_from_the_lcd32_data[12] : R7        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
bidir_port_to_and_from_the_lcd32_data[10] : R8        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
bidir_port_to_and_from_the_lcd32_data[8] : R9        : bidir  : 3.3-V LVTTL       :         : 4         : Y              
bidir_port_to_and_from_the_lcd32_data[6] : R10       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
bidir_port_to_and_from_the_lcd32_data[0] : R11       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
RA[4]                        : R12       : output : 3.3-V LVTTL       :         : 4         : Y              
RA[6]                        : R13       : output : 3.3-V LVTTL       :         : 4         : Y              
RA[8]                        : R14       : output : 3.3-V LVTTL       :         : 4         : Y              
GND                          : R15       : gnd    :                   :         :           :                
RA[11]                       : R16       : output : 3.3-V LVTTL       :         : 5         : Y              
VCCIO3                       : T1        : power  :                   : 3.3V    : 3         :                
S_DQM[0]                     : T2        : output : 3.3-V LVTTL       :         : 3         : Y              
SCLK_from_the_spi_touch      : T3        : output : 3.3-V LVTTL       :         : 3         : Y              
in_port_to_the_touch_irq     : T4        : input  : 3.3-V LVTTL       :         : 3         : Y              
out_port_from_the_lcd_rd     : T5        : output : 3.3-V LVTTL       :         : 3         : Y              
out_port_from_the_lcd_rs     : T6        : output : 3.3-V LVTTL       :         : 3         : Y              
bidir_port_to_and_from_the_lcd32_data[15] : T7        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
bidir_port_to_and_from_the_lcd32_data[13] : T8        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
bidir_port_to_and_from_the_lcd32_data[11] : T9        : bidir  : 3.3-V LVTTL       :         : 4         : Y              
bidir_port_to_and_from_the_lcd32_data[9] : T10       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
bidir_port_to_and_from_the_lcd32_data[7] : T11       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
RA[5]                        : T12       : output : 3.3-V LVTTL       :         : 4         : Y              
RA[7]                        : T13       : output : 3.3-V LVTTL       :         : 4         : Y              
RA[9]                        : T14       : output : 3.3-V LVTTL       :         : 4         : Y              
RA[12]                       : T15       : output : 3.3-V LVTTL       :         : 4         : Y              
VCCIO4                       : T16       : power  :                   : 3.3V    : 4         :                
