SYSTEM CORE_SOPC
{
   System_Wizard_Version = "11.00";
   System_Wizard_Build = "157";
   # 
   # Generated by: com.altera.sopcmodel.ensemble.EnsembleGeneratePTF
   # Date: 2012.09.06.17:04:26
   # 
   #    clock_source "clk"
   #    altera_nios2 "cpu"
   #    altera_avalon_sysid "sysid"
   #    altera_avalon_epcs_flash_controller "epcs"
   #    altera_avalon_new_sdram_controller "sdram"
   #    altera_avalon_jtag_uart "jtag_uart"
   #    altera_avalon_spi "spi_touch"
   #    altera_avalon_pio "lcd_cs"
   #    altera_avalon_pio "touch_cs"
   #    altera_avalon_pio "lcd_rs"
   #    altera_avalon_pio "touch_irq"
   #    altera_avalon_pio "reset"
   #    altera_avalon_pio "lcd_wr"
   #    altera_avalon_pio "lcd32_data"
   #    altera_avalon_pio "lcd_rd"
   #    altera_avalon_pio "bl_p"
   #    altera_avalon_pio "bl_n"
   # 
   #    Contains 38 connections.
   # 
   Builder_Application = "sopc_builder_ca";
   #. values for Builder_Application are:
   #.    sopc_builder_preview --> 6.1p, 7.0p prerelease versions
   #.    sopc_builder_ca      --> 7.1 and later
   #.    (missing) --> 6.0 or earlier
   WIZARD_SCRIPT_ARGUMENTS 
   {
      hdl_language = "verilog";
      device_family = "CYCLONEIVE";
      device_family_id = "CYCLONEIVE";
      generate_sdk = "0";
      do_build_sim = "0";
      hardcopy_compatible = "0";
      CLOCKS 
      {
         CLOCK clk
         {
            frequency = "50000000";
            source = "External";
            Is_Clock_Source = "0";
            display_name = "clk";
            pipeline = "0";
            clock_module_connection_point_for_c2h = "clk.clk";
         }
      }
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      clock_freq = "50000000";
      board_class = "";
      view_master_columns = "1";
      view_master_priorities = "0";
      generate_hdl = "";
      bustype_column_width = "0";
      clock_column_width = "80";
      name_column_width = "75";
      desc_column_width = "75";
      base_column_width = "75";
      end_column_width = "75";
      BOARD_INFO 
      {
         altera_avalon_epcs_flash_controller 
         {
            reference_designators = "";
         }
      }
   }
   MODULE cpu
   {
      MASTER instruction_master
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT i_address
            {
               type = "address";
               width = "27";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT i_read
            {
               type = "read";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT i_readdata
            {
               type = "readdata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT i_readdatavalid
            {
               type = "readdatavalid";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT i_waitrequest
            {
               type = "waitrequest";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_resetrequest
            {
               type = "resetrequest";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Asynchronous = "0";
            DBS_Big_Endian = "0";
            Adapts_To = "";
            Do_Stream_Reads = "0";
            Do_Stream_Writes = "0";
            Max_Address_Width = "32";
            Data_Width = "32";
            Address_Width = "27";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "";
            Linewrap_Bursts = "";
            Burst_On_Burst_Boundaries_Only = "";
            Always_Burst_Max_Burst = "";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            Is_Instruction_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "0";
            Address_Group = "0";
            Has_IRQ = "0";
            Irq_Scheme = "individual_requests";
            Interrupt_Range = "0-0";
         }
         MEMORY_MAP 
         {
            Entry cpu/jtag_debug_module
            {
               address = "0x00001000";
               span = "0x00000800";
               is_bridge = "0";
            }
            Entry epcs/epcs_control_port
            {
               address = "0x00000000";
               span = "0x00000800";
               is_bridge = "0";
            }
            Entry sdram/s1
            {
               address = "0x04000000";
               span = "0x02000000";
               is_bridge = "0";
            }
         }
      }
      MASTER custom_instruction_master
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "nios_custom_instruction";
            Data_Width = "32";
            Address_Width = "8";
            Is_Custom_Instruction = "1";
            Is_Enabled = "0";
            Max_Address_Width = "8";
            Base_Address = "N/A";
            Is_Visible = "0";
         }
         PORT_WIRING 
         {
            PORT dataa
            {
               type = "dataa";
               width = "32";
               direction = "output";
            }
            PORT datab
            {
               type = "datab";
               width = "32";
               direction = "output";
            }
            PORT result
            {
               type = "result";
               width = "32";
               direction = "input";
            }
            PORT clk_en
            {
               type = "clk_en";
               width = "1";
               direction = "output";
            }
            PORT reset
            {
               type = "reset";
               width = "1";
               direction = "output";
            }
            PORT start
            {
               type = "start";
               width = "1";
               direction = "output";
            }
            PORT done
            {
               type = "done";
               width = "1";
               direction = "input";
            }
            PORT n
            {
               type = "n";
               width = "8";
               direction = "output";
            }
            PORT a
            {
               type = "a";
               width = "5";
               direction = "output";
            }
            PORT b
            {
               type = "b";
               width = "5";
               direction = "output";
            }
            PORT c
            {
               type = "c";
               width = "5";
               direction = "output";
            }
            PORT readra
            {
               type = "readra";
               width = "1";
               direction = "output";
            }
            PORT readrb
            {
               type = "readrb";
               width = "1";
               direction = "output";
            }
            PORT writerc
            {
               type = "writerc";
               width = "1";
               direction = "output";
            }
         }
      }
      SLAVE jtag_debug_module
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "dynamic";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Address_Span = "2048";
            Read_Latency = "0";
            Is_Memory_Device = "1";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "9";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            Accepts_External_Connections = "1";
            Requires_Internal_Connections = "";
            MASTERED_BY cpu/instruction_master
            {
               priority = "1";
               Offset_Address = "0x00001000";
            }
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00001000";
            }
            Base_Address = "0x00001000";
            Is_Readable = "1";
            Is_Writeable = "1";
            Uses_Tri_State_Data_Bus = "0";
            Has_IRQ = "0";
            JTAG_Hub_Base_Id = "1118278";
            JTAG_Hub_Instance_Id = "0";
            Address_Group = "0";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
         }
         PORT_WIRING 
         {
            PORT jtag_debug_module_address
            {
               type = "address";
               width = "9";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_begintransfer
            {
               type = "begintransfer";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_byteenable
            {
               type = "byteenable";
               width = "4";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_debugaccess
            {
               type = "debugaccess";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_select
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_write
            {
               type = "write";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
         }
      }
      MASTER data_master
      {
         SYSTEM_BUILDER_INFO 
         {
            Has_IRQ = "1";
            Irq_Scheme = "individual_requests";
            Bus_Type = "avalon";
            Is_Asynchronous = "0";
            DBS_Big_Endian = "0";
            Adapts_To = "";
            Do_Stream_Reads = "0";
            Do_Stream_Writes = "0";
            Max_Address_Width = "32";
            Data_Width = "32";
            Address_Width = "27";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "1";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            Is_Data_Master = "1";
            Address_Group = "0";
            Is_Readable = "1";
            Is_Writeable = "1";
            Interrupt_Range = "0-31";
         }
         PORT_WIRING 
         {
            PORT d_irq
            {
               type = "irq";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT d_address
            {
               type = "address";
               width = "27";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT d_byteenable
            {
               type = "byteenable";
               width = "4";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT d_read
            {
               type = "read";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT d_readdata
            {
               type = "readdata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT d_readdatavalid
            {
               type = "readdatavalid";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT d_waitrequest
            {
               type = "waitrequest";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT d_write
            {
               type = "write";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT d_writedata
            {
               type = "writedata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT jtag_debug_module_debugaccess_to_roms
            {
               type = "debugaccess";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         MEMORY_MAP 
         {
            Entry cpu/jtag_debug_module
            {
               address = "0x00001000";
               span = "0x00000800";
               is_bridge = "0";
            }
            Entry sysid/control_slave
            {
               address = "0x000018c0";
               span = "0x00000008";
               is_bridge = "0";
            }
            Entry epcs/epcs_control_port
            {
               address = "0x00000000";
               span = "0x00000800";
               is_bridge = "0";
            }
            Entry sdram/s1
            {
               address = "0x04000000";
               span = "0x02000000";
               is_bridge = "0";
            }
            Entry jtag_uart/avalon_jtag_slave
            {
               address = "0x000018c8";
               span = "0x00000008";
               is_bridge = "0";
            }
            Entry spi_touch/spi_control_port
            {
               address = "0x00001800";
               span = "0x00000020";
               is_bridge = "0";
            }
            Entry lcd_cs/s1
            {
               address = "0x00001820";
               span = "0x00000010";
               is_bridge = "0";
            }
            Entry touch_cs/s1
            {
               address = "0x00001830";
               span = "0x00000010";
               is_bridge = "0";
            }
            Entry lcd_rs/s1
            {
               address = "0x00001840";
               span = "0x00000010";
               is_bridge = "0";
            }
            Entry touch_irq/s1
            {
               address = "0x00001850";
               span = "0x00000010";
               is_bridge = "0";
            }
            Entry reset/s1
            {
               address = "0x00001860";
               span = "0x00000010";
               is_bridge = "0";
            }
            Entry lcd_wr/s1
            {
               address = "0x00001870";
               span = "0x00000010";
               is_bridge = "0";
            }
            Entry lcd32_data/s1
            {
               address = "0x00001880";
               span = "0x00000010";
               is_bridge = "0";
            }
            Entry lcd_rd/s1
            {
               address = "0x00001890";
               span = "0x00000010";
               is_bridge = "0";
            }
            Entry bl_p/s1
            {
               address = "0x000018a0";
               span = "0x00000010";
               is_bridge = "0";
            }
            Entry bl_n/s1
            {
               address = "0x000018b0";
               span = "0x00000010";
               is_bridge = "0";
            }
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         cache_has_dcache = "0";
         cache_dcache_size = "0";
         cache_dcache_line_size = "0";
         cache_dcache_bursts = "0";
         cache_dcache_ram_block_type = "AUTO";
         num_tightly_coupled_data_masters = "0";
         gui_num_tightly_coupled_data_masters = "0";
         gui_include_tightly_coupled_data_masters = "0";
         gui_omit_avalon_data_master = "0";
         cache_has_icache = "1";
         cache_icache_size = "2048";
         cache_icache_line_size = "32";
         cache_icache_ram_block_type = "AUTO";
         cache_icache_bursts = "0";
         num_tightly_coupled_instruction_masters = "0";
         gui_num_tightly_coupled_instruction_masters = "0";
         gui_include_tightly_coupled_instruction_masters = "0";
         debug_level = "2";
         include_oci = "1";
         oci_num_xbrk = "0";
         oci_num_dbrk = "0";
         oci_dbrk_trace = "0";
         oci_dbrk_pairs = "0";
         oci_onchip_trace = "0";
         oci_offchip_trace = "0";
         oci_data_trace = "0";
         include_third_party_debug_port = "0";
         oci_trace_addr_width = "7";
         oci_debugreq_signals = "0";
         oci_trigger_arming = "1";
         oci_embedded_pll = "0";
         oci_assign_jtag_instance_id = "0";
         oci_jtag_instance_id = "0";
         oci_num_pm = "0";
         oci_pm_width = "32";
         performance_counters_present = "0";
         performance_counters_width = "32";
         always_encrypt = "1";
         debug_simgen = "0";
         activate_model_checker = "0";
         activate_test_end_checker = "0";
         activate_trace = "1";
         activate_monitors = "1";
         clear_x_bits_ld_non_bypass = "1";
         bit_31_bypass_dcache = "1";
         hdl_sim_caches_cleared = "1";
         hbreak_test = "0";
         allow_full_address_range = "0";
         extra_exc_info = "0";
         branch_prediction_type = "Dynamic";
         bht_ptr_sz = "8";
         bht_index_pc_only = "0";
         gui_branch_prediction_type = "Automatic";
         full_waveform_signals = "0";
         export_pcb = "0";
         big_endian = "0";
         avalon_debug_port_present = "0";
         illegal_instructions_trap = "0";
         illegal_memory_access_detection = "0";
         illegal_mem_exc = "0";
         slave_access_error_exc = "0";
         division_error_exc = "0";
         eic_present = "0";
         num_shadow_reg_sets = "0";
         gui_mmu_present = "0";
         mmu_present = "0";
         process_id_num_bits = "8";
         tlb_ptr_sz = "7";
         tlb_num_ways = "16";
         udtlb_num_entries = "6";
         uitlb_num_entries = "4";
         fast_tlb_miss_exc_slave = "";
         fast_tlb_miss_exc_offset = "0x00000000";
         mpu_present = "0";
         mpu_num_data_regions = "8";
         mpu_num_inst_regions = "8";
         mpu_min_data_region_size_log2 = "12";
         mpu_min_inst_region_size_log2 = "12";
         mpu_use_limit = "0";
         hardware_divide_present = "0";
         gui_hardware_divide_setting = "0";
         hardware_multiply_present = "1";
         hardware_multiply_impl = "embedded_mul";
         shift_rot_impl = "fast_le_shift";
         gui_hardware_multiply_setting = "embedded_mul_fast_le_shift";
         reset_slave = "epcs/epcs_control_port";
         break_slave = "cpu/jtag_debug_module";
         exc_slave = "sdram/s1";
         reset_offset = "0x00000000";
         break_offset = "0x00000020";
         exc_offset = "0x00000020";
         cpu_reset = "0";
         CPU_Implementation = "fast";
         cpu_selection = "f";
         device_family_id = "CYCLONEIVE";
         address_stall_present = "1";
         dsp_block_supports_shift = "0";
         mrams_present = "0";
         cpuid_value = "0";
         dont_overwrite_cpuid = "1";
         allow_legacy_sdk = "1";
         legacy_sdk_support = "1";
         inst_addr_width = "27";
         data_addr_width = "27";
         CPU_Architecture = "nios2";
         cache_icache_burst_type = "none";
         oci_sync_depth = "2";
         hardware_divide_impl = "variable_latency";
         hardware_multiply_omits_msw = "1";
         break_slave_override = "";
         break_offset_override = "0x20";
         altera_show_unreleased_features = "0";
         altera_show_unpublished_features = "0";
         altera_internal_test = "0";
         alt_log_port_base = "";
         alt_log_port_type = "";
         cpuid_sz = "1";
         gui_illegal_instructions_trap = "0";
         advanced_exc = "0";
         gui_illegal_memory_access_detection = "0";
         cache_omit_dcache = "0";
         cache_omit_icache = "0";
         omit_instruction_master = "0";
         omit_data_master = "0";
         ras_ptr_sz = "4";
         jtb_ptr_sz = "5";
         ibuf_ptr_sz = "4";
         always_bypass_dcache = "0";
         iss_trace_on = "0";
         iss_trace_warning = "1";
         iss_trace_info = "1";
         iss_trace_disassembly = "0";
         iss_trace_registers = "0";
         iss_trace_instr_count = "0";
         iss_software_debug = "0";
         iss_software_debug_port = "9996";
         iss_memory_dump_start = "";
         iss_memory_dump_end = "";
         Boot_Copier = "boot_loader_cfi.srec";
         Boot_Copier_EPCS = "boot_loader_epcs.srec";
         Boot_Copier_EPCS_SII_SIII_CIII = "boot_loader_epcs_sii_siii_ciii.srec";
         Boot_Copier_BE = "boot_loader_cfi_be.srec";
         Boot_Copier_EPCS_BE = "boot_loader_epcs_be.srec";
         Boot_Copier_EPCS_SII_SIII_CIII_BE = "boot_loader_epcs_sii_siii_ciii_be.srec";
         CONSTANTS 
         {
            CONSTANT __nios_catch_irqs__
            {
               value = "1";
               comment = "Include panic handler for all irqs (needs uart)";
            }
            CONSTANT __nios_use_constructors__
            {
               value = "1";
               comment = "Call c++ static constructors";
            }
            CONSTANT __nios_use_small_printf__
            {
               value = "1";
               comment = "Smaller non-ANSI printf, with no floating point";
            }
            CONSTANT nasys_has_icache
            {
               value = "1";
               comment = "True if instruction cache present";
            }
            CONSTANT nasys_icache_size
            {
               value = "2048";
               comment = "Size in bytes of instruction cache";
            }
            CONSTANT nasys_icache_line_size
            {
               value = "32";
               comment = "Size in bytes of each icache line";
            }
            CONSTANT nasys_icache_line_size_log2
            {
               value = "5";
               comment = "Log2 size in bytes of each icache line";
            }
            CONSTANT nasys_has_dcache
            {
               value = "0";
               comment = "True if instruction cache present";
            }
            CONSTANT nasys_dcache_size
            {
               value = "0";
               comment = "Size in bytes of data cache";
            }
            CONSTANT nasys_dcache_line_size
            {
               value = "0";
               comment = "Size in bytes of each dcache line";
            }
            CONSTANT nasys_dcache_line_size_log2
            {
               value = "-Infinity";
               comment = "Log2 size in bytes of each dcache line";
            }
         }
         license_status = "";
         mainmem_slave = "sdram/s1";
         datamem_slave = "sdram/s1";
         maincomm_slave = "";
         germs_monitor_id = "";
      }
      class = "altera_nios2";
      class_version = "7.08110";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         Parameters_Signature = "";
         Is_CPU = "1";
         Instantiate_In_System_Module = "1";
         Required_Device_Family = "STRATIX,STRATIXGX,STRATIXII,STRATIXIIGX,STRATIXIIGXLITE,STRATIXIII,STRATIXIV,STRATIXV,CYCLONE,CYCLONEII,CYCLONEIII,CYCLONEIVE,HARDCOPYIII,ARRIAII,ARRIAIIGZ,TARPON,HARDCOPYIV,STINGRAY";
         Default_Module_Name = "cpu";
         Top_Level_Ports_Are_Enumerated = "1";
         View 
         {
            Settings_Summary = "Nios II/f
            <br>&nbsp;&nbsp;2-Kbyte Instruction Cache
            
            <br>&nbsp;&nbsp;JTAG Debug Module
            ";
            MESSAGES 
            {
            }
         }
      }
      iss_model_name = "altera_nios2";
      HDL_INFO 
      {
         # The list of files associated with this module (for synthesis
         # and other purposes) depends on the users' wizard-choices.
         # This section will be filled-in by the Generator_Program
         # after the module logic has been created and the
         # various filenames are known.
      }
      MASTER tightly_coupled_instruction_master_0
      {
         PORT_WIRING 
         {
            # The number and kind of ports that appear on this module
            # depends on the user's wizard-choices.
            # This section will be filled-in by the Generator_Program after
            # the module logic has been created and the ports are known.
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Is_Instruction_Master = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_instruction_master_1
      {
         PORT_WIRING 
         {
            # The number and kind of ports that appear on this module
            # depends on the user's wizard-choices.
            # This section will be filled-in by the Generator_Program after
            # the module logic has been created and the ports are known.
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Instruction_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "0";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_instruction_master_2
      {
         PORT_WIRING 
         {
            # The number and kind of ports that appear on this module
            # depends on the user's wizard-choices.
            # This section will be filled-in by the Generator_Program after
            # the module logic has been created and the ports are known.
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Instruction_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "0";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_instruction_master_3
      {
         PORT_WIRING 
         {
            # The number and kind of ports that appear on this module
            # depends on the user's wizard-choices.
            # This section will be filled-in by the Generator_Program after
            # the module logic has been created and the ports are known.
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Instruction_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "0";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER data_master2
      {
         PORT_WIRING 
         {
            # The number and kind of ports that appear on this module
            # depends on the user's wizard-choices.
            # This section will be filled-in by the Generator_Program after
            # the module logic has been created and the ports are known.
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "1";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
         }
      }
      MASTER tightly_coupled_data_master_0
      {
         PORT_WIRING 
         {
            # The number and kind of ports that appear on this module
            # depends on the user's wizard-choices.
            # This section will be filled-in by the Generator_Program after
            # the module logic has been created and the ports are known.
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_data_master_1
      {
         PORT_WIRING 
         {
            # The number and kind of ports that appear on this module
            # depends on the user's wizard-choices.
            # This section will be filled-in by the Generator_Program after
            # the module logic has been created and the ports are known.
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_data_master_2
      {
         PORT_WIRING 
         {
            # The number and kind of ports that appear on this module
            # depends on the user's wizard-choices.
            # This section will be filled-in by the Generator_Program after
            # the module logic has been created and the ports are known.
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_data_master_3
      {
         PORT_WIRING 
         {
            # The number and kind of ports that appear on this module
            # depends on the user's wizard-choices.
            # This section will be filled-in by the Generator_Program after
            # the module logic has been created and the ports are known.
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Is_Big_Endian = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      PORT_WIRING 
      {
         PORT jtag_debug_trigout
         {
            width = "1";
            direction = "output";
            Is_Enabled = "0";
         }
         PORT jtag_debug_offchip_trace_clk
         {
            width = "1";
            direction = "output";
            Is_Enabled = "0";
         }
         PORT jtag_debug_offchip_trace_data
         {
            width = "18";
            direction = "output";
            Is_Enabled = "0";
         }
         PORT clkx2
         {
            width = "1";
            direction = "input";
            Is_Enabled = "0";
            visible = "0";
         }
      }
   }
   MODULE sysid
   {
      SLAVE control_slave
      {
         PORT_WIRING 
         {
            PORT clock
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "1";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x000018c0";
            }
            Base_Address = "0x000018c0";
            Has_IRQ = "0";
            Address_Group = "0";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
         }
      }
      class = "altera_avalon_sysid";
      class_version = "7.08110";
      SYSTEM_BUILDER_INFO 
      {
         Date_Modified = "";
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Fixed_Module_Name = "sysid";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         View 
         {
            Settings_Summary = "No system ID yet.  <br> 
                                  A unique ID is assigned every time <br> 
                                  the system is generated.";
            MESSAGES 
            {
            }
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         id = "0";
         timestamp = "1346922198";
         regenerate_values = "0";
      }
      HDL_INFO 
      {
         # The list of files associated with this module (for synthesis
         # and other purposes) depends on the users' wizard-choices.
         # This section will be filled-in by the Generator_Program
         # after the module logic has been created and the
         # various filenames are known.
      }
      PORT_WIRING 
      {
         # The number and kind of ports that appear on this module
         # depends on the user's wizard-choices.
         # This section will be filled-in by the Generator_Program
         # after the module logic has been created and the ports are known.
         #
      }
   }
   MODULE epcs
   {
      SLAVE epcs_control_port
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT irq
            {
               type = "irq";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "9";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT dataavailable
            {
               type = "dataavailable";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT endofpacket
            {
               type = "endofpacket";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT read_n
            {
               type = "read_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT readyfordata
            {
               type = "readyfordata";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Has_IRQ = "1";
            Bus_Type = "avalon";
            Write_Wait_States = "1cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "dynamic";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "1";
            Address_Span = "2048";
            Read_Latency = "0";
            Is_Memory_Device = "1";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "1";
            Data_Width = "32";
            Address_Width = "9";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/instruction_master
            {
               priority = "1";
               Offset_Address = "0x00000000";
            }
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00000000";
            }
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "0";
            }
            Base_Address = "0x00000000";
            Address_Group = "0";
         }
         WIZARD_SCRIPT_ARGUMENTS 
         {
            class = "altera_avalon_epcs_flash_controller";
            flash_reference_designator = "";
         }
      }
      PORT_WIRING 
      {
         PORT dclk
         {
            type = "export";
            width = "1";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT sce
         {
            type = "export";
            width = "1";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT sdo
         {
            type = "export";
            width = "1";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT data0
         {
            type = "export";
            width = "1";
            direction = "input";
            Is_Enabled = "1";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         databits = "8";
         targetclock = "20";
         clockunits = "MHz";
         clockmult = "1000000";
         numslaves = "1";
         ismaster = "1";
         clockpolarity = "0";
         clockphase = "0";
         lsbfirst = "0";
         extradelay = "0";
         targetssdelay = "100";
         delayunits = "us";
         delaymult = "1e-06";
         prefix = "epcs_";
         register_offset = "0x400";
         ignore_legacy_check = "1";
         use_asmi_atom = "0";
      }
      class = "altera_avalon_epcs_flash_controller";
      class_version = "7.08110";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         Instantiate_In_System_Module = "1";
         Required_Device_Family = "STRATIX,CYCLONE,CYCLONEII,CYCLONEIII,STRATIXIII,STRATIXII,STRATIXIIGX,ARRIAGX,STRATIXIIGXLITE,STRATIXIV,STRATIXV,ARRIAII,ARRIAIIGZ,TARPON,STINGRAY,CYCLONEIVE";
         Fixed_Module_Name = "epcs_controller";
         Top_Level_Ports_Are_Enumerated = "1";
         View 
         {
            MESSAGES 
            {
            }
         }
      }
   }
   MODULE sdram
   {
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT az_addr
            {
               type = "address";
               width = "24";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT az_be_n
            {
               type = "byteenable_n";
               width = "2";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT az_cs
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT az_data
            {
               type = "writedata";
               width = "16";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT az_rd_n
            {
               type = "read_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT az_wr_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT za_data
            {
               type = "readdata";
               width = "16";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT za_valid
            {
               type = "readdatavalid";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT za_waitrequest
            {
               type = "waitrequest";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT zs_addr
            {
               direction = "output";
               width = "13";
               Is_Enabled = "1";
            }
            PORT zs_ba
            {
               direction = "output";
               width = "2";
               Is_Enabled = "1";
            }
            PORT zs_cas_n
            {
               direction = "output";
               width = "1";
               Is_Enabled = "1";
            }
            PORT zs_cke
            {
               direction = "output";
               width = "1";
               Is_Enabled = "1";
            }
            PORT zs_cs_n
            {
               direction = "output";
               width = "1";
               Is_Enabled = "1";
            }
            PORT zs_dq
            {
               direction = "inout";
               width = "16";
               Is_Enabled = "1";
            }
            PORT zs_dqm
            {
               direction = "output";
               width = "2";
               Is_Enabled = "1";
            }
            PORT zs_ras_n
            {
               direction = "output";
               width = "1";
               Is_Enabled = "1";
            }
            PORT zs_we_n
            {
               direction = "output";
               width = "1";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Read_Wait_States = "peripheral_controlled";
            Write_Wait_States = "peripheral_controlled";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "dynamic";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Address_Span = "33554432";
            Read_Latency = "0";
            Is_Memory_Device = "1";
            Maximum_Pending_Read_Transactions = "7";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "16";
            Address_Width = "24";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/instruction_master
            {
               priority = "1";
               Offset_Address = "0x04000000";
            }
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x04000000";
            }
            Base_Address = "0x04000000";
            Has_IRQ = "0";
            Simulation_Num_Lanes = "1";
            Address_Group = "0";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
         }
      }
      PORT_WIRING 
      {
         PORT zs_addr
         {
            type = "export";
            width = "13";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT zs_ba
         {
            type = "export";
            width = "2";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT zs_cas_n
         {
            type = "export";
            width = "1";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT zs_cke
         {
            type = "export";
            width = "1";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT zs_cs_n
         {
            type = "export";
            width = "1";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT zs_dq
         {
            type = "export";
            width = "16";
            direction = "inout";
            Is_Enabled = "1";
         }
         PORT zs_dqm
         {
            type = "export";
            width = "2";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT zs_ras_n
         {
            type = "export";
            width = "1";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT zs_we_n
         {
            type = "export";
            width = "1";
            direction = "output";
            Is_Enabled = "1";
         }
      }
      iss_model_name = "altera_memory";
      WIZARD_SCRIPT_ARGUMENTS 
      {
         register_data_in = "1";
         sim_model_base = "0";
         sdram_data_width = "16";
         sdram_addr_width = "13";
         sdram_row_width = "13";
         sdram_col_width = "9";
         sdram_num_chipselects = "1";
         sdram_num_banks = "4";
         refresh_period = "15.625";
         powerup_delay = "100.0";
         cas_latency = "3";
         t_rfc = "70.0";
         t_rp = "20.0";
         t_mrd = "3";
         t_rcd = "20.0";
         t_ac = "5.5";
         t_wr = "14.0";
         init_refresh_commands = "2";
         init_nop_delay = "0.0";
         shared_data = "0";
         sdram_bank_width = "2";
         tristate_bridge_slave = "";
         starvation_indicator = "0";
         is_initialized = "1";
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL a
            {
               name = "az_addr";
               radix = "hexadecimal";
            }
            SIGNAL b
            {
               name = "az_be_n";
               radix = "hexadecimal";
            }
            SIGNAL c
            {
               name = "az_cs";
            }
            SIGNAL d
            {
               name = "az_data";
               radix = "hexadecimal";
            }
            SIGNAL e
            {
               name = "az_rd_n";
            }
            SIGNAL f
            {
               name = "az_wr_n";
            }
            SIGNAL h
            {
               name = "za_data";
               radix = "hexadecimal";
            }
            SIGNAL i
            {
               name = "za_valid";
            }
            SIGNAL j
            {
               name = "za_waitrequest";
            }
            SIGNAL l
            {
               name = "CODE";
               radix = "ascii";
            }
            SIGNAL g
            {
               name = "clk";
            }
            SIGNAL k
            {
               name = "za_cannotrefresh";
               suppress = "1";
            }
            SIGNAL m
            {
               name = "zs_addr";
               radix = "hexadecimal";
               suppress = "0";
            }
            SIGNAL n
            {
               name = "zs_ba";
               radix = "hexadecimal";
               suppress = "0";
            }
            SIGNAL o
            {
               name = "zs_cs_n";
               radix = "hexadecimal";
               suppress = "0";
            }
            SIGNAL p
            {
               name = "zs_ras_n";
               suppress = "0";
            }
            SIGNAL q
            {
               name = "zs_cas_n";
               suppress = "0";
            }
            SIGNAL r
            {
               name = "zs_we_n";
               suppress = "0";
            }
            SIGNAL s
            {
               name = "zs_dq";
               radix = "hexadecimal";
               suppress = "0";
            }
            SIGNAL t
            {
               name = "zs_dqm";
               radix = "hexadecimal";
               suppress = "0";
            }
            SIGNAL u
            {
               name = "zt_addr";
               radix = "hexadecimal";
               suppress = "1";
            }
            SIGNAL v
            {
               name = "zt_ba";
               radix = "hexadecimal";
               suppress = "1";
            }
            SIGNAL w
            {
               name = "zt_oe";
               suppress = "1";
            }
            SIGNAL x
            {
               name = "zt_cke";
               suppress = "1";
            }
            SIGNAL y
            {
               name = "zt_chipselect";
               suppress = "1";
            }
            SIGNAL z0
            {
               name = "zt_lock_n";
               suppress = "1";
            }
            SIGNAL z1
            {
               name = "zt_ras_n";
               suppress = "1";
            }
            SIGNAL z2
            {
               name = "zt_cas_n";
               suppress = "1";
            }
            SIGNAL z3
            {
               name = "zt_we_n";
               suppress = "1";
            }
            SIGNAL z4
            {
               name = "zt_cs_n";
               radix = "hexadecimal";
               suppress = "1";
            }
            SIGNAL z5
            {
               name = "zt_dqm";
               radix = "hexadecimal";
               suppress = "1";
            }
            SIGNAL z6
            {
               name = "zt_data";
               radix = "hexadecimal";
               suppress = "1";
            }
            SIGNAL z7
            {
               name = "tz_data";
               radix = "hexadecimal";
               suppress = "1";
            }
            SIGNAL z8
            {
               name = "tz_waitrequest";
               suppress = "1";
            }
         }
         Fix_Me_Up = "";
      }
      SYSTEM_BUILDER_INFO 
      {
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Default_Module_Name = "sdram";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         Disable_Simulation_Port_Wiring = "0";
         View 
         {
            MESSAGES 
            {
            }
            Settings_Summary = "16777216 x 16<br>
                Memory size: 32 MBytes<br>
                256 MBits
                ";
         }
      }
      class = "altera_avalon_new_sdram_controller";
      class_version = "7.08110";
   }
   MODULE jtag_uart
   {
      SLAVE avalon_jtag_slave
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT rst_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_irq
            {
               type = "irq";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT av_chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_address
            {
               type = "address";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_read_n
            {
               type = "read_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT av_write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT av_waitrequest
            {
               type = "waitrequest";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT dataavailable
            {
               type = "dataavailable";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT readyfordata
            {
               type = "readyfordata";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Has_IRQ = "1";
            Bus_Type = "avalon";
            Read_Wait_States = "peripheral_controlled";
            Write_Wait_States = "peripheral_controlled";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "1";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "1";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            JTAG_Hub_Base_Id = "262254";
            JTAG_Hub_Instance_Id = "0";
            Connection_Limit = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x000018c8";
            }
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "1";
            }
            Base_Address = "0x000018c8";
            Address_Group = "0";
         }
      }
      class = "altera_avalon_jtag_uart";
      class_version = "7.08110";
      iss_model_name = "altera_avalon_jtag_uart";
      WIZARD_SCRIPT_ARGUMENTS 
      {
         write_depth = "64";
         read_depth = "64";
         write_threshold = "8";
         read_threshold = "8";
         read_char_stream = "";
         showascii = "1";
         relativepath = "1";
         read_le = "0";
         write_le = "0";
         altera_show_unreleased_jtag_uart_features = "1";
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL av_chipselect
            {
               name = "av_chipselect";
            }
            SIGNAL av_address
            {
               name = "av_address";
               radix = "hexadecimal";
            }
            SIGNAL av_read_n
            {
               name = "av_read_n";
            }
            SIGNAL av_readdata
            {
               name = "av_readdata";
               radix = "hexadecimal";
            }
            SIGNAL av_write_n
            {
               name = "av_write_n";
            }
            SIGNAL av_writedata
            {
               name = "av_writedata";
               radix = "hexadecimal";
            }
            SIGNAL av_waitrequest
            {
               name = "av_waitrequest";
            }
            SIGNAL dataavailable
            {
               name = "dataavailable";
            }
            SIGNAL readyfordata
            {
               name = "readyfordata";
            }
            SIGNAL av_irq
            {
               name = "av_irq";
            }
         }
         INTERACTIVE_IN drive
         {
            enable = "0";
            file = "_input_data_stream.dat";
            mutex = "_input_data_mutex.dat";
            log = "_in.log";
            rate = "100";
            signals = "temp,list";
            exe = "nios2-terminal";
         }
         INTERACTIVE_OUT log
         {
            enable = "1";
            exe = "perl -- atail-f.pl";
            file = "_output_stream.dat";
            radix = "ascii";
            signals = "temp,list";
         }
         Fix_Me_Up = "";
      }
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         Instantiate_In_System_Module = "1";
         Iss_Launch_Telnet = "0";
         Top_Level_Ports_Are_Enumerated = "1";
         View 
         {
            MESSAGES 
            {
            }
            Settings_Summary = "<br>Write Depth: 64; Write IRQ Threshold: 8
                <br>Read  Depth: 64; Read  IRQ Threshold: 8";
         }
      }
   }
   MODULE spi_touch
   {
      SLAVE spi_control_port
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT irq
            {
               type = "irq";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT data_from_cpu
            {
               type = "writedata";
               width = "16";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT data_to_cpu
            {
               type = "readdata";
               width = "16";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT mem_addr
            {
               type = "address";
               width = "3";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT read_n
            {
               type = "read_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT spi_select
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT dataavailable
            {
               type = "dataavailable";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT endofpacket
            {
               type = "endofpacket";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
            PORT readyfordata
            {
               type = "readyfordata";
               width = "1";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Has_IRQ = "1";
            Bus_Type = "avalon";
            Write_Wait_States = "1cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "16";
            Address_Width = "3";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00001800";
            }
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "2";
            }
            Base_Address = "0x00001800";
            Address_Group = "0";
         }
      }
      PORT_WIRING 
      {
         PORT MISO
         {
            type = "export";
            width = "1";
            direction = "input";
            Is_Enabled = "1";
         }
         PORT MOSI
         {
            type = "export";
            width = "1";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT SCLK
         {
            type = "export";
            width = "1";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT SS_n
         {
            type = "export";
            width = "1";
            direction = "output";
            Is_Enabled = "1";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         databits = "8";
         datawidth = "16";
         targetclock = "1000000";
         clockunits = "Hz";
         clockmult = "1";
         numslaves = "1";
         ismaster = "1";
         clockpolarity = "0";
         clockphase = "0";
         lsbfirst = "0";
         extradelay = "0";
         insert_sync = "0";
         sync_reg_depth = "2";
         disableAvalonFlowControl = "0";
         targetssdelay = "0.0";
         delayunits = "ns";
         delaymult = "1.0E-9";
         prefix = "spi_";
      }
      class = "altera_avalon_spi";
      class_version = "7.08110";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         Instantiate_In_System_Module = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         View 
         {
            MESSAGES 
            {
            }
         }
      }
   }
   MODULE lcd_cs
   {
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "2";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "2";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00001820";
            }
            Base_Address = "0x00001820";
            Has_IRQ = "0";
            Address_Group = "0";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Readable = "0";
            Is_Writable = "1";
         }
      }
      PORT_WIRING 
      {
         PORT out_port
         {
            type = "export";
            width = "32";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT in_port
         {
            direction = "input";
            Is_Enabled = "0";
            width = "32";
         }
         PORT bidir_port
         {
            direction = "inout";
            Is_Enabled = "0";
            width = "32";
         }
      }
      class = "altera_avalon_pio";
      class_version = "7.08110";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         Date_Modified = "";
         View 
         {
            MESSAGES 
            {
            }
            Settings_Summary = " 32-bit PIO using <br>
					
					
					 output pins";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0";
         has_tri = "0";
         has_out = "1";
         has_in = "0";
         capture = "0";
         Data_Width = "1";
         reset_value = "0";
         edge_type = "NONE";
         irq_type = "NONE";
         bit_clearing_edge_register = "0";
         bit_modifying_output_register = "0";
      }
      HDL_INFO 
      {
         # The list of files associated with this module (for synthesis
         # and other purposes) depends on the users' wizard-choices.
         # This section will be filled-in by the Generator_Program
         # after the module logic has been created and the
         # various filenames are known.
      }
   }
   MODULE touch_cs
   {
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "2";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "2";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00001830";
            }
            Base_Address = "0x00001830";
            Has_IRQ = "0";
            Address_Group = "0";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Readable = "0";
            Is_Writable = "1";
         }
      }
      PORT_WIRING 
      {
         PORT out_port
         {
            type = "export";
            width = "32";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT in_port
         {
            direction = "input";
            Is_Enabled = "0";
            width = "32";
         }
         PORT bidir_port
         {
            direction = "inout";
            Is_Enabled = "0";
            width = "32";
         }
      }
      class = "altera_avalon_pio";
      class_version = "7.08110";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         Date_Modified = "";
         View 
         {
            MESSAGES 
            {
            }
            Settings_Summary = " 32-bit PIO using <br>
					
					
					 output pins";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0";
         has_tri = "0";
         has_out = "1";
         has_in = "0";
         capture = "0";
         Data_Width = "1";
         reset_value = "0";
         edge_type = "NONE";
         irq_type = "NONE";
         bit_clearing_edge_register = "0";
         bit_modifying_output_register = "0";
      }
      HDL_INFO 
      {
         # The list of files associated with this module (for synthesis
         # and other purposes) depends on the users' wizard-choices.
         # This section will be filled-in by the Generator_Program
         # after the module logic has been created and the
         # various filenames are known.
      }
   }
   MODULE lcd_rs
   {
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "2";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "2";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00001840";
            }
            Base_Address = "0x00001840";
            Has_IRQ = "0";
            Address_Group = "0";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Readable = "0";
            Is_Writable = "1";
         }
      }
      PORT_WIRING 
      {
         PORT out_port
         {
            type = "export";
            width = "32";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT in_port
         {
            direction = "input";
            Is_Enabled = "0";
            width = "32";
         }
         PORT bidir_port
         {
            direction = "inout";
            Is_Enabled = "0";
            width = "32";
         }
      }
      class = "altera_avalon_pio";
      class_version = "7.08110";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         Date_Modified = "";
         View 
         {
            MESSAGES 
            {
            }
            Settings_Summary = " 32-bit PIO using <br>
					
					
					 output pins";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0";
         has_tri = "0";
         has_out = "1";
         has_in = "0";
         capture = "0";
         Data_Width = "1";
         reset_value = "0";
         edge_type = "NONE";
         irq_type = "NONE";
         bit_clearing_edge_register = "0";
         bit_modifying_output_register = "0";
      }
      HDL_INFO 
      {
         # The list of files associated with this module (for synthesis
         # and other purposes) depends on the users' wizard-choices.
         # This section will be filled-in by the Generator_Program
         # after the module logic has been created and the
         # various filenames are known.
      }
   }
   MODULE touch_irq
   {
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "2";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "2";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00001850";
            }
            Base_Address = "0x00001850";
            Has_IRQ = "0";
            Address_Group = "0";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Readable = "1";
            Is_Writable = "0";
         }
      }
      PORT_WIRING 
      {
         PORT in_port
         {
            type = "export";
            width = "32";
            direction = "input";
            Is_Enabled = "1";
         }
         PORT out_port
         {
            direction = "output";
            Is_Enabled = "0";
            width = "32";
         }
         PORT bidir_port
         {
            direction = "inout";
            Is_Enabled = "0";
            width = "32";
         }
      }
      class = "altera_avalon_pio";
      class_version = "7.08110";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         Date_Modified = "";
         View 
         {
            MESSAGES 
            {
            }
            Settings_Summary = " 32-bit PIO using <br>
					
					 input pins with edge type NONE and interrupt source NONE
					";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0";
         has_tri = "0";
         has_out = "0";
         has_in = "1";
         capture = "0";
         Data_Width = "1";
         reset_value = "0";
         edge_type = "NONE";
         irq_type = "NONE";
         bit_clearing_edge_register = "0";
         bit_modifying_output_register = "0";
      }
      HDL_INFO 
      {
         # The list of files associated with this module (for synthesis
         # and other purposes) depends on the users' wizard-choices.
         # This section will be filled-in by the Generator_Program
         # after the module logic has been created and the
         # various filenames are known.
      }
   }
   MODULE reset
   {
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "2";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "2";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00001860";
            }
            Base_Address = "0x00001860";
            Has_IRQ = "0";
            Address_Group = "0";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Readable = "0";
            Is_Writable = "1";
         }
      }
      PORT_WIRING 
      {
         PORT out_port
         {
            type = "export";
            width = "32";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT in_port
         {
            direction = "input";
            Is_Enabled = "0";
            width = "32";
         }
         PORT bidir_port
         {
            direction = "inout";
            Is_Enabled = "0";
            width = "32";
         }
      }
      class = "altera_avalon_pio";
      class_version = "7.08110";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         Date_Modified = "";
         View 
         {
            MESSAGES 
            {
            }
            Settings_Summary = " 32-bit PIO using <br>
					
					
					 output pins";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0";
         has_tri = "0";
         has_out = "1";
         has_in = "0";
         capture = "0";
         Data_Width = "1";
         reset_value = "0";
         edge_type = "NONE";
         irq_type = "NONE";
         bit_clearing_edge_register = "0";
         bit_modifying_output_register = "0";
      }
      HDL_INFO 
      {
         # The list of files associated with this module (for synthesis
         # and other purposes) depends on the users' wizard-choices.
         # This section will be filled-in by the Generator_Program
         # after the module logic has been created and the
         # various filenames are known.
      }
   }
   MODULE lcd_wr
   {
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "2";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "2";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00001870";
            }
            Base_Address = "0x00001870";
            Has_IRQ = "0";
            Address_Group = "0";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Readable = "0";
            Is_Writable = "1";
         }
      }
      PORT_WIRING 
      {
         PORT out_port
         {
            type = "export";
            width = "32";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT in_port
         {
            direction = "input";
            Is_Enabled = "0";
            width = "32";
         }
         PORT bidir_port
         {
            direction = "inout";
            Is_Enabled = "0";
            width = "32";
         }
      }
      class = "altera_avalon_pio";
      class_version = "7.08110";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         Date_Modified = "";
         View 
         {
            MESSAGES 
            {
            }
            Settings_Summary = " 32-bit PIO using <br>
					
					
					 output pins";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0";
         has_tri = "0";
         has_out = "1";
         has_in = "0";
         capture = "0";
         Data_Width = "1";
         reset_value = "0";
         edge_type = "NONE";
         irq_type = "NONE";
         bit_clearing_edge_register = "0";
         bit_modifying_output_register = "0";
      }
      HDL_INFO 
      {
         # The list of files associated with this module (for synthesis
         # and other purposes) depends on the users' wizard-choices.
         # This section will be filled-in by the Generator_Program
         # after the module logic has been created and the
         # various filenames are known.
      }
   }
   MODULE lcd32_data
   {
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "2";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "2";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00001880";
            }
            Base_Address = "0x00001880";
            Has_IRQ = "0";
            Address_Group = "0";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Readable = "1";
            Is_Writable = "1";
         }
      }
      PORT_WIRING 
      {
         PORT bidir_port
         {
            type = "export";
            width = "32";
            direction = "inout";
            Is_Enabled = "1";
         }
         PORT in_port
         {
            direction = "input";
            Is_Enabled = "0";
            width = "32";
         }
         PORT out_port
         {
            direction = "output";
            Is_Enabled = "0";
            width = "32";
         }
      }
      class = "altera_avalon_pio";
      class_version = "7.08110";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         Date_Modified = "";
         View 
         {
            MESSAGES 
            {
            }
            Settings_Summary = " 32-bit PIO using <br>
					 tri-state pins with edge type NONE and interrupt source NONE
					
					";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0";
         has_tri = "1";
         has_out = "0";
         has_in = "0";
         capture = "0";
         Data_Width = "16";
         reset_value = "0";
         edge_type = "NONE";
         irq_type = "NONE";
         bit_clearing_edge_register = "0";
         bit_modifying_output_register = "0";
      }
      HDL_INFO 
      {
         # The list of files associated with this module (for synthesis
         # and other purposes) depends on the users' wizard-choices.
         # This section will be filled-in by the Generator_Program
         # after the module logic has been created and the
         # various filenames are known.
      }
   }
   MODULE lcd_rd
   {
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "2";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "2";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x00001890";
            }
            Base_Address = "0x00001890";
            Has_IRQ = "0";
            Address_Group = "0";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Readable = "0";
            Is_Writable = "1";
         }
      }
      PORT_WIRING 
      {
         PORT out_port
         {
            type = "export";
            width = "32";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT in_port
         {
            direction = "input";
            Is_Enabled = "0";
            width = "32";
         }
         PORT bidir_port
         {
            direction = "inout";
            Is_Enabled = "0";
            width = "32";
         }
      }
      class = "altera_avalon_pio";
      class_version = "7.08110";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         Date_Modified = "";
         View 
         {
            MESSAGES 
            {
            }
            Settings_Summary = " 32-bit PIO using <br>
					
					
					 output pins";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0";
         has_tri = "0";
         has_out = "1";
         has_in = "0";
         capture = "0";
         Data_Width = "1";
         reset_value = "0";
         edge_type = "NONE";
         irq_type = "NONE";
         bit_clearing_edge_register = "0";
         bit_modifying_output_register = "0";
      }
      HDL_INFO 
      {
         # The list of files associated with this module (for synthesis
         # and other purposes) depends on the users' wizard-choices.
         # This section will be filled-in by the Generator_Program
         # after the module logic has been created and the
         # various filenames are known.
      }
   }
   MODULE bl_p
   {
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "2";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "2";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x000018a0";
            }
            Base_Address = "0x000018a0";
            Has_IRQ = "0";
            Address_Group = "0";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Readable = "0";
            Is_Writable = "1";
         }
      }
      PORT_WIRING 
      {
         PORT out_port
         {
            type = "export";
            width = "32";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT in_port
         {
            direction = "input";
            Is_Enabled = "0";
            width = "32";
         }
         PORT bidir_port
         {
            direction = "inout";
            Is_Enabled = "0";
            width = "32";
         }
      }
      class = "altera_avalon_pio";
      class_version = "7.08110";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         Date_Modified = "";
         View 
         {
            MESSAGES 
            {
            }
            Settings_Summary = " 32-bit PIO using <br>
					
					
					 output pins";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0";
         has_tri = "0";
         has_out = "1";
         has_in = "0";
         capture = "0";
         Data_Width = "1";
         reset_value = "0";
         edge_type = "NONE";
         irq_type = "NONE";
         bit_clearing_edge_register = "0";
         bit_modifying_output_register = "0";
      }
      HDL_INFO 
      {
         # The list of files associated with this module (for synthesis
         # and other purposes) depends on the users' wizard-choices.
         # This section will be filled-in by the Generator_Program
         # after the module logic has been created and the
         # various filenames are known.
      }
   }
   MODULE bl_n
   {
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               type = "reset_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT address
            {
               type = "address";
               width = "2";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT write_n
            {
               type = "write_n";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               type = "writedata";
               width = "32";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               type = "chipselect";
               width = "1";
               direction = "input";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               type = "readdata";
               width = "32";
               direction = "output";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Write_Wait_States = "0cycles";
            Read_Wait_States = "1cycles";
            Hold_Time = "0cycles";
            Setup_Time = "0cycles";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Well_Behaved_Waitrequest = "0";
            Is_Nonvolatile_Storage = "0";
            Read_Latency = "0";
            Is_Memory_Device = "0";
            Maximum_Pending_Read_Transactions = "0";
            Minimum_Uninterrupted_Run_Length = "1";
            Accepts_Internal_Connections = "1";
            Write_Latency = "0";
            Is_Flash = "0";
            Data_Width = "32";
            Address_Width = "2";
            Maximum_Burst_Size = "1";
            Register_Incoming_Signals = "0";
            Register_Outgoing_Signals = "0";
            Interleave_Bursts = "0";
            Linewrap_Bursts = "0";
            Burst_On_Burst_Boundaries_Only = "0";
            Always_Burst_Max_Burst = "0";
            Is_Big_Endian = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu/data_master
            {
               priority = "1";
               Offset_Address = "0x000018b0";
            }
            Base_Address = "0x000018b0";
            Has_IRQ = "0";
            Address_Group = "0";
            IRQ_MASTER cpu/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Readable = "0";
            Is_Writable = "1";
         }
      }
      PORT_WIRING 
      {
         PORT out_port
         {
            type = "export";
            width = "32";
            direction = "output";
            Is_Enabled = "1";
         }
         PORT in_port
         {
            direction = "input";
            Is_Enabled = "0";
            width = "32";
         }
         PORT bidir_port
         {
            direction = "inout";
            Is_Enabled = "0";
            width = "32";
         }
      }
      class = "altera_avalon_pio";
      class_version = "7.08110";
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         Has_Clock = "1";
         Date_Modified = "";
         View 
         {
            MESSAGES 
            {
            }
            Settings_Summary = " 32-bit PIO using <br>
					
					
					 output pins";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0";
         has_tri = "0";
         has_out = "1";
         has_in = "0";
         capture = "0";
         Data_Width = "1";
         reset_value = "0";
         edge_type = "NONE";
         irq_type = "NONE";
         bit_clearing_edge_register = "0";
         bit_modifying_output_register = "0";
      }
      HDL_INFO 
      {
         # The list of files associated with this module (for synthesis
         # and other purposes) depends on the users' wizard-choices.
         # This section will be filled-in by the Generator_Program
         # after the module logic has been created and the
         # various filenames are known.
      }
   }
}
