Arduino Reference - DigitalRead

Arduino

Reference Language | Libraries | Comparison | Changes

## digitalRead()

#### Description

Reads the value from a specified digital pin, either HIGH or LOW.

#### Syntax

digitalRead(pin)

#### Parameters

pin: the number of the digital pin you want to read (int)

#### Returns

HIGH or LOW

#### Example

    int ledPin = 13; // LED connected to digital pin 13
    int inPin = 7;   // pushbutton connected to digital pin 7
    int val = 0;     // variable to store the read value

    void setup()
    {
      pinMode(ledPin, OUTPUT);      // sets the digital pin 13 as output
      pinMode(inPin, INPUT);      // sets the digital pin 7 as input
    }

    void loop()
    {
      val = digitalRead(inPin);   // read the input pin
      digitalWrite(ledPin, val);    // sets the LED to the button's value
    }

Sets pin 13 to the same value as the pin 7, which is an input.

#### Note

If the pin isn't connected to anything, digitalRead() can return either HIGH or LOW (and this can change randomly).

The analog input pins can be used as digital pins, referred to as A0, A1, etc.

#### See also

- pinMode()
- digitalWrite()
- Tutorial: Digital Pins

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes