Arduino Reference - StreamReadBytes

Arduino

Reference Language | Libraries | Comparison | Changes

## readBytes()

#### Description

readBytes() read characters from a stream into a buffer. The function terminates if the determined length has been read, or it times out (see setTimeout()).

readBytes() returns the number of characters placed in the buffer. A 0 means no valid data was found.

This function is part of the Stream class, and is called by any class that inherits from it (Wire, Serial, etc). See the Stream class main page for more information.

#### Syntax

stream.readBytes(buffer, length)

#### Parameters

stream : an instance of a class that inherits from Stream.
buffer: the buffer to store the bytes in (char[] or byte[])
length : the number of bytes to read (int)

#### Returns

byte

#### See also

- Stream

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes