Arduino Reference - LiquidCrystalCreateChar

Arduino

Reference Language | Libraries | Comparison | Changes

LiquidCrystal

## createChar()

#### Description

Create a custom character (gylph) for use on the LCD. Up to eight characters of 5x8 pixels are supported (numbered 0 to 7). The appearance of each custom character is specified by an array of eight bytes, one for each row. The five least significant bits of each byte determine the pixels in that row. To display a custom character on the screen, write() its number.

#### Syntax

lcd.createChar(num, data)

#### Parameters

lcd: a variable of type LiquidCrystal

num: which character to create (0 to 7)

data: the character's pixel data

#### Example

    #include <LiquidCrystal.h>

    LiquidCrystal lcd(12, 11, 5, 4, 3, 2);

    byte smiley[8] = {
      B00000,
      B10001,
      B00000,
      B00000,
      B10001,
      B01110,
      B00000,
    };

    void setup() {
      lcd.createChar(0, smiley);
      lcd.begin(16, 2);
      lcd.write(0);
    }

    void loop() {}

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes