Not committed
--------------------------------------------------------------------------------
--- opcodes/avr-dis.c.orig	2007-08-06 13:58:38.000000000 -0600
+++ opcodes/avr-dis.c	2008-04-09 16:37:17.233737600 -0600
@@ -50,7 +50,7 @@ static const char * comment_start = "0x"
 
 static int
 avr_operand (unsigned int insn, unsigned int insn2, unsigned int pc, int constraint,
-             char *buf, char *comment, int regs, int *sym, bfd_vma *sym_addr)
+             char *opcode_str, char *buf, char *comment, int regs, int *sym, bfd_vma *sym_addr)
 {
   int ok = 1;
   *sym = 0;
@@ -118,8 +118,18 @@ avr_operand (unsigned int insn, unsigned
 
     case 'z':
       *buf++ = 'Z';
-      if (insn & 0x1)
-	*buf++ = '+';
+
+      /* Check for post-increment. */
+      char *s;
+      for (s = opcode_str; *s; ++s)
+        {
+          if (*s == '+')
+            {
+              *buf++ = '+';
+              break;
+            }
+        }
+
       *buf = '\0';
       if (AVR_UNDEF_P (insn))
 	sprintf (comment, _("undefined"));
@@ -226,6 +236,10 @@ avr_operand (unsigned int insn, unsigned
 	sprintf (comment, "%d", x);
       }
       break;
+
+    case 'E':
+      sprintf (buf, "%d", (insn >> 4) & 15);
+      break;
       
     case '?':
       *buf = '\0';
@@ -331,7 +345,8 @@ print_insn_avr (bfd_vma addr, disassembl
 
   if (opcode->name)
     {
-      char *op = opcode->constraints;
+      char *constraints = opcode->constraints;
+      char *opcode_str = opcode->opcode;
 
       insn2 = 0;
       ok = 1;
@@ -342,14 +357,14 @@ print_insn_avr (bfd_vma addr, disassembl
 	  cmd_len = 4;
 	}
 
-      if (*op && *op != '?')
+      if (*constraints && *constraints != '?')
 	{
-	  int regs = REGISTER_P (*op);
+	  int regs = REGISTER_P (*constraints);
 
-	  ok = avr_operand (insn, insn2, addr, *op, op1, comment1, 0, &sym_op1, &sym_addr1);
+	  ok = avr_operand (insn, insn2, addr, *constraints, opcode_str, op1, comment1, 0, &sym_op1, &sym_addr1);
 
-	  if (ok && *(++op) == ',')
-	    ok = avr_operand (insn, insn2, addr, *(++op), op2,
+	  if (ok && *(++constraints) == ',')
+	    ok = avr_operand (insn, insn2, addr, *(++constraints), opcode_str, op2,
 			      *comment1 ? comment2 : comment1, regs, &sym_op2, &sym_addr2);
 	}
     }
--- gas/config/tc-avr.c.orig	2008-08-29 10:58:02.000000000 -0600
+++ gas/config/tc-avr.c	2008-09-22 14:11:05.345349200 -0600
@@ -27,20 +27,21 @@
 
 struct avr_opcodes_s
 {
-  char *        name;
-  char *        constraints;
-  int           insn_size;		/* In words.  */
-  int           isa;
+  char *name;
+  char *constraints;
+  char *opcode;
+  int insn_size;		/* In words.  */
+  int isa;
   unsigned int  bin_opcode;
 };
 
 #define AVR_INSN(NAME, CONSTR, OPCODE, SIZE, ISA, BIN) \
-{#NAME, CONSTR, SIZE, ISA, BIN},
+{#NAME, CONSTR, OPCODE, SIZE, ISA, BIN},
 
 struct avr_opcodes_s avr_opcodes[] =
 {
   #include "opcode/avr.h"
-  {NULL, NULL, 0, 0, 0}
+  {NULL, NULL, NULL, 0, 0, 0}
 };
 
 const char comment_chars[] = ";";
@@ -79,6 +80,13 @@ static struct mcu_type_s mcu_types[] =
   {"avr5",       AVR_ISA_AVR51,   bfd_mach_avr5},
   {"avr51",      AVR_ISA_AVR51,   bfd_mach_avr51},
   {"avr6",       AVR_ISA_AVR6,    bfd_mach_avr6},
+  {"avrxmega1",  AVR_ISA_XMEGA,   bfd_mach_avrxmega1},
+  {"avrxmega2",  AVR_ISA_XMEGA,   bfd_mach_avrxmega2},
+  {"avrxmega3",  AVR_ISA_XMEGA,   bfd_mach_avrxmega3},
+  {"avrxmega4",  AVR_ISA_XMEGA,   bfd_mach_avrxmega4},
+  {"avrxmega5",  AVR_ISA_XMEGA,   bfd_mach_avrxmega5},
+  {"avrxmega6",  AVR_ISA_XMEGA,   bfd_mach_avrxmega6},
+  {"avrxmega7",  AVR_ISA_XMEGA,   bfd_mach_avrxmega7},
   {"at90s1200",  AVR_ISA_1200,    bfd_mach_avr1},
   {"attiny11",   AVR_ISA_AVR1,    bfd_mach_avr1},
   {"attiny12",   AVR_ISA_AVR1,    bfd_mach_avr1},
@@ -185,6 +193,8 @@ static struct mcu_type_s mcu_types[] =
   {"at90usb1287",AVR_ISA_AVR51,   bfd_mach_avr51},
   {"atmega2560", AVR_ISA_AVR6,    bfd_mach_avr6},
   {"atmega2561", AVR_ISA_AVR6,    bfd_mach_avr6},
+  {"atxmega64a1", AVR_ISA_XMEGA,  bfd_mach_avrxmega5},
+  {"atxmega128a1", AVR_ISA_XMEGA, bfd_mach_avrxmega7},
   {NULL, 0, 0}
 };
 
@@ -789,7 +799,12 @@ avr_operand (struct avr_opcodes_s *opcod
       if (*str == '+')
 	{
 	  ++str;
-	  op_mask |= 1;
+          char *s;
+          for (s = opcode->opcode; *s; ++s)
+            {
+              if (*s == '+')
+                op_mask |= (1 << (15 - (s - opcode->opcode)));
+            }
 	}
 
       /* attiny26 can do "lpm" and "lpm r,Z" but not "lpm r,Z+".  */
@@ -906,6 +921,16 @@ avr_operand (struct avr_opcodes_s *opcod
       }
       break;
 
+    case 'E':
+      {
+	unsigned int x;
+
+	x = avr_get_constant (str, 15);
+	str = input_line_pointer;
+	op_mask |= (x << 4);
+      }
+      break;
+    
     case '?':
       break;
 
--- include/opcode/avr.h.orig	2008-04-09 14:03:00.411627300 -0600
+++ include/opcode/avr.h	2008-04-09 16:34:28.329060900 -0600
@@ -30,6 +30,8 @@
 #define AVR_ISA_BRK   0x0400 /* device has BREAK (on-chip debug) */
 #define AVR_ISA_EIND  0x0800 /* device has >128K program memory (none yet) */
 #define AVR_ISA_MOVW  0x1000 /* device has MOVW */
+#define AVR_ISA_SPMX  0x2000 /* device has SPM Z[+] */
+#define AVR_ISA_DES   0x4000 /* device has DES */
 
 #define AVR_ISA_TINY1 (AVR_ISA_1200 | AVR_ISA_LPM)
 #define AVR_ISA_PWMx  (AVR_ISA_M8   | AVR_ISA_BRK)
@@ -53,6 +55,8 @@
 #define AVR_ISA_94K   (AVR_ISA_M603 | AVR_ISA_MUL | AVR_ISA_MOVW | AVR_ISA_LPMX)
 #define AVR_ISA_M323  (AVR_ISA_M161 | AVR_ISA_BRK)
 #define AVR_ISA_M128  (AVR_ISA_M323 | AVR_ISA_ELPM | AVR_ISA_ELPMX)
+#define AVR_ISA_M256  (AVR_ISA_M128 | AVR_ISA_EIND)
+#define AVR_ISA_XMEGA (AVR_ISA_M256 | AVR_ISA_SPMX | AVR_ISA_DES)
 
 #define AVR_ISA_ALL   0xFFFF
 
@@ -98,6 +102,7 @@
    L - signed pc relative offset from -2048 to 2047
    h - absolute code address (call, jmp)
    S - immediate value from 0 to 7 (S = s << 4)
+   E - immediate value from 0 to 15, shifted left by 4 (des)
    ? - use this opcode entry if no parameters, else use next opcode entry
 
    Order is important - some binary opcodes have more than one name,
@@ -158,7 +163,8 @@ AVR_INSN (reti, "",    "1001010100011000
 AVR_INSN (sleep,"",    "1001010110001000", 1, AVR_ISA_1200, 0x9588)
 AVR_INSN (break,"",    "1001010110011000", 1, AVR_ISA_BRK,  0x9598)
 AVR_INSN (wdr,  "",    "1001010110101000", 1, AVR_ISA_1200, 0x95a8)
-AVR_INSN (spm,  "",    "1001010111101000", 1, AVR_ISA_SPM,  0x95e8)
+AVR_INSN (spm,  "?",   "1001010111101000", 1, AVR_ISA_SPM,  0x95e8)
+AVR_INSN (spm,  "z",   "10010101111+1000", 1, AVR_ISA_SPMX, 0x95e8)
 
 AVR_INSN (adc,  "r,r", "000111rdddddrrrr", 1, AVR_ISA_1200, 0x1c00)
 AVR_INSN (add,  "r,r", "000011rdddddrrrr", 1, AVR_ISA_1200, 0x0c00)
@@ -272,3 +278,6 @@ AVR_INSN (st,   "e,r", "100!001rrrrree-+
 AVR_INSN (eicall, "",  "1001010100011001", 1, AVR_ISA_EIND, 0x9519)
 AVR_INSN (eijmp, "",   "1001010000011001", 1, AVR_ISA_EIND, 0x9419)
 
+/* DES instruction for encryption and decryption */
+AVR_INSN (des,  "E",   "10010100EEEE1011", 1, AVR_ISA_DES,  0x940B)
+
Index: bfd/archures.c
===================================================================
RCS file: /cvs/src/src/bfd/archures.c,v
retrieving revision 1.130
diff -a -u -p -r1.130 archures.c
--- bfd/archures.c	4 Feb 2008 19:15:50 -0000	1.130
+++ bfd/archures.c	14 Feb 2008 18:01:43 -0000
@@ -352,6 +352,13 @@ DESCRIPTION
 .#define bfd_mach_avr4		4
 .#define bfd_mach_avr5		5
 .#define bfd_mach_avr6		6
+.#define bfd_mach_avrxmega1 101
+.#define bfd_mach_avrxmega2 102
+.#define bfd_mach_avrxmega3 103
+.#define bfd_mach_avrxmega4 104
+.#define bfd_mach_avrxmega5 105
+.#define bfd_mach_avrxmega6 106
+.#define bfd_mach_avrxmega7 107
 .  bfd_arch_bfin,        {* ADI Blackfin *}
 .#define bfd_mach_bfin          1
 .  bfd_arch_cr16,       {* National Semiconductor CompactRISC (ie CR16). *}
--- bfd/cpu-avr.c.orig	2008-08-08 23:35:12.000000000 -0600
+++ bfd/cpu-avr.c	2008-09-22 14:14:33.969548200 -0600
@@ -126,7 +126,29 @@ static const bfd_arch_info_type arch_inf
   N (22, bfd_mach_avr51, "avr:51", FALSE, & arch_info_struct[9]),
 
   /* 3-Byte PC.  */
-  N (22, bfd_mach_avr6, "avr:6", FALSE, NULL)
+  N (22, bfd_mach_avr6, "avr:6", FALSE, & arch_info_struct[10]),
+  
+  /* Xmega 1 */
+  N (24, bfd_mach_avrxmega1, "avr:101", FALSE, & arch_info_struct[11]),
+
+  /* Xmega 2 */
+  N (24, bfd_mach_avrxmega2, "avr:102", FALSE, & arch_info_struct[12]),
+  
+  /* Xmega 3 */
+  N (24, bfd_mach_avrxmega3, "avr:103", FALSE, & arch_info_struct[13]),
+  
+  /* Xmega 4 */
+  N (24, bfd_mach_avrxmega4, "avr:104", FALSE, & arch_info_struct[14]),
+  
+  /* Xmega 5 */
+  N (24, bfd_mach_avrxmega5, "avr:105", FALSE, & arch_info_struct[15]),
+  
+  /* Xmega 6 */
+  N (24, bfd_mach_avrxmega6, "avr:106", FALSE, & arch_info_struct[16]),
+  
+  /* Xmega 7 */
+  N (24, bfd_mach_avrxmega7, "avr:107", FALSE, NULL)
+  
 };
 
 const bfd_arch_info_type bfd_avr_arch =
--- include/elf/avr.h.orig	2008-08-08 23:35:13.000000000 -0600
+++ include/elf/avr.h	2008-09-22 14:16:17.550944200 -0600
@@ -40,6 +40,13 @@
 #define E_AVR_MACH_AVR5 5
 #define E_AVR_MACH_AVR51 51
 #define E_AVR_MACH_AVR6 6 
+#define E_AVR_MACH_XMEGA1 101
+#define E_AVR_MACH_XMEGA2 102
+#define E_AVR_MACH_XMEGA3 103
+#define E_AVR_MACH_XMEGA4 104
+#define E_AVR_MACH_XMEGA5 105
+#define E_AVR_MACH_XMEGA6 106
+#define E_AVR_MACH_XMEGA7 107
 
 /* Relocations.  */
 START_RELOC_NUMBERS (elf_avr_reloc_type)
Index: ld/Makefile.am
===================================================================
RCS file: /cvs/src/src/ld/Makefile.am,v
retrieving revision 1.244
diff -a -u -p -r1.244 Makefile.am
--- ld/Makefile.am	24 Oct 2007 04:56:47 -0000	1.244
+++ ld/Makefile.am	14 Feb 2008 18:01:45 -0000
@@ -138,6 +138,13 @@ ALL_EMULATIONS = \
 	eavr4.o \
 	eavr5.o \
 	eavr6.o \
+	eavrxmega1.o \
+	eavrxmega2.o \
+	eavrxmega3.o \
+	eavrxmega4.o \
+	eavrxmega5.o \
+	eavrxmega6.o \
+	eavrxmega7.o \
 	ecoff_i860.o \
 	ecoff_sparc.o \
 	eelf32_spu.o \
@@ -622,6 +629,34 @@ eavr6.c: $(srcdir)/emulparams/avr6.sh $(
   $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
   ${GEN_DEPENDS}
 	${GENSCRIPTS} avr6 "$(tdir_avr2)"
+eavrxmega1.c: $(srcdir)/emulparams/avrxmega1.sh \
+  $(srcdir)/emultempl/avrelf.em $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
+  ${GEN_DEPENDS}
+	${GENSCRIPTS} avrxmega1 "$(tdir_avr2)"
+eavrxmega2.c: $(srcdir)/emulparams/avrxmega2.sh \
+  $(srcdir)/emultempl/avrelf.em $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
+  ${GEN_DEPENDS}
+	${GENSCRIPTS} avrxmega2 "$(tdir_avr2)"
+eavrxmega3.c: $(srcdir)/emulparams/avrxmega3.sh \
+  $(srcdir)/emultempl/avrelf.em $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
+  ${GEN_DEPENDS}
+	${GENSCRIPTS} avrxmega3 "$(tdir_avr2)"
+eavrxmega4.c: $(srcdir)/emulparams/avrxmega4.sh \
+  $(srcdir)/emultempl/avrelf.em $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
+  ${GEN_DEPENDS}
+	${GENSCRIPTS} avrxmega4 "$(tdir_avr2)"
+eavrxmega5.c: $(srcdir)/emulparams/avrxmega5.sh \
+  $(srcdir)/emultempl/avrelf.em $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
+  ${GEN_DEPENDS}
+	${GENSCRIPTS} avrxmega5 "$(tdir_avr2)"
+eavrxmega6.c: $(srcdir)/emulparams/avrxmega6.sh \
+  $(srcdir)/emultempl/avrelf.em $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
+  ${GEN_DEPENDS}
+	${GENSCRIPTS} avrxmega6 "$(tdir_avr2)"
+eavrxmega7.c: $(srcdir)/emulparams/avrxmega7.sh \
+  $(srcdir)/emultempl/avrelf.em $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
+  ${GEN_DEPENDS}
+	${GENSCRIPTS} avrxmega7 "$(tdir_avr2)"
 ecoff_i860.c: $(srcdir)/emulparams/coff_i860.sh \
   $(srcdir)/emultempl/generic.em $(srcdir)/scripttempl/i860coff.sc ${GEN_DEPENDS}
 	${GENSCRIPTS} coff_i860 "$(tdir_coff_i860)"
Index: ld/Makefile.in
===================================================================
RCS file: /cvs/src/src/ld/Makefile.in,v
retrieving revision 1.262
diff -a -u -p -r1.262 Makefile.in
--- ld/Makefile.in	24 Oct 2007 04:56:47 -0000	1.262
+++ ld/Makefile.in	14 Feb 2008 18:01:45 -0000
@@ -385,6 +385,13 @@ ALL_EMULATIONS = \
 	eavr4.o \
 	eavr5.o \
 	eavr6.o \
+	eavrxmega1.o \
+	eavrxmega2.o \
+	eavrxmega3.o \
+	eavrxmega4.o \
+	eavrxmega5.o \
+	eavrxmega6.o \
+	eavrxmega7.o \
 	ecoff_i860.o \
 	ecoff_sparc.o \
 	eelf32_spu.o \
@@ -1448,6 +1455,34 @@ eavr6.c: $(srcdir)/emulparams/avr6.sh $(
   $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
   ${GEN_DEPENDS}
 	${GENSCRIPTS} avr6 "$(tdir_avr2)"
+eavrxmega1.c: $(srcdir)/emulparams/avrxmega1.sh \
+  $(srcdir)/emultempl/avrelf.em $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
+  ${GEN_DEPENDS}
+	${GENSCRIPTS} avrxmega1 "$(tdir_avr2)"
+eavrxmega2.c: $(srcdir)/emulparams/avrxmega2.sh \
+  $(srcdir)/emultempl/avrelf.em $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
+  ${GEN_DEPENDS}
+	${GENSCRIPTS} avrxmega2 "$(tdir_avr2)"
+eavrxmega3.c: $(srcdir)/emulparams/avrxmega3.sh \
+  $(srcdir)/emultempl/avrelf.em $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
+  ${GEN_DEPENDS}
+	${GENSCRIPTS} avrxmega3 "$(tdir_avr2)"
+eavrxmega4.c: $(srcdir)/emulparams/avrxmega4.sh \
+  $(srcdir)/emultempl/avrelf.em $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
+  ${GEN_DEPENDS}
+	${GENSCRIPTS} avrxmega4 "$(tdir_avr2)"
+eavrxmega5.c: $(srcdir)/emulparams/avrxmega5.sh \
+  $(srcdir)/emultempl/avrelf.em $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
+  ${GEN_DEPENDS}
+	${GENSCRIPTS} avrxmega5 "$(tdir_avr2)"
+eavrxmega6.c: $(srcdir)/emulparams/avrxmega6.sh \
+  $(srcdir)/emultempl/avrelf.em $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
+  ${GEN_DEPENDS}
+	${GENSCRIPTS} avrxmega6 "$(tdir_avr2)"
+eavrxmega7.c: $(srcdir)/emulparams/avrxmega7.sh \
+  $(srcdir)/emultempl/avrelf.em $(ELF_DEPS) $(srcdir)/scripttempl/avr.sc \
+  ${GEN_DEPENDS}
+	${GENSCRIPTS} avrxmega7 "$(tdir_avr2)"
 ecoff_i860.c: $(srcdir)/emulparams/coff_i860.sh \
   $(srcdir)/emultempl/generic.em $(srcdir)/scripttempl/i860coff.sc ${GEN_DEPENDS}
 	${GENSCRIPTS} coff_i860 "$(tdir_coff_i860)"
--- ld/configure.tgt.orig	2008-08-08 23:35:13.000000000 -0600
+++ ld/configure.tgt	2008-09-22 14:17:42.272546800 -0600
@@ -107,7 +107,7 @@ xscale-*-coff)		targ_emul=armcoff ;;
 xscale-*-elf)		targ_emul=armelf
 			;;
 avr-*-*)		targ_emul=avr2
-			targ_extra_emuls="avr1 avr25 avr3 avr31 avr35 avr4 avr5 avr51 avr6"
+			targ_extra_emuls="avr1 avr25 avr3 avr31 avr35 avr4 avr5 avr51 avr6 avrxmega1 avrxmega2 avrxmega3 avrxmega4 avrxmega5 avrxmega6 avrxmega7"
 			;;
 bfin-*-elf)		targ_emul=elf32bfin;
 			targ_extra_emuls="elf32bfinfd"
Index: ld/emultempl/avrelf.em
===================================================================
RCS file: /cvs/src/src/ld/emultempl/avrelf.em,v
retrieving revision 1.5
diff -a -u -p -r1.5 avrelf.em
--- ld/emultempl/avrelf.em	17 Aug 2007 13:50:48 -0000	1.5
+++ ld/emultempl/avrelf.em	14 Feb 2008 18:01:45 -0000
@@ -71,8 +71,10 @@ avr_elf_${EMULATION_NAME}_before_allocat
 
   gld${EMULATION_NAME}_before_allocation ();
 
-  /* We only need stubs for the avr6 family.  */
-  if (strcmp ("${EMULATION_NAME}","avr6"))
+  /* We only need stubs for avr6, avrxmega6, and avrxmega7. */
+  if (strcmp ("${EMULATION_NAME}","avr6") 
+      && strcmp ("${EMULATION_NAME}","avrxmega6")
+      && strcmp ("${EMULATION_NAME}","avrxmega7") )
     avr_no_stubs = TRUE;
 
   avr_elf_set_global_bfd_parameters ();
--- /dev/null	2008-02-14 11:03:14.488602600 -0700
+++ ld/emulparams/avrxmega1.sh	2008-02-14 09:08:29.531250000 -0700
@@ -0,0 +1,12 @@
+ARCH=avr:101
+MACHINE=
+SCRIPT_NAME=avr
+OUTPUT_FORMAT="elf32-avr"
+MAXPAGESIZE=1
+EMBEDDED=yes
+TEMPLATE_NAME=elf32
+
+TEXT_LENGTH=1024K
+DATA_ORIGIN=0x802000
+DATA_LENGTH=0xffa0
+EXTRA_EM_FILE=avrelf
--- /dev/null	2008-02-14 11:03:18.394502600 -0700
+++ ld/emulparams/avrxmega2.sh	2008-02-14 09:08:29.546875000 -0700
@@ -0,0 +1,12 @@
+ARCH=avr:102
+MACHINE=
+SCRIPT_NAME=avr
+OUTPUT_FORMAT="elf32-avr"
+MAXPAGESIZE=1
+EMBEDDED=yes
+TEMPLATE_NAME=elf32
+
+TEXT_LENGTH=1024K
+DATA_ORIGIN=0x802000
+DATA_LENGTH=0xffa0
+EXTRA_EM_FILE=avrelf
--- /dev/null	2008-02-14 11:03:22.050425000 -0700
+++ ld/emulparams/avrxmega3.sh	2008-02-14 09:08:29.546875000 -0700
@@ -0,0 +1,12 @@
+ARCH=avr:103
+MACHINE=
+SCRIPT_NAME=avr
+OUTPUT_FORMAT="elf32-avr"
+MAXPAGESIZE=1
+EMBEDDED=yes
+TEMPLATE_NAME=elf32
+
+TEXT_LENGTH=1024K
+DATA_ORIGIN=0x802000
+DATA_LENGTH=0xffa0
+EXTRA_EM_FILE=avrelf
--- /dev/null	2008-02-14 11:03:25.784465400 -0700
+++ ld/emulparams/avrxmega4.sh	2008-02-14 09:08:29.546875000 -0700
@@ -0,0 +1,12 @@
+ARCH=avr:104
+MACHINE=
+SCRIPT_NAME=avr
+OUTPUT_FORMAT="elf32-avr"
+MAXPAGESIZE=1
+EMBEDDED=yes
+TEMPLATE_NAME=elf32
+
+TEXT_LENGTH=1024K
+DATA_ORIGIN=0x802000
+DATA_LENGTH=0xffa0
+EXTRA_EM_FILE=avrelf
--- /dev/null	2008-02-14 11:03:25.784465400 -0700
+++ ld/emulparams/avrxmega5.sh	2008-02-14 09:08:29.546875000 -0700
@@ -0,0 +1,12 @@
+ARCH=avr:105
+MACHINE=
+SCRIPT_NAME=avr
+OUTPUT_FORMAT="elf32-avr"
+MAXPAGESIZE=1
+EMBEDDED=yes
+TEMPLATE_NAME=elf32
+
+TEXT_LENGTH=1024K
+DATA_ORIGIN=0x802000
+DATA_LENGTH=0xffa0
+EXTRA_EM_FILE=avrelf
--- /dev/null	2008-02-14 11:03:25.784465400 -0700
+++ ld/emulparams/avrxmega6.sh	2008-02-14 09:08:29.546875000 -0700
@@ -0,0 +1,12 @@
+ARCH=avr:106
+MACHINE=
+SCRIPT_NAME=avr
+OUTPUT_FORMAT="elf32-avr"
+MAXPAGESIZE=1
+EMBEDDED=yes
+TEMPLATE_NAME=elf32
+
+TEXT_LENGTH=1024K
+DATA_ORIGIN=0x802000
+DATA_LENGTH=0xffa0
+EXTRA_EM_FILE=avrelf
--- /dev/null	2008-02-14 11:03:25.784465400 -0700
+++ ld/emulparams/avrxmega7.sh	2008-02-14 09:08:29.546875000 -0700
@@ -0,0 +1,12 @@
+ARCH=avr:107
+MACHINE=
+SCRIPT_NAME=avr
+OUTPUT_FORMAT="elf32-avr"
+MAXPAGESIZE=1
+EMBEDDED=yes
+TEMPLATE_NAME=elf32
+
+TEXT_LENGTH=1024K
+DATA_ORIGIN=0x802000
+DATA_LENGTH=0xffa0
+EXTRA_EM_FILE=avrelf
--- bfd/elf32-avr.c.old	2008-10-14 11:27:16.515625000 -0600
+++ bfd/elf32-avr.c	2008-10-14 11:46:35.453125000 -0600
@@ -1324,6 +1324,34 @@ bfd_elf_avr_final_write_processing (bfd 
     case bfd_mach_avr6:
       val = E_AVR_MACH_AVR6;
       break;
+
+    case bfd_mach_avrxmega1:
+      val = E_AVR_MACH_XMEGA1;
+      break;
+
+    case bfd_mach_avrxmega2:
+      val = E_AVR_MACH_XMEGA2;
+      break;
+
+    case bfd_mach_avrxmega3:
+      val = E_AVR_MACH_XMEGA3;
+      break;
+
+    case bfd_mach_avrxmega4:
+      val = E_AVR_MACH_XMEGA4;
+      break;
+
+    case bfd_mach_avrxmega5:
+      val = E_AVR_MACH_XMEGA5;
+      break;
+
+    case bfd_mach_avrxmega6:
+      val = E_AVR_MACH_XMEGA6;
+      break;
+
+    case bfd_mach_avrxmega7:
+      val = E_AVR_MACH_XMEGA7;
+      break;
     }
 
   elf_elfheader (abfd)->e_machine = EM_AVR;
@@ -1386,6 +1414,34 @@ elf32_avr_object_p (bfd *abfd)
 	case E_AVR_MACH_AVR6:
 	  e_set = bfd_mach_avr6;
 	  break;
+
+	case E_AVR_MACH_XMEGA1:
+	  e_set = bfd_mach_avrxmega1;
+	  break;
+
+	case E_AVR_MACH_XMEGA2:
+	  e_set = bfd_mach_avrxmega2;
+	  break;
+
+	case E_AVR_MACH_XMEGA3:
+	  e_set = bfd_mach_avrxmega3;
+	  break;
+
+	case E_AVR_MACH_XMEGA4:
+	  e_set = bfd_mach_avrxmega4;
+	  break;
+
+	case E_AVR_MACH_XMEGA5:
+	  e_set = bfd_mach_avrxmega5;
+	  break;
+
+	case E_AVR_MACH_XMEGA6:
+	  e_set = bfd_mach_avrxmega6;
+	  break;
+
+	case E_AVR_MACH_XMEGA7:
+	  e_set = bfd_mach_avrxmega7;
+	  break;
 	}
     }
   return bfd_default_set_arch_mach (abfd, bfd_arch_avr,
