Arduino Reference - EthernetLocalIP

Arduino

Reference Language | Libraries | Comparison | Changes

Ethernet

## Ethernet.localIP()

#### Description

Obtains the IP address of the Ethernet shield. Useful when the address is auto assigned through DHCP.

#### Syntax

Ethernet.localIP();

#### Parameters

none

#### Returns

the IP address

#### Example

#include <SPI.h>
#include <Ethernet.h>
// Enter a MAC address for your controller below.
// Newer Ethernet shields have a MAC address printed on a sticker on the shield
byte mac[] = {
0x00, 0xAA, 0xBB, 0xCC, 0xDE, 0x02 };
// Initialize the Ethernet client library
// with the IP address and port of the server
// that you want to connect to (port 80 is default for HTTP):
EthernetClient client;
void setup() {
// start the serial library:
Serial.begin(9600);
// start the Ethernet connection:
if (Ethernet.begin(mac) == 0) {
Serial.println("Failed to configure Ethernet using DHCP");
// no point in carrying on, so do nothing forevermore:
for(;;)
;
}
// print your local IP address:
Serial.println(Ethernet.localIP());
}
void loop() {
}
[Get Code]
Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes