Arduino Reference - Available

Arduino

Serial

## available()

#### Description

Get the number of bytes (characters) available for reading from the serial port. This is data that's already arrived and stored in the serial receive buffer (which holds 64 bytes). available() inherits from the Stream utility class.

#### Syntax

Serial.available()

Arduino Mega only:
Serial1.available()
Serial2.available()
Serial3.available()

### Parameters

none

#### Returns

the number of bytes available to read

### Example

int incomingByte = 0; // for incoming serial data
void setup() {
Serial.begin(9600); // opens serial port, sets data rate to 9600 bps
}
void loop() {
// send data only when you receive data:
if (Serial.available() > 0) {
// read the incoming byte:
incomingByte = Serial.read();
// say what you got:
Serial.print("I received: ");
Serial.println(incomingByte, DEC);
}
}
[Get Code]

Arduino Mega example:

void setup() {
Serial.begin(9600);
Serial1.begin(9600);
}
void loop() {
// read from port 0, send to port 1:
if (Serial.available()) {
int inByte = Serial.read();
Serial1.print(inByte, BYTE);
}
// read from port 1, send to port 0:
if (Serial1.available()) {
int inByte = Serial1.read();
Serial.print(inByte, BYTE);
}
}
[Get Code]

#### See also

- begin()
- end()
- available()
- read()
- peek()
- parseInt()
- flush()
- print()
- println()
- write()
- SerialEvent()
- Stream.available()

Reference Home

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes