Static Call Graph - [UART1_746 Configuration\UART1_746 Configuration.axf]

# Static Call Graph for image UART1_746 Configuration\UART1_746 Configuration.axf

#<CALLGRAPH># ARM Linker, 5050169: Last Updated: Tue Nov 20 10:40:52 2018

### Maximum Stack Usage = 308 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ Touch_Draw ⇒ GT911_TEST ⇒ GT911_Scan ⇒ BSP_LCD_FillCircle ⇒ BSP_LCD_DrawHLine ⇒ LL_FillBuffer ⇒ HAL_DMA2D_Start ⇒ DMA2D_SetConfig

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - BusFault_Handler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - CEC_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA2D_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - DebugMon_Handler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - ETH_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - EXTI9_5_IRQHandler from stm32f7xx_it.o(i.EXTI9_5_IRQHandler) referenced from startup_stm32f746xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - FMC_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - FPU_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - HardFault_Handler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - I2C4_ER_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - I2C4_EV_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - LPTIM1_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - LTDC_ER_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - LTDC_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - MemManage_Handler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - NMI_Handler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - PendSV_Handler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - QUADSPI_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - RNG_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - Reset_Handler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - SAI1_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - SAI2_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - SDMMC1_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - SPDIF_RX_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - SPI4_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - SPI5_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - SPI6_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - SVC_Handler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - SysTick_Handler from stm32f7xx_it.o(i.SysTick_Handler) referenced from startup_stm32f746xx.o(RESET)
  - SystemInit from system_stm32f7xx.o(i.SystemInit) referenced from startup_stm32f746xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - UART4_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - UART5_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - UART7_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - UART8_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - USART1_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - USART3_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - USART6_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - UsageFault_Handler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f746xx.o(.text) referenced from startup_stm32f746xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f746xx.o(.text)
  - fputc from main.o(i.fputc) referenced from printf8.o(i.__0printf$8)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f746xx.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f746xx.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f746xx.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f746xx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f746xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f746xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f746xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f746xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f746xx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  CEC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA2D_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  FMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  I2C4_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  I2C4_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  LPTIM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  LTDC_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  LTDC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  QUADSPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  SAI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  SAI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  SDMMC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  SPDIF_RX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  SPI6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  UART7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  UART8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f746xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f746xx.o(RESET)

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> HAL_LTDC_ConfigLayer
  - >> GT911_Scan

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  BSP_LCD_Clear (Thumb, 48 bytes, Stack size 16 bytes, stm32746g_lcd.o(i.BSP_LCD_Clear))
  [Stack]

  - Max Depth = 92
  - Call Chain = BSP_LCD_Clear ⇒ LL_FillBuffer ⇒ HAL_DMA2D_Start ⇒ DMA2D_SetConfig
  [Calls]
  - >> BSP_LCD_GetYSize
  - >> BSP_LCD_GetXSize
  - >> LL_FillBuffer
  [Called By]
  - >> Touch_Draw

  BSP_LCD_DisplayChar (Thumb, 44 bytes, Stack size 8 bytes, stm32746g_lcd.o(i.BSP_LCD_DisplayChar))
  [Stack]

  - Max Depth = 72
  - Call Chain = BSP_LCD_DisplayChar ⇒ DrawChar ⇒ BSP_LCD_DrawPixel
  [Calls]
  - >> DrawChar
  [Called By]
  - >> BSP_LCD_DisplayStringAt

  BSP_LCD_DisplayStringAt (Thumb, 192 bytes, Stack size 32 bytes, stm32746g_lcd.o(i.BSP_LCD_DisplayStringAt))
  [Stack]

  - Max Depth = 104
  - Call Chain = BSP_LCD_DisplayStringAt ⇒ BSP_LCD_DisplayChar ⇒ DrawChar ⇒ BSP_LCD_DrawPixel
  [Calls]
  - >> BSP_LCD_GetXSize
  - >> BSP_LCD_DisplayChar
  [Called By]
  - >> Touch_Draw

  BSP_LCD_DrawCircle (Thumb, 270 bytes, Stack size 52 bytes, stm32746g_lcd.o(i.BSP_LCD_DrawCircle))
  [Stack]

  - Max Depth = 68
  - Call Chain = BSP_LCD_DrawCircle ⇒ BSP_LCD_DrawPixel
  [Calls]
  - >> BSP_LCD_DrawPixel
  [Called By]
  - >> BSP_LCD_FillCircle

  BSP_LCD_DrawHLine (Thumb, 114 bytes, Stack size 24 bytes, stm32746g_lcd.o(i.BSP_LCD_DrawHLine))
  [Stack]

  - Max Depth = 100
  - Call Chain = BSP_LCD_DrawHLine ⇒ LL_FillBuffer ⇒ HAL_DMA2D_Start ⇒ DMA2D_SetConfig
  [Calls]
  - >> BSP_LCD_GetXSize
  - >> LL_FillBuffer
  [Called By]
  - >> GT911_Scan
  - >> BSP_LCD_FillCircle

  BSP_LCD_DrawPixel (Thumb, 90 bytes, Stack size 16 bytes, stm32746g_lcd.o(i.BSP_LCD_DrawPixel))
  [Stack]

  - Max Depth = 16
  - Call Chain = BSP_LCD_DrawPixel
  [Calls]
  - >> BSP_LCD_GetXSize
  [Called By]
  - >> BSP_LCD_DrawCircle
  - >> DrawChar

  BSP_LCD_DrawVLine (Thumb, 126 bytes, Stack size 24 bytes, stm32746g_lcd.o(i.BSP_LCD_DrawVLine))
  [Stack]

  - Max Depth = 100
  - Call Chain = BSP_LCD_DrawVLine ⇒ LL_FillBuffer ⇒ HAL_DMA2D_Start ⇒ DMA2D_SetConfig
  [Calls]
  - >> BSP_LCD_GetXSize
  - >> LL_FillBuffer
  [Called By]
  - >> GT911_Scan

  BSP_LCD_FillCircle (Thumb, 186 bytes, Stack size 56 bytes, stm32746g_lcd.o(i.BSP_LCD_FillCircle))
  [Stack]

  - Max Depth = 156
  - Call Chain = BSP_LCD_FillCircle ⇒ BSP_LCD_DrawHLine ⇒ LL_FillBuffer ⇒ HAL_DMA2D_Start ⇒ DMA2D_SetConfig
  [Calls]
  - >> BSP_LCD_SetTextColor
  - >> BSP_LCD_DrawHLine
  - >> BSP_LCD_DrawCircle
  [Called By]
  - >> GT911_Scan

  BSP_LCD_GetXSize (Thumb, 22 bytes, Stack size 0 bytes, stm32746g_lcd.o(i.BSP_LCD_GetXSize))
  [Called By]

  - >> BSP_LCD_DrawVLine
  - >> BSP_LCD_DrawPixel
  - >> BSP_LCD_DrawHLine
  - >> BSP_LCD_DisplayStringAt
  - >> BSP_LCD_Clear

  BSP_LCD_GetYSize (Thumb, 22 bytes, Stack size 0 bytes, stm32746g_lcd.o(i.BSP_LCD_GetYSize))
  [Called By]

  - >> BSP_LCD_Clear

  BSP_LCD_Init (Thumb, 16 bytes, Stack size 8 bytes, stm32746g_lcd.o(i.BSP_LCD_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = BSP_LCD_Init ⇒ BSP_SDRAM_Init ⇒ BSP_SDRAM_Initialization_sequence ⇒ HAL_SDRAM_SendCommand ⇒ FMC_SDRAM_SendCommand
  [Calls]
  - >> BSP_SDRAM_Init
  - >> BSP_LCD_SetFont
  [Called By]
  - >> main

  BSP_LCD_SelectLayer (Thumb, 6 bytes, Stack size 0 bytes, stm32746g_lcd.o(i.BSP_LCD_SelectLayer))
  [Called By]

  - >> Touch_Draw

  BSP_LCD_SetBackColor (Thumb, 18 bytes, Stack size 0 bytes, stm32746g_lcd.o(i.BSP_LCD_SetBackColor))
  [Called By]

  - >> Touch_Draw

  BSP_LCD_SetFont (Thumb, 18 bytes, Stack size 0 bytes, stm32746g_lcd.o(i.BSP_LCD_SetFont))
  [Called By]

  - >> BSP_LCD_Init

  BSP_LCD_SetLayerVisible (Thumb, 40 bytes, Stack size 0 bytes, stm32746g_lcd.o(i.BSP_LCD_SetLayerVisible))
  [Called By]

  - >> Touch_Draw

  BSP_LCD_SetTextColor (Thumb, 16 bytes, Stack size 0 bytes, stm32746g_lcd.o(i.BSP_LCD_SetTextColor))
  [Called By]

  - >> GT911_Scan
  - >> BSP_LCD_FillCircle

  BSP_SDRAM_Init (Thumb, 22 bytes, Stack size 8 bytes, stm32746g_sdram.o(i.BSP_SDRAM_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = BSP_SDRAM_Init ⇒ BSP_SDRAM_Initialization_sequence ⇒ HAL_SDRAM_SendCommand ⇒ FMC_SDRAM_SendCommand
  [Calls]
  - >> BSP_SDRAM_Initialization_sequence
  [Called By]
  - >> BSP_LCD_Init

  BSP_SDRAM_Initialization_sequence (Thumb, 130 bytes, Stack size 32 bytes, stm32746g_sdram.o(i.BSP_SDRAM_Initialization_sequence))
  [Stack]

  - Max Depth = 72
  - Call Chain = BSP_SDRAM_Initialization_sequence ⇒ HAL_SDRAM_SendCommand ⇒ FMC_SDRAM_SendCommand
  [Calls]
  - >> HAL_Delay
  - >> HAL_SDRAM_SendCommand
  - >> HAL_SDRAM_ProgramRefreshRate
  [Called By]
  - >> BSP_SDRAM_Init

  CT_I2C_Ack (Thumb, 74 bytes, Stack size 16 bytes, ct_i2c.o(i.CT_I2C_Ack))
  [Stack]

  - Max Depth = 80
  - Call Chain = CT_I2C_Ack ⇒ CT_SDA_OUT ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> delay_us
  - >> CT_SDA_OUT
  [Called By]
  - >> CT_I2C_Read_Byte

  CT_I2C_Init (Thumb, 82 bytes, Stack size 40 bytes, ct_i2c.o(i.CT_I2C_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = CT_I2C_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> GT911_TEST

  CT_I2C_NAck (Thumb, 62 bytes, Stack size 16 bytes, ct_i2c.o(i.CT_I2C_NAck))
  [Stack]

  - Max Depth = 80
  - Call Chain = CT_I2C_NAck ⇒ CT_SDA_OUT ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> delay_us
  - >> CT_SDA_OUT
  [Called By]
  - >> CT_I2C_Read_Byte

  CT_I2C_Read_Byte (Thumb, 114 bytes, Stack size 32 bytes, ct_i2c.o(i.CT_I2C_Read_Byte))
  [Stack]

  - Max Depth = 112
  - Call Chain = CT_I2C_Read_Byte ⇒ CT_I2C_NAck ⇒ CT_SDA_OUT ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_ReadPin
  - >> CT_I2C_NAck
  - >> CT_I2C_Ack
  - >> delay_us
  - >> CT_SDA_IN
  [Called By]
  - >> GT911_RD_Reg

  CT_I2C_Send_Byte (Thumb, 136 bytes, Stack size 24 bytes, ct_i2c.o(i.CT_I2C_Send_Byte))
  [Stack]

  - Max Depth = 88
  - Call Chain = CT_I2C_Send_Byte ⇒ CT_SDA_OUT ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> delay_us
  - >> CT_SDA_OUT
  [Called By]
  - >> GT911_WR_Reg
  - >> GT911_RD_Reg

  CT_I2C_Start (Thumb, 80 bytes, Stack size 16 bytes, ct_i2c.o(i.CT_I2C_Start))
  [Stack]

  - Max Depth = 80
  - Call Chain = CT_I2C_Start ⇒ CT_SDA_OUT ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> delay_us
  - >> CT_SDA_OUT
  [Called By]
  - >> GT911_WR_Reg
  - >> GT911_RD_Reg

  CT_I2C_Stop (Thumb, 64 bytes, Stack size 16 bytes, ct_i2c.o(i.CT_I2C_Stop))
  [Stack]

  - Max Depth = 80
  - Call Chain = CT_I2C_Stop ⇒ CT_SDA_OUT ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> delay_us
  - >> CT_SDA_OUT
  [Called By]
  - >> GT911_WR_Reg
  - >> GT911_RD_Reg
  - >> CT_I2C_Wait_Ack

  CT_I2C_Wait_Ack (Thumb, 94 bytes, Stack size 24 bytes, ct_i2c.o(i.CT_I2C_Wait_Ack))
  [Stack]

  - Max Depth = 104
  - Call Chain = CT_I2C_Wait_Ack ⇒ CT_I2C_Stop ⇒ CT_SDA_OUT ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_ReadPin
  - >> CT_I2C_Stop
  - >> delay_us
  - >> CT_SDA_IN
  [Called By]
  - >> GT911_WR_Reg
  - >> GT911_RD_Reg

  EXTI9_5_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f7xx_it.o(i.EXTI9_5_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = EXTI9_5_IRQHandler ⇒ HAL_GPIO_EXTI_IRQHandler
  [Calls]
  - >> HAL_GPIO_EXTI_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f746xx.o(RESET)

  FMC_SDRAM_Init (Thumb, 94 bytes, Stack size 20 bytes, stm32f7xx_ll_fmc.o(i.FMC_SDRAM_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = FMC_SDRAM_Init
  [Called By]
  - >> HAL_SDRAM_Init

  FMC_SDRAM_ProgramRefreshRate (Thumb, 12 bytes, Stack size 0 bytes, stm32f7xx_ll_fmc.o(i.FMC_SDRAM_ProgramRefreshRate))
  [Called By]

  - >> HAL_SDRAM_ProgramRefreshRate

  FMC_SDRAM_SendCommand (Thumb, 72 bytes, Stack size 24 bytes, stm32f7xx_ll_fmc.o(i.FMC_SDRAM_SendCommand))
  [Stack]

  - Max Depth = 24
  - Call Chain = FMC_SDRAM_SendCommand
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_SDRAM_SendCommand

  FMC_SDRAM_Timing_Init (Thumb, 130 bytes, Stack size 28 bytes, stm32f7xx_ll_fmc.o(i.FMC_SDRAM_Timing_Init))
  [Stack]

  - Max Depth = 28
  - Call Chain = FMC_SDRAM_Timing_Init
  [Called By]
  - >> HAL_SDRAM_Init

  GT911_Scan (Thumb, 606 bytes, Stack size 104 bytes, gt911.o(i.GT911_Scan))
  [Stack]

  - Max Depth = 260
  - Call Chain = GT911_Scan ⇒ BSP_LCD_FillCircle ⇒ BSP_LCD_DrawHLine ⇒ LL_FillBuffer ⇒ HAL_DMA2D_Start ⇒ DMA2D_SetConfig
  [Calls]
  - >> HAL_Delay
  - >> GT911_WR_Reg
  - >> GT911_RD_Reg
  - >> BSP_LCD_SetTextColor
  - >> BSP_LCD_FillCircle
  - >> BSP_LCD_DrawVLine
  - >> BSP_LCD_DrawHLine
  - >> __aeabi_memcpy4
  [Called By]
  - >> GT911_TEST

  GT911_TEST (Thumb, 102 bytes, Stack size 16 bytes, gt911.o(i.GT911_TEST))
  [Stack]

  - Max Depth = 276
  - Call Chain = GT911_TEST ⇒ GT911_Scan ⇒ BSP_LCD_FillCircle ⇒ BSP_LCD_DrawHLine ⇒ LL_FillBuffer ⇒ HAL_DMA2D_Start ⇒ DMA2D_SetConfig
  [Calls]
  - >> GT911_Scan
  - >> GT911_Reset_Sequence
  - >> GT911_RD_Reg
  - >> CT_I2C_Init
  - >> __2printf
  [Called By]
  - >> Touch_Draw

  HAL_DMA2D_ConfigLayer (Thumb, 218 bytes, Stack size 20 bytes, stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_ConfigLayer))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_DMA2D_ConfigLayer
  [Called By]
  - >> LL_FillBuffer
  - >> main

  HAL_DMA2D_Init (Thumb, 90 bytes, Stack size 16 bytes, stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_DMA2D_Init ⇒ HAL_DMA2D_MspInit
  [Calls]
  - >> HAL_DMA2D_MspInit
  [Called By]
  - >> LL_FillBuffer
  - >> main

  HAL_DMA2D_MspInit (Thumb, 30 bytes, Stack size 8 bytes, stm32f7xx_hal_msp.o(i.HAL_DMA2D_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_DMA2D_MspInit
  [Called By]
  - >> HAL_DMA2D_Init

  HAL_DMA2D_PollForTransfer (Thumb, 220 bytes, Stack size 32 bytes, stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_PollForTransfer))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_DMA2D_PollForTransfer
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> LL_FillBuffer

  HAL_DMA2D_Start (Thumb, 62 bytes, Stack size 24 bytes, stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_Start))
  [Stack]

  - Max Depth = 44
  - Call Chain = HAL_DMA2D_Start ⇒ DMA2D_SetConfig
  [Calls]
  - >> DMA2D_SetConfig
  [Called By]
  - >> LL_FillBuffer

  HAL_DMA_Init (Thumb, 134 bytes, Stack size 24 bytes, stm32f7xx_hal_dma.o(i.HAL_DMA_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_DMA_Init
  [Calls]
  - >> DMA_CalcBaseAndBitshift
  [Called By]
  - >> MX_DMA_Init

  HAL_Delay (Thumb, 22 bytes, Stack size 16 bytes, stm32f7xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> GT911_Scan
  - >> GT911_Reset_Sequence
  - >> BSP_SDRAM_Initialization_sequence
  - >> Touch_Draw

  HAL_GPIO_EXTI_Callback (Thumb, 12 bytes, Stack size 0 bytes, main.o(i.HAL_GPIO_EXTI_Callback))
  [Called By]

  - >> HAL_GPIO_EXTI_IRQHandler

  HAL_GPIO_EXTI_IRQHandler (Thumb, 18 bytes, Stack size 8 bytes, stm32f7xx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_GPIO_EXTI_IRQHandler
  [Calls]
  - >> HAL_GPIO_EXTI_Callback
  [Called By]
  - >> EXTI9_5_IRQHandler

  HAL_GPIO_Init (Thumb, 418 bytes, Stack size 40 bytes, stm32f7xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> MX_GPIO_Init
  - >> GT911_Reset_Sequence
  - >> CT_I2C_Init
  - >> CT_SDA_OUT
  - >> CT_SDA_IN
  - >> HAL_UART_MspInit
  - >> HAL_LTDC_MspInit
  - >> HAL_FMC_MspInit

  HAL_GPIO_ReadPin (Thumb, 10 bytes, Stack size 0 bytes, stm32f7xx_hal_gpio.o(i.HAL_GPIO_ReadPin))
  [Called By]

  - >> CT_I2C_Wait_Ack
  - >> CT_I2C_Read_Byte

  HAL_GPIO_WritePin (Thumb, 10 bytes, Stack size 0 bytes, stm32f7xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> GT911_Reset_Sequence
  - >> CT_I2C_Wait_Ack
  - >> CT_I2C_Stop
  - >> CT_I2C_Start
  - >> CT_I2C_Send_Byte
  - >> CT_I2C_Read_Byte
  - >> CT_I2C_NAck
  - >> CT_I2C_Ack
  - >> main

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f7xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_PWREx_EnableOverDrive
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> UART_WaitOnFlagUntilTimeout
  - >> HAL_DMA2D_PollForTransfer
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_Delay
  - >> FMC_SDRAM_SendCommand

  HAL_IncTick (Thumb, 10 bytes, Stack size 0 bytes, stm32f7xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 22 bytes, Stack size 8 bytes, stm32f7xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_InitTick
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_MspInit
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 34 bytes, Stack size 8 bytes, stm32f7xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_LTDC_ConfigLayer (Thumb, 82 bytes, Stack size 24 bytes, stm32f7xx_hal_ltdc.o(i.HAL_LTDC_ConfigLayer))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_LTDC_ConfigLayer ⇒ LTDC_SetConfig
  [Calls]
  - >> LTDC_SetConfig
  - >> __aeabi_memcpy4
  [Called By]
  - >> MX_LTDC_Init

  HAL_LTDC_Init (Thumb, 252 bytes, Stack size 24 bytes, stm32f7xx_hal_ltdc.o(i.HAL_LTDC_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = HAL_LTDC_Init ⇒ HAL_LTDC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_LTDC_MspInit
  [Called By]
  - >> MX_LTDC_Init

  HAL_LTDC_MspInit (Thumb, 230 bytes, Stack size 48 bytes, stm32f7xx_hal_msp.o(i.HAL_LTDC_MspInit))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_LTDC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_LTDC_Init

  HAL_MspInit (Thumb, 22 bytes, Stack size 8 bytes, stm32f7xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 22 bytes, Stack size 0 bytes, stm32f7xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> MX_GPIO_Init

  HAL_NVIC_SetPriority (Thumb, 60 bytes, Stack size 16 bytes, stm32f7xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> MX_GPIO_Init
  - >> HAL_MspInit
  - >> SystemClock_Config

  HAL_NVIC_SetPriorityGrouping (Thumb, 28 bytes, Stack size 8 bytes, stm32f7xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_NVIC_SetPriorityGrouping
  [Called By]
  - >> HAL_Init
  - >> HAL_MspInit

  HAL_PWREx_EnableOverDrive (Thumb, 100 bytes, Stack size 24 bytes, stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_EnableOverDrive))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_PWREx_EnableOverDrive
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCCEx_PeriphCLKConfig (Thumb, 1708 bytes, Stack size 40 bytes, stm32f7xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCCEx_PeriphCLKConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_ClockConfig (Thumb, 450 bytes, Stack size 32 bytes, stm32f7xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_InitTick
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 38 bytes, Stack size 4 bytes, stm32f7xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_InitTick
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  - >> SystemClock_Config

  HAL_RCC_GetPCLK1Freq (Thumb, 36 bytes, Stack size 4 bytes, stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_RCC_GetPCLK1Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 36 bytes, Stack size 4 bytes, stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 120 bytes, Stack size 12 bytes, stm32f7xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_GetHCLKFreq
  - >> UART_SetConfig

  HAL_RCC_OscConfig (Thumb, 914 bytes, Stack size 40 bytes, stm32f7xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SDRAM_Init (Thumb, 66 bytes, Stack size 16 bytes, stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Init))
  [Stack]

  - Max Depth = 104
  - Call Chain = HAL_SDRAM_Init ⇒ HAL_SDRAM_MspInit ⇒ HAL_FMC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> FMC_SDRAM_Timing_Init
  - >> FMC_SDRAM_Init
  - >> HAL_SDRAM_MspInit
  [Called By]
  - >> MX_FMC_Init

  HAL_SDRAM_MspInit (Thumb, 4 bytes, Stack size 0 bytes, stm32f7xx_hal_msp.o(i.HAL_SDRAM_MspInit))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_SDRAM_MspInit ⇒ HAL_FMC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_FMC_MspInit
  [Called By]
  - >> HAL_SDRAM_Init

  HAL_SDRAM_ProgramRefreshRate (Thumb, 34 bytes, Stack size 8 bytes, stm32f7xx_hal_sdram.o(i.HAL_SDRAM_ProgramRefreshRate))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SDRAM_ProgramRefreshRate
  [Calls]
  - >> FMC_SDRAM_ProgramRefreshRate
  [Called By]
  - >> BSP_SDRAM_Initialization_sequence

  HAL_SDRAM_SendCommand (Thumb, 48 bytes, Stack size 16 bytes, stm32f7xx_hal_sdram.o(i.HAL_SDRAM_SendCommand))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_SDRAM_SendCommand ⇒ FMC_SDRAM_SendCommand
  [Calls]
  - >> FMC_SDRAM_SendCommand
  [Called By]
  - >> BSP_SDRAM_Initialization_sequence

  HAL_SYSTICK_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f7xx_hal_cortex.o(i.HAL_SYSTICK_CLKSourceConfig))
  [Called By]

  - >> SystemClock_Config

  HAL_SYSTICK_Callback (Thumb, 2 bytes, Stack size 0 bytes, stm32f7xx_hal_cortex.o(i.HAL_SYSTICK_Callback))
  [Called By]

  - >> HAL_SYSTICK_IRQHandler

  HAL_SYSTICK_Config (Thumb, 38 bytes, Stack size 8 bytes, stm32f7xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_Config
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> SystemClock_Config

  HAL_SYSTICK_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, stm32f7xx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_Callback
  [Called By]
  - >> SysTick_Handler

  HAL_UART_Init (Thumb, 106 bytes, Stack size 8 bytes, stm32f7xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> UART_SetConfig
  - >> UART_CheckIdleState
  - >> UART_AdvFeatureConfig
  - >> HAL_UART_MspInit
  [Called By]
  - >> MX_USART1_UART_Init

  HAL_UART_MspInit (Thumb, 58 bytes, Stack size 32 bytes, stm32f7xx_hal_msp.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_Init

  HAL_UART_Transmit (Thumb, 200 bytes, Stack size 32 bytes, stm32f7xx_hal_uart.o(i.HAL_UART_Transmit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> fputc

  SysTick_Handler (Thumb, 14 bytes, Stack size 8 bytes, stm32f7xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_IRQHandler
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f746xx.o(RESET)

  SystemClock_Config (Thumb, 168 bytes, Stack size 224 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 280
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_PWREx_EnableOverDrive
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_RCC_ClockConfig
  - >> HAL_SYSTICK_CLKSourceConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> main

  SystemInit (Thumb, 68 bytes, Stack size 12 bytes, system_stm32f7xx.o(i.SystemInit))
  [Stack]

  - Max Depth = 12
  - Call Chain = SystemInit
  [Address Reference Count : 1]
  - startup_stm32f746xx.o(.text)

  Touch_Draw (Thumb, 80 bytes, Stack size 8 bytes, main.o(i.Touch_Draw))
  [Stack]

  - Max Depth = 284
  - Call Chain = Touch_Draw ⇒ GT911_TEST ⇒ GT911_Scan ⇒ BSP_LCD_FillCircle ⇒ BSP_LCD_DrawHLine ⇒ LL_FillBuffer ⇒ HAL_DMA2D_Start ⇒ DMA2D_SetConfig
  [Calls]
  - >> HAL_Delay
  - >> GT911_TEST
  - >> BSP_LCD_SetLayerVisible
  - >> BSP_LCD_SetBackColor
  - >> BSP_LCD_SelectLayer
  - >> BSP_LCD_DisplayStringAt
  - >> BSP_LCD_Clear
  [Called By]
  - >> main

  UART_AdvFeatureConfig (Thumb, 200 bytes, Stack size 0 bytes, stm32f7xx_hal_uart.o(i.UART_AdvFeatureConfig))
  [Called By]

  - >> HAL_UART_Init

  UART_CheckIdleState (Thumb, 78 bytes, Stack size 16 bytes, stm32f7xx_hal_uart.o(i.UART_CheckIdleState))
  [Stack]

  - Max Depth = 48
  - Call Chain = UART_CheckIdleState ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> HAL_UART_Init

  UART_SetConfig (Thumb, 534 bytes, Stack size 32 bytes, stm32f7xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 52
  - Call Chain = UART_SetConfig ⇒ HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  [Called By]
  - >> HAL_UART_Init

  UART_WaitOnFlagUntilTimeout (Thumb, 146 bytes, Stack size 32 bytes, stm32f7xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 32
  - Call Chain = UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> UART_CheckIdleState
  - >> HAL_UART_Transmit

  __0printf$8 (Thumb, 22 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$8 (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> GT911_TEST

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  fputc (Thumb, 20 bytes, Stack size 16 bytes, main.o(i.fputc))
  [Stack]

  - Max Depth = 80
  - Call Chain = fputc ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  [Address Reference Count : 1]
  - printf8.o(i.__0printf$8)

  main (Thumb, 194 bytes, Stack size 24 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 308
  - Call Chain = main ⇒ Touch_Draw ⇒ GT911_TEST ⇒ GT911_Scan ⇒ BSP_LCD_FillCircle ⇒ BSP_LCD_DrawHLine ⇒ LL_FillBuffer ⇒ HAL_DMA2D_Start ⇒ DMA2D_SetConfig
  [Calls]
  - >> HAL_DMA2D_Init
  - >> HAL_DMA2D_ConfigLayer
  - >> HAL_Init
  - >> HAL_GPIO_WritePin
  - >> MX_USART1_UART_Init
  - >> MX_LTDC_Init
  - >> MX_GPIO_Init
  - >> MX_FMC_Init
  - >> MX_DMA_Init
  - >> BSP_LCD_Init
  - >> Touch_Draw
  - >> SystemClock_Config
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  DMA_CalcBaseAndBitshift (Thumb, 34 bytes, Stack size 0 bytes, stm32f7xx_hal_dma.o(i.DMA_CalcBaseAndBitshift))
  [Called By]

  - >> HAL_DMA_Init

  NVIC_SetPriority (Thumb, 34 bytes, Stack size 0 bytes, stm32f7xx_hal_cortex.o(i.NVIC_SetPriority))
  [Called By]

  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority

  DMA2D_SetConfig (Thumb, 140 bytes, Stack size 20 bytes, stm32f7xx_hal_dma2d.o(i.DMA2D_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = DMA2D_SetConfig
  [Called By]
  - >> HAL_DMA2D_Start

  LTDC_SetConfig (Thumb, 464 bytes, Stack size 48 bytes, stm32f7xx_hal_ltdc.o(i.LTDC_SetConfig))
  [Stack]

  - Max Depth = 48
  - Call Chain = LTDC_SetConfig
  [Called By]
  - >> HAL_LTDC_ConfigLayer

  MX_DMA_Init (Thumb, 80 bytes, Stack size 24 bytes, main.o(i.MX_DMA_Init))
  [Stack]

  - Max Depth = 48
  - Call Chain = MX_DMA_Init ⇒ HAL_DMA_Init
  [Calls]
  - >> HAL_DMA_Init
  [Called By]
  - >> main

  MX_FMC_Init (Thumb, 80 bytes, Stack size 48 bytes, main.o(i.MX_FMC_Init))
  [Stack]

  - Max Depth = 152
  - Call Chain = MX_FMC_Init ⇒ HAL_SDRAM_Init ⇒ HAL_SDRAM_MspInit ⇒ HAL_FMC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SDRAM_Init
  [Called By]
  - >> main

  MX_GPIO_Init (Thumb, 224 bytes, Stack size 40 bytes, main.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = MX_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> main

  MX_LTDC_Init (Thumb, 198 bytes, Stack size 136 bytes, main.o(i.MX_LTDC_Init))
  [Stack]

  - Max Depth = 248
  - Call Chain = MX_LTDC_Init ⇒ HAL_LTDC_Init ⇒ HAL_LTDC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_LTDC_Init
  - >> HAL_LTDC_ConfigLayer
  [Called By]
  - >> main

  MX_USART1_UART_Init (Thumb, 40 bytes, Stack size 8 bytes, main.o(i.MX_USART1_UART_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = MX_USART1_UART_Init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_Init
  [Called By]
  - >> main

  HAL_FMC_MspInit (Thumb, 154 bytes, Stack size 48 bytes, stm32f7xx_hal_msp.o(i.HAL_FMC_MspInit))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_FMC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_SDRAM_MspInit

  DrawChar (Thumb, 168 bytes, Stack size 48 bytes, stm32746g_lcd.o(i.DrawChar))
  [Stack]

  - Max Depth = 64
  - Call Chain = DrawChar ⇒ BSP_LCD_DrawPixel
  [Calls]
  - >> BSP_LCD_DrawPixel
  [Called By]
  - >> BSP_LCD_DisplayChar

  LL_FillBuffer (Thumb, 142 bytes, Stack size 32 bytes, stm32746g_lcd.o(i.LL_FillBuffer))
  [Stack]

  - Max Depth = 76
  - Call Chain = LL_FillBuffer ⇒ HAL_DMA2D_Start ⇒ DMA2D_SetConfig
  [Calls]
  - >> HAL_DMA2D_Start
  - >> HAL_DMA2D_PollForTransfer
  - >> HAL_DMA2D_Init
  - >> HAL_DMA2D_ConfigLayer
  [Called By]
  - >> BSP_LCD_DrawVLine
  - >> BSP_LCD_DrawHLine
  - >> BSP_LCD_Clear

  CT_SDA_IN (Thumb, 30 bytes, Stack size 24 bytes, ct_i2c.o(i.CT_SDA_IN))
  [Stack]

  - Max Depth = 64
  - Call Chain = CT_SDA_IN ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> CT_I2C_Wait_Ack
  - >> CT_I2C_Read_Byte

  CT_SDA_OUT (Thumb, 30 bytes, Stack size 24 bytes, ct_i2c.o(i.CT_SDA_OUT))
  [Stack]

  - Max Depth = 64
  - Call Chain = CT_SDA_OUT ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> CT_I2C_Stop
  - >> CT_I2C_Start
  - >> CT_I2C_Send_Byte
  - >> CT_I2C_NAck
  - >> CT_I2C_Ack

  delay_us (Thumb, 10 bytes, Stack size 0 bytes, ct_i2c.o(i.delay_us))
  [Called By]

  - >> CT_I2C_Wait_Ack
  - >> CT_I2C_Stop
  - >> CT_I2C_Start
  - >> CT_I2C_Send_Byte
  - >> CT_I2C_Read_Byte
  - >> CT_I2C_NAck
  - >> CT_I2C_Ack

  GT911_RD_Reg (Thumb, 100 bytes, Stack size 24 bytes, gt911.o(i.GT911_RD_Reg))
  [Stack]

  - Max Depth = 136
  - Call Chain = GT911_RD_Reg ⇒ CT_I2C_Read_Byte ⇒ CT_I2C_NAck ⇒ CT_SDA_OUT ⇒ HAL_GPIO_Init
  [Calls]
  - >> CT_I2C_Wait_Ack
  - >> CT_I2C_Stop
  - >> CT_I2C_Start
  - >> CT_I2C_Send_Byte
  - >> CT_I2C_Read_Byte
  [Called By]
  - >> GT911_Scan
  - >> GT911_TEST

  GT911_Reset_Sequence (Thumb, 150 bytes, Stack size 48 bytes, gt911.o(i.GT911_Reset_Sequence))
  [Stack]

  - Max Depth = 88
  - Call Chain = GT911_Reset_Sequence ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> HAL_Delay
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> GT911_TEST

  GT911_WR_Reg (Thumb, 82 bytes, Stack size 24 bytes, gt911.o(i.GT911_WR_Reg))
  [Stack]

  - Max Depth = 128
  - Call Chain = GT911_WR_Reg ⇒ CT_I2C_Wait_Ack ⇒ CT_I2C_Stop ⇒ CT_SDA_OUT ⇒ HAL_GPIO_Init
  [Calls]
  - >> CT_I2C_Wait_Ack
  - >> CT_I2C_Stop
  - >> CT_I2C_Start
  - >> CT_I2C_Send_Byte
  [Called By]
  - >> GT911_Scan

  _printf_core (Thumb, 996 bytes, Stack size 104 bytes, printf8.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  [Called By]
  - >> __0printf$8

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printf8.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printf8.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  ### Undefined Global Symbols