Static Call Graph - [LCD\LCD.axf]

# Static Call Graph for image LCD\LCD.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Wed Oct 26 16:28:02 2022

### Maximum Stack Usage = 384 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority

### Mutually Recursive functions

- ADC3_IRQHandler ⇒ ADC3_IRQHandler

  ### Function Pointers

  - ADC3_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - ADC_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - BDMA_Channel0_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - BDMA_Channel1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - BDMA_Channel2_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - BDMA_Channel3_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - BDMA_Channel4_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - BDMA_Channel5_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - BDMA_Channel6_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - BDMA_Channel7_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - BusFault_Handler from stm32h7xx_it.o(i.BusFault_Handler) referenced from startup_stm32h743xx.o(RESET)
  - CEC_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - COMP1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - CRS_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DCMI_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DFSDM1_FLT0_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DFSDM1_FLT1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DFSDM1_FLT2_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DFSDM1_FLT3_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA2D_IRQHandler from stm32h7xx_it.o(i.DMA2D_IRQHandler) referenced from startup_stm32h743xx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMAMUX1_OVR_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DMAMUX2_OVR_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - DebugMon_Handler from stm32h7xx_it.o(i.DebugMon_Handler) referenced from startup_stm32h743xx.o(RESET)
  - ETH_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - EXTI9_5_IRQHandler from stm32h7xx_it.o(i.EXTI9_5_IRQHandler) referenced from startup_stm32h743xx.o(RESET)
  - FDCAN1_IT0_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - FDCAN1_IT1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - FDCAN2_IT0_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - FDCAN2_IT1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - FDCAN_CAL_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - FMC_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - FPU_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - HRTIM1_FLT_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - HRTIM1_Master_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - HRTIM1_TIMA_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - HRTIM1_TIMB_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - HRTIM1_TIMC_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - HRTIM1_TIMD_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - HRTIM1_TIME_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - HSEM1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - HardFault_Handler from stm32h7xx_it.o(i.HardFault_Handler) referenced from startup_stm32h743xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - I2C4_ER_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - I2C4_EV_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - JPEG_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - LPTIM1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - LPTIM2_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - LPTIM3_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - LPTIM4_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - LPTIM5_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - LPUART1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - LTDC_ER_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - LTDC_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - MDIOS_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - MDIOS_WKUP_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - MDMA_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - MemManage_Handler from stm32h7xx_it.o(i.MemManage_Handler) referenced from startup_stm32h743xx.o(RESET)
  - NMI_Handler from stm32h7xx_it.o(i.NMI_Handler) referenced from startup_stm32h743xx.o(RESET)
  - OTG_FS_EP1_IN_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - OTG_FS_EP1_OUT_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - PVD_AVD_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - PendSV_Handler from stm32h7xx_it.o(i.PendSV_Handler) referenced from startup_stm32h743xx.o(RESET)
  - QUADSPI_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - RCC_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - RNG_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - Reset_Handler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - SAI1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - SAI2_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - SAI3_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - SAI4_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - SDMMC1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - SDMMC2_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - SPDIF_RX_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - SPI4_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - SPI5_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - SPI6_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - SVC_Handler from stm32h7xx_it.o(i.SVC_Handler) referenced from startup_stm32h743xx.o(RESET)
  - SWPMI1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - SysTick_Handler from stm32h7xx_it.o(i.SysTick_Handler) referenced from startup_stm32h743xx.o(RESET)
  - SystemInit from system_stm32h7xx.o(i.SystemInit) referenced from startup_stm32h743xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM15_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM16_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM17_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - UART4_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - UART5_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - UART7_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - UART8_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - USART1_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - USART2_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - USART3_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - USART6_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - UsageFault_Handler from stm32h7xx_it.o(i.UsageFault_Handler) referenced from startup_stm32h743xx.o(RESET)
  - WAKEUP_PIN_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32h743xx.o(.text) referenced from startup_stm32h743xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32h743xx.o(.text)
  - fputc from usart.o(i.fputc) referenced from printf5.o(i.__0printf$5)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Calls]

  - >> ADC3_IRQHandler
  [Called By]
  - >> ADC3_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32h743xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  BDMA_Channel0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  BDMA_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  BDMA_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  BDMA_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  BDMA_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  BDMA_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  BDMA_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  BDMA_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  CEC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  COMP1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  CRS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DFSDM1_FLT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DFSDM1_FLT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DFSDM1_FLT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DFSDM1_FLT3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMAMUX1_OVR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DMAMUX2_OVR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  FDCAN1_IT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  FDCAN1_IT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  FDCAN2_IT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  FDCAN2_IT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  FDCAN_CAL_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  FMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  HRTIM1_FLT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  HRTIM1_Master_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  HRTIM1_TIMA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  HRTIM1_TIMB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  HRTIM1_TIMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  HRTIM1_TIMD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  HRTIM1_TIME_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  HSEM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  I2C4_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  I2C4_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  JPEG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  LPTIM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  LPTIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  LPTIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  LPTIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  LPTIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  LPUART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  LTDC_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  LTDC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  MDIOS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  MDIOS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  MDMA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  OTG_FS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  OTG_FS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  PVD_AVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  QUADSPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SAI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SAI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SAI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SAI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SDMMC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SDMMC2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SPDIF_RX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SPI6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SWPMI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM16_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM17_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  UART7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  UART8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  WAKEUP_PIN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h743xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_uldivmod
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> UART_SetConfig
  - >> _printf_core

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> HAL_LTDC_ConfigLayer

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> HAL_UART_MspInit
  - >> HAL_TIM_MspPostInit
  - >> HAL_LTDC_MspInit
  - >> MX_TIM2_Init
  - >> MX_LTDC_Init
  - >> MX_GPIO_Init
  - >> SystemClock_Config

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  BSP_LCD_Clear (Thumb, 56 bytes, Stack size 24 bytes, bsp_rgb_lcd.o(i.BSP_LCD_Clear))
  [Stack]

  - Max Depth = 128
  - Call Chain = BSP_LCD_Clear ⇒ LL_FillBuffer ⇒ HAL_DMA2D_Init ⇒ HAL_DMA2D_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> BSP_LCD_GetYSize
  - >> BSP_LCD_GetXSize
  - >> LL_FillBuffer
  [Called By]
  - >> Paint_Clear

  BSP_LCD_DrawPixel (Thumb, 98 bytes, Stack size 12 bytes, bsp_rgb_lcd.o(i.BSP_LCD_DrawPixel))
  [Stack]

  - Max Depth = 12
  - Call Chain = BSP_LCD_DrawPixel
  [Calls]
  - >> BSP_LCD_GetXSize
  [Called By]
  - >> Paint_SetPixel

  BSP_LCD_GetXSize (Thumb, 22 bytes, Stack size 0 bytes, bsp_rgb_lcd.o(i.BSP_LCD_GetXSize))
  [Called By]

  - >> BSP_LCD_DrawPixel
  - >> BSP_LCD_Clear

  BSP_LCD_GetYSize (Thumb, 22 bytes, Stack size 0 bytes, bsp_rgb_lcd.o(i.BSP_LCD_GetYSize))
  [Called By]

  - >> BSP_LCD_Clear

  BSP_LCD_Init (Thumb, 30 bytes, Stack size 8 bytes, bsp_rgb_lcd.o(i.BSP_LCD_Init))
  [Stack]

  - Max Depth = 60
  - Call Chain = BSP_LCD_Init ⇒ BSP_SDRAM_Init ⇒ BSP_SDRAM_Initialization_sequence ⇒ HAL_SDRAM_SendCommand ⇒ FMC_SDRAM_SendCommand
  [Calls]
  - >> BSP_SDRAM_Init
  - >> BSP_LCD_SetLayerVisible
  - >> BSP_LCD_SelectLayer
  [Called By]
  - >> main

  BSP_LCD_SelectLayer (Thumb, 6 bytes, Stack size 0 bytes, bsp_rgb_lcd.o(i.BSP_LCD_SelectLayer))
  [Called By]

  - >> BSP_LCD_Init

  BSP_LCD_SetLayerVisible (Thumb, 74 bytes, Stack size 8 bytes, bsp_rgb_lcd.o(i.BSP_LCD_SetLayerVisible))
  [Stack]

  - Max Depth = 8
  - Call Chain = BSP_LCD_SetLayerVisible
  [Called By]
  - >> BSP_LCD_Init

  BSP_SDRAM_Init (Thumb, 18 bytes, Stack size 8 bytes, bsp_sdram.o(i.BSP_SDRAM_Init))
  [Stack]

  - Max Depth = 52
  - Call Chain = BSP_SDRAM_Init ⇒ BSP_SDRAM_Initialization_sequence ⇒ HAL_SDRAM_SendCommand ⇒ FMC_SDRAM_SendCommand
  [Calls]
  - >> BSP_SDRAM_Initialization_sequence
  [Called By]
  - >> BSP_LCD_Init

  BSP_SDRAM_Initialization_sequence (Thumb, 140 bytes, Stack size 16 bytes, bsp_sdram.o(i.BSP_SDRAM_Initialization_sequence))
  [Stack]

  - Max Depth = 44
  - Call Chain = BSP_SDRAM_Initialization_sequence ⇒ HAL_SDRAM_SendCommand ⇒ FMC_SDRAM_SendCommand
  [Calls]
  - >> HAL_Delay
  - >> HAL_SDRAM_SendCommand
  - >> HAL_SDRAM_ProgramRefreshRate
  [Called By]
  - >> BSP_SDRAM_Init

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32h7xx_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  DEV_Delay_us (Thumb, 18 bytes, Stack size 0 bytes, dev_config.o(i.DEV_Delay_us))
  [Called By]

  - >> I2C_NAck
  - >> I2C_Ack
  - >> I2C_Wait_Ack
  - >> I2C_Stop
  - >> I2C_Start
  - >> I2C_Send_Byte
  - >> I2C_Read_Byte

  DEV_Set_GPIOMode (Thumb, 64 bytes, Stack size 40 bytes, dev_config.o(i.DEV_Set_GPIOMode))
  [Stack]

  - Max Depth = 64
  - Call Chain = DEV_Set_GPIOMode ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> I2C_NAck
  - >> I2C_Ack
  - >> I2C_Wait_Ack
  - >> I2C_Stop
  - >> I2C_Start
  - >> I2C_Send_Byte
  - >> I2C_Read_Byte
  - >> GT7385_Reset

  DMA2D_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32h7xx_it.o(i.DMA2D_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA2D_IRQHandler ⇒ HAL_DMA2D_IRQHandler
  [Calls]
  - >> HAL_DMA2D_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32h743xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32h7xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32h7xx_it.o(i.EXTI9_5_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = EXTI9_5_IRQHandler ⇒ HAL_GPIO_EXTI_IRQHandler
  [Calls]
  - >> HAL_GPIO_EXTI_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32h743xx.o(RESET)

  Error_Handler (Thumb, 10 bytes, Stack size 8 bytes, main.o(i.Error_Handler))
  [Stack]

  - Max Depth = 32
  - Call Chain = Error_Handler ⇒ __2printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> MX_USART1_UART_Init
  - >> MX_TIM2_Init
  - >> MX_LTDC_Init
  - >> MX_FMC_Init
  - >> MX_DMA2D_Init
  - >> MX_CRC_Init
  - >> SystemClock_Config

  FMC_SDRAM_Init (Thumb, 116 bytes, Stack size 12 bytes, stm32h7xx_ll_fmc.o(i.FMC_SDRAM_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = FMC_SDRAM_Init
  [Called By]
  - >> HAL_SDRAM_Init

  FMC_SDRAM_ProgramRefreshRate (Thumb, 14 bytes, Stack size 0 bytes, stm32h7xx_ll_fmc.o(i.FMC_SDRAM_ProgramRefreshRate))
  [Called By]

  - >> HAL_SDRAM_ProgramRefreshRate

  FMC_SDRAM_SendCommand (Thumb, 38 bytes, Stack size 12 bytes, stm32h7xx_ll_fmc.o(i.FMC_SDRAM_SendCommand))
  [Stack]

  - Max Depth = 12
  - Call Chain = FMC_SDRAM_SendCommand
  [Called By]
  - >> HAL_SDRAM_SendCommand

  FMC_SDRAM_Timing_Init (Thumb, 152 bytes, Stack size 16 bytes, stm32h7xx_ll_fmc.o(i.FMC_SDRAM_Timing_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = FMC_SDRAM_Timing_Init
  [Called By]
  - >> HAL_SDRAM_Init

  GT7385_Init (Thumb, 26 bytes, Stack size 0 bytes, gt7385.o(i.GT7385_Init))
  [Stack]

  - Max Depth = 248
  - Call Chain = GT7385_Init ⇒ GT7385_Scan ⇒ Paint_DrawLine ⇒ Paint_DrawPoint ⇒ Paint_SetPixel ⇒ __2printf
  [Calls]
  - >> __2printf
  - >> GT7385_Scan
  - >> GT7385_Reset
  - >> GT7385_Read_ID
  - >> GT7385_Read_FirmwareVersion
  [Called By]
  - >> Touch_Draw

  GT7385_Scan (Thumb, 906 bytes, Stack size 112 bytes, gt7385.o(i.GT7385_Scan))
  [Stack]

  - Max Depth = 248
  - Call Chain = GT7385_Scan ⇒ Paint_DrawLine ⇒ Paint_DrawPoint ⇒ Paint_SetPixel ⇒ __2printf
  [Calls]
  - >> Paint_DrawLine
  - >> Paint_DrawCircle
  - >> HAL_Delay
  - >> __2printf
  - >> GT7385_WR_Reg
  - >> GT7385_RD_Reg
  [Called By]
  - >> GT7385_Init

  HAL_CRCEx_Polynomial_Set (Thumb, 100 bytes, Stack size 12 bytes, stm32h7xx_hal_crc_ex.o(i.HAL_CRCEx_Polynomial_Set))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_CRCEx_Polynomial_Set
  [Called By]
  - >> HAL_CRC_Init

  HAL_CRC_Init (Thumb, 128 bytes, Stack size 8 bytes, stm32h7xx_hal_crc.o(i.HAL_CRC_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_CRC_Init ⇒ HAL_CRCEx_Polynomial_Set
  [Calls]
  - >> HAL_CRC_MspInit
  - >> HAL_CRCEx_Polynomial_Set
  [Called By]
  - >> MX_CRC_Init

  HAL_CRC_MspInit (Thumb, 40 bytes, Stack size 8 bytes, crc.o(i.HAL_CRC_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_CRC_MspInit
  [Called By]
  - >> HAL_CRC_Init

  HAL_DMA2D_CLUTLoadingCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32h7xx_hal_dma2d.o(i.HAL_DMA2D_CLUTLoadingCpltCallback))
  [Called By]

  - >> HAL_DMA2D_IRQHandler

  HAL_DMA2D_ConfigLayer (Thumb, 296 bytes, Stack size 20 bytes, stm32h7xx_hal_dma2d.o(i.HAL_DMA2D_ConfigLayer))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_DMA2D_ConfigLayer
  [Called By]
  - >> MX_DMA2D_Init
  - >> LL_FillBuffer

  HAL_DMA2D_IRQHandler (Thumb, 358 bytes, Stack size 16 bytes, stm32h7xx_hal_dma2d.o(i.HAL_DMA2D_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_DMA2D_IRQHandler
  [Calls]
  - >> HAL_DMA2D_LineEventCallback
  - >> HAL_DMA2D_CLUTLoadingCpltCallback
  [Called By]
  - >> DMA2D_IRQHandler

  HAL_DMA2D_Init (Thumb, 156 bytes, Stack size 8 bytes, stm32h7xx_hal_dma2d.o(i.HAL_DMA2D_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_DMA2D_Init ⇒ HAL_DMA2D_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_DMA2D_MspInit
  [Called By]
  - >> MX_DMA2D_Init
  - >> LL_FillBuffer

  HAL_DMA2D_LineEventCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32h7xx_hal_dma2d.o(i.HAL_DMA2D_LineEventCallback))
  [Called By]

  - >> HAL_DMA2D_IRQHandler

  HAL_DMA2D_MspInit (Thumb, 58 bytes, Stack size 16 bytes, dma2d.o(i.HAL_DMA2D_MspInit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_DMA2D_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  [Called By]
  - >> HAL_DMA2D_Init

  HAL_DMA2D_PollForTransfer (Thumb, 360 bytes, Stack size 24 bytes, stm32h7xx_hal_dma2d.o(i.HAL_DMA2D_PollForTransfer))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_DMA2D_PollForTransfer
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> LL_FillBuffer

  HAL_DMA2D_Start (Thumb, 78 bytes, Stack size 32 bytes, stm32h7xx_hal_dma2d.o(i.HAL_DMA2D_Start))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_DMA2D_Start ⇒ DMA2D_SetConfig
  [Calls]
  - >> DMA2D_SetConfig
  [Called By]
  - >> LL_FillBuffer

  HAL_Delay (Thumb, 36 bytes, Stack size 16 bytes, stm32h7xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> main
  - >> Touch_Draw
  - >> GT7385_Scan
  - >> GT7385_Reset
  - >> GT7385_Read_ID
  - >> BSP_SDRAM_Initialization_sequence

  HAL_GPIO_EXTI_Callback (Thumb, 18 bytes, Stack size 0 bytes, main.o(i.HAL_GPIO_EXTI_Callback))
  [Called By]

  - >> HAL_GPIO_EXTI_IRQHandler

  HAL_GPIO_EXTI_IRQHandler (Thumb, 24 bytes, Stack size 8 bytes, stm32h7xx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_GPIO_EXTI_IRQHandler
  [Calls]
  - >> HAL_GPIO_EXTI_Callback
  [Called By]
  - >> EXTI9_5_IRQHandler

  HAL_GPIO_Init (Thumb, 534 bytes, Stack size 24 bytes, stm32h7xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_MspInit
  - >> HAL_TIM_MspPostInit
  - >> HAL_LTDC_MspInit
  - >> HAL_FMC_MspInit
  - >> MX_GPIO_Init
  - >> GT7385_Reset
  - >> DEV_Set_GPIOMode

  HAL_GPIO_ReadPin (Thumb, 16 bytes, Stack size 0 bytes, stm32h7xx_hal_gpio.o(i.HAL_GPIO_ReadPin))
  [Called By]

  - >> I2C_Wait_Ack
  - >> I2C_Read_Byte

  HAL_GPIO_WritePin (Thumb, 10 bytes, Stack size 0 bytes, stm32h7xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> MX_GPIO_Init
  - >> main
  - >> I2C_NAck
  - >> I2C_Ack
  - >> I2C_Wait_Ack
  - >> I2C_Stop
  - >> I2C_Start
  - >> I2C_Send_Byte
  - >> I2C_Read_Byte
  - >> GT7385_Reset

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32h7xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_UART_Transmit
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_Delay
  - >> RCCEx_PLL3_Config
  - >> RCCEx_PLL2_Config
  - >> HAL_DMA2D_PollForTransfer
  - >> UART_WaitOnFlagUntilTimeout
  - >> UART_CheckIdleState

  HAL_IncTick (Thumb, 16 bytes, Stack size 0 bytes, stm32h7xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 28 bytes, Stack size 8 bytes, stm32h7xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_InitTick
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_MspInit
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 64 bytes, Stack size 16 bytes, stm32h7xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_LTDC_ConfigLayer (Thumb, 94 bytes, Stack size 16 bytes, stm32h7xx_hal_ltdc.o(i.HAL_LTDC_ConfigLayer))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_LTDC_ConfigLayer ⇒ LTDC_SetConfig
  [Calls]
  - >> LTDC_SetConfig
  - >> __aeabi_memcpy4
  [Called By]
  - >> MX_LTDC_Init

  HAL_LTDC_Init (Thumb, 278 bytes, Stack size 16 bytes, stm32h7xx_hal_ltdc.o(i.HAL_LTDC_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_LTDC_Init ⇒ HAL_LTDC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_LTDC_MspInit
  [Called By]
  - >> MX_LTDC_Init

  HAL_LTDC_MspInit (Thumb, 566 bytes, Stack size 32 bytes, ltdc.o(i.HAL_LTDC_MspInit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_LTDC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> __aeabi_memclr4
  [Called By]
  - >> HAL_LTDC_Init

  HAL_MspInit (Thumb, 32 bytes, Stack size 8 bytes, stm32h7xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_MspInit
  [Called By]
  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 32 bytes, Stack size 0 bytes, stm32h7xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> HAL_DMA2D_MspInit
  - >> MX_GPIO_Init

  HAL_NVIC_SetPriority (Thumb, 122 bytes, Stack size 40 bytes, stm32h7xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> __NVIC_SetPriority
  - >> __NVIC_GetPriorityGrouping
  [Called By]
  - >> HAL_DMA2D_MspInit
  - >> MX_GPIO_Init
  - >> HAL_InitTick

  HAL_NVIC_SetPriorityGrouping (Thumb, 32 bytes, Stack size 0 bytes, stm32h7xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_Init

  HAL_RCCEx_GetD1SysClockFreq (Thumb, 44 bytes, Stack size 8 bytes, stm32h7xx_hal_rcc_ex.o(i.HAL_RCCEx_GetD1SysClockFreq))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_RCCEx_GetD1SysClockFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_GetHCLKFreq

  HAL_RCCEx_GetD3PCLK1Freq (Thumb, 34 bytes, Stack size 8 bytes, stm32h7xx_hal_rcc_ex.o(i.HAL_RCCEx_GetD3PCLK1Freq))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCCEx_GetD3PCLK1Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCCEx_GetD1SysClockFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCCEx_GetPLL2ClockFreq (Thumb, 532 bytes, Stack size 16 bytes, stm32h7xx_hal_rcc_ex.o(i.HAL_RCCEx_GetPLL2ClockFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_RCCEx_GetPLL2ClockFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCCEx_GetPLL3ClockFreq (Thumb, 532 bytes, Stack size 16 bytes, stm32h7xx_hal_rcc_ex.o(i.HAL_RCCEx_GetPLL3ClockFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_RCCEx_GetPLL3ClockFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCCEx_PeriphCLKConfig (Thumb, 2868 bytes, Stack size 24 bytes, stm32h7xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_RCCEx_PeriphCLKConfig ⇒ RCCEx_PLL3_Config
  [Calls]
  - >> RCCEx_PLL3_Config
  - >> RCCEx_PLL2_Config
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_ClockConfig (Thumb, 574 bytes, Stack size 16 bytes, stm32h7xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_InitTick
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 42 bytes, Stack size 8 bytes, stm32h7xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_RCC_GetHCLKFreq ⇒ HAL_RCCEx_GetD1SysClockFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCCEx_GetD1SysClockFreq
  [Called By]
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  - >> HAL_RCCEx_GetD3PCLK1Freq

  HAL_RCC_GetPCLK1Freq (Thumb, 34 bytes, Stack size 8 bytes, stm32h7xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCC_GetPCLK1Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCCEx_GetD1SysClockFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 36 bytes, Stack size 8 bytes, stm32h7xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCCEx_GetD1SysClockFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 556 bytes, Stack size 16 bytes, stm32h7xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_GetD1SysClockFreq

  HAL_RCC_OscConfig (Thumb, 1716 bytes, Stack size 16 bytes, stm32h7xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SDRAM_Init (Thumb, 76 bytes, Stack size 16 bytes, stm32h7xx_hal_sdram.o(i.HAL_SDRAM_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_SDRAM_Init ⇒ HAL_SDRAM_MspInit ⇒ HAL_FMC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SDRAM_MspInit
  - >> FMC_SDRAM_Timing_Init
  - >> FMC_SDRAM_Init
  [Called By]
  - >> MX_FMC_Init

  HAL_SDRAM_MspInit (Thumb, 10 bytes, Stack size 8 bytes, fmc.o(i.HAL_SDRAM_MspInit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_SDRAM_MspInit ⇒ HAL_FMC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_FMC_MspInit
  [Called By]
  - >> HAL_SDRAM_Init

  HAL_SDRAM_ProgramRefreshRate (Thumb, 40 bytes, Stack size 16 bytes, stm32h7xx_hal_sdram.o(i.HAL_SDRAM_ProgramRefreshRate))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_SDRAM_ProgramRefreshRate
  [Calls]
  - >> FMC_SDRAM_ProgramRefreshRate
  [Called By]
  - >> BSP_SDRAM_Initialization_sequence

  HAL_SDRAM_SendCommand (Thumb, 58 bytes, Stack size 16 bytes, stm32h7xx_hal_sdram.o(i.HAL_SDRAM_SendCommand))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_SDRAM_SendCommand ⇒ FMC_SDRAM_SendCommand
  [Calls]
  - >> FMC_SDRAM_SendCommand
  [Called By]
  - >> BSP_SDRAM_Initialization_sequence

  HAL_SYSTICK_Config (Thumb, 52 bytes, Stack size 16 bytes, stm32h7xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_SYSTICK_Config ⇒ __NVIC_SetPriority
  [Calls]
  - >> __NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick

  HAL_TIMEx_MasterConfigSynchronization (Thumb, 98 bytes, Stack size 12 bytes, stm32h7xx_hal_tim_ex.o(i.HAL_TIMEx_MasterConfigSynchronization))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> MX_TIM2_Init

  HAL_TIM_MspPostInit (Thumb, 80 bytes, Stack size 32 bytes, tim.o(i.HAL_TIM_MspPostInit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> __aeabi_memclr4
  [Called By]
  - >> MX_TIM2_Init

  HAL_TIM_PWM_ConfigChannel (Thumb, 372 bytes, Stack size 16 bytes, stm32h7xx_hal_tim.o(i.HAL_TIM_PWM_ConfigChannel))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_PWM_ConfigChannel ⇒ TIM_OC6_SetConfig
  [Calls]
  - >> TIM_OC6_SetConfig
  - >> TIM_OC5_SetConfig
  - >> TIM_OC4_SetConfig
  - >> TIM_OC3_SetConfig
  - >> TIM_OC2_SetConfig
  - >> TIM_OC1_SetConfig
  [Called By]
  - >> MX_TIM2_Init

  HAL_TIM_PWM_Init (Thumb, 52 bytes, Stack size 8 bytes, stm32h7xx_hal_tim.o(i.HAL_TIM_PWM_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_TIM_PWM_Init ⇒ HAL_TIM_PWM_MspInit
  [Calls]
  - >> HAL_TIM_PWM_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> MX_TIM2_Init

  HAL_TIM_PWM_MspInit (Thumb, 40 bytes, Stack size 8 bytes, tim.o(i.HAL_TIM_PWM_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_TIM_PWM_MspInit
  [Called By]
  - >> HAL_TIM_PWM_Init

  HAL_TIM_PWM_Start (Thumb, 92 bytes, Stack size 12 bytes, stm32h7xx_hal_tim.o(i.HAL_TIM_PWM_Start))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_TIM_PWM_Start ⇒ TIM_CCxChannelCmd
  [Calls]
  - >> TIM_CCxChannelCmd
  [Called By]
  - >> main

  HAL_UART_Init (Thumb, 120 bytes, Stack size 8 bytes, stm32h7xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 120
  - Call Chain = HAL_UART_Init ⇒ UART_SetConfig ⇒ HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCCEx_GetD1SysClockFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  - >> UART_CheckIdleState
  - >> UART_AdvFeatureConfig
  [Called By]
  - >> MX_USART1_UART_Init

  HAL_UART_MspInit (Thumb, 114 bytes, Stack size 32 bytes, usart.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> __aeabi_memclr4
  [Called By]
  - >> HAL_UART_Init

  HAL_UART_Transmit (Thumb, 198 bytes, Stack size 32 bytes, stm32h7xx_hal_uart.o(i.HAL_UART_Transmit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> fputc

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32h7xx_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  I2C_Ack (Thumb, 76 bytes, Stack size 8 bytes, analog_i2c.o(i.I2C_Ack))
  [Stack]

  - Max Depth = 72
  - Call Chain = I2C_Ack ⇒ DEV_Set_GPIOMode ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> DEV_Set_GPIOMode
  - >> DEV_Delay_us
  [Called By]
  - >> I2C_Read_Byte

  I2C_NAck (Thumb, 64 bytes, Stack size 8 bytes, analog_i2c.o(i.I2C_NAck))
  [Stack]

  - Max Depth = 72
  - Call Chain = I2C_NAck ⇒ DEV_Set_GPIOMode ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> DEV_Set_GPIOMode
  - >> DEV_Delay_us
  [Called By]
  - >> I2C_Read_Byte

  I2C_Read_Byte (Thumb, 106 bytes, Stack size 16 bytes, analog_i2c.o(i.I2C_Read_Byte))
  [Stack]

  - Max Depth = 88
  - Call Chain = I2C_Read_Byte ⇒ I2C_NAck ⇒ DEV_Set_GPIOMode ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_ReadPin
  - >> I2C_NAck
  - >> I2C_Ack
  - >> DEV_Set_GPIOMode
  - >> DEV_Delay_us
  [Called By]
  - >> GT7385_RD_Reg

  I2C_Send_Byte (Thumb, 144 bytes, Stack size 16 bytes, analog_i2c.o(i.I2C_Send_Byte))
  [Stack]

  - Max Depth = 80
  - Call Chain = I2C_Send_Byte ⇒ DEV_Set_GPIOMode ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> DEV_Set_GPIOMode
  - >> DEV_Delay_us
  [Called By]
  - >> GT7385_WR_Reg
  - >> GT7385_RD_Reg

  I2C_Start (Thumb, 82 bytes, Stack size 8 bytes, analog_i2c.o(i.I2C_Start))
  [Stack]

  - Max Depth = 72
  - Call Chain = I2C_Start ⇒ DEV_Set_GPIOMode ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> DEV_Set_GPIOMode
  - >> DEV_Delay_us
  [Called By]
  - >> GT7385_WR_Reg
  - >> GT7385_RD_Reg

  I2C_Stop (Thumb, 66 bytes, Stack size 8 bytes, analog_i2c.o(i.I2C_Stop))
  [Stack]

  - Max Depth = 72
  - Call Chain = I2C_Stop ⇒ DEV_Set_GPIOMode ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> DEV_Set_GPIOMode
  - >> DEV_Delay_us
  [Called By]
  - >> I2C_Wait_Ack
  - >> GT7385_WR_Reg
  - >> GT7385_RD_Reg

  I2C_Wait_Ack (Thumb, 92 bytes, Stack size 8 bytes, analog_i2c.o(i.I2C_Wait_Ack))
  [Stack]

  - Max Depth = 80
  - Call Chain = I2C_Wait_Ack ⇒ I2C_Stop ⇒ DEV_Set_GPIOMode ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_ReadPin
  - >> I2C_Stop
  - >> DEV_Set_GPIOMode
  - >> DEV_Delay_us
  [Called By]
  - >> GT7385_WR_Reg
  - >> GT7385_RD_Reg

  MX_CRC_Init (Thumb, 42 bytes, Stack size 8 bytes, crc.o(i.MX_CRC_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = MX_CRC_Init ⇒ Error_Handler ⇒ __2printf
  [Calls]
  - >> HAL_CRC_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MX_DMA2D_Init (Thumb, 62 bytes, Stack size 8 bytes, dma2d.o(i.MX_DMA2D_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = MX_DMA2D_Init ⇒ HAL_DMA2D_Init ⇒ HAL_DMA2D_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_DMA2D_Init
  - >> HAL_DMA2D_ConfigLayer
  - >> Error_Handler
  [Called By]
  - >> main

  MX_FMC_Init (Thumb, 100 bytes, Stack size 32 bytes, fmc.o(i.MX_FMC_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = MX_FMC_Init ⇒ HAL_SDRAM_Init ⇒ HAL_SDRAM_MspInit ⇒ HAL_FMC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SDRAM_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MX_GPIO_Init (Thumb, 390 bytes, Stack size 32 bytes, gpio.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = MX_GPIO_Init ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  - >> HAL_GPIO_WritePin
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  MX_LTDC_Init (Thumb, 288 bytes, Stack size 112 bytes, ltdc.o(i.MX_LTDC_Init))
  [Stack]

  - Max Depth = 184
  - Call Chain = MX_LTDC_Init ⇒ HAL_LTDC_Init ⇒ HAL_LTDC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_LTDC_Init
  - >> HAL_LTDC_ConfigLayer
  - >> Error_Handler
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  MX_TIM2_Init (Thumb, 124 bytes, Stack size 48 bytes, tim.o(i.MX_TIM2_Init))
  [Stack]

  - Max Depth = 104
  - Call Chain = MX_TIM2_Init ⇒ HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_TIM_PWM_Init
  - >> HAL_TIM_PWM_ConfigChannel
  - >> HAL_TIMEx_MasterConfigSynchronization
  - >> HAL_TIM_MspPostInit
  - >> Error_Handler
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  MX_USART1_UART_Init (Thumb, 64 bytes, Stack size 8 bytes, usart.o(i.MX_USART1_UART_Init))
  [Stack]

  - Max Depth = 128
  - Call Chain = MX_USART1_UART_Init ⇒ HAL_UART_Init ⇒ UART_SetConfig ⇒ HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCCEx_GetD1SysClockFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_UART_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32h7xx_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32h7xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  Paint_Clear (Thumb, 12 bytes, Stack size 8 bytes, gui_paint.o(i.Paint_Clear))
  [Stack]

  - Max Depth = 136
  - Call Chain = Paint_Clear ⇒ BSP_LCD_Clear ⇒ LL_FillBuffer ⇒ HAL_DMA2D_Init ⇒ HAL_DMA2D_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> BSP_LCD_Clear
  [Called By]
  - >> main
  - >> Touch_Draw

  Paint_DrawChar (Thumb, 276 bytes, Stack size 40 bytes, gui_paint.o(i.Paint_DrawChar))
  [Stack]

  - Max Depth = 88
  - Call Chain = Paint_DrawChar ⇒ Paint_SetPixel ⇒ __2printf
  [Calls]
  - >> __2printf
  - >> Paint_SetPixel
  [Called By]
  - >> Paint_DrawString_EN

  Paint_DrawCircle (Thumb, 508 bytes, Stack size 40 bytes, gui_paint.o(i.Paint_DrawCircle))
  [Stack]

  - Max Depth = 120
  - Call Chain = Paint_DrawCircle ⇒ Paint_DrawPoint ⇒ Paint_SetPixel ⇒ __2printf
  [Calls]
  - >> __2printf
  - >> Paint_DrawPoint
  [Called By]
  - >> Touch_Draw
  - >> GT7385_Scan

  Paint_DrawLine (Thumb, 256 bytes, Stack size 56 bytes, gui_paint.o(i.Paint_DrawLine))
  [Stack]

  - Max Depth = 136
  - Call Chain = Paint_DrawLine ⇒ Paint_DrawPoint ⇒ Paint_SetPixel ⇒ __2printf
  [Calls]
  - >> __2printf
  - >> Paint_DrawPoint
  [Called By]
  - >> Paint_DrawRectangle
  - >> Touch_Draw
  - >> GT7385_Scan

  Paint_DrawPoint (Thumb, 162 bytes, Stack size 32 bytes, gui_paint.o(i.Paint_DrawPoint))
  [Stack]

  - Max Depth = 80
  - Call Chain = Paint_DrawPoint ⇒ Paint_SetPixel ⇒ __2printf
  [Calls]
  - >> Paint_SetPixel
  [Called By]
  - >> Paint_DrawLine
  - >> Paint_DrawCircle

  Paint_DrawRectangle (Thumb, 188 bytes, Stack size 48 bytes, gui_paint.o(i.Paint_DrawRectangle))
  [Stack]

  - Max Depth = 184
  - Call Chain = Paint_DrawRectangle ⇒ Paint_DrawLine ⇒ Paint_DrawPoint ⇒ Paint_SetPixel ⇒ __2printf
  [Calls]
  - >> Paint_DrawLine
  - >> __2printf
  [Called By]
  - >> Touch_Draw

  Paint_DrawString_CN (Thumb, 538 bytes, Stack size 56 bytes, gui_paint.o(i.Paint_DrawString_CN))
  [Stack]

  - Max Depth = 104
  - Call Chain = Paint_DrawString_CN ⇒ Paint_SetPixel ⇒ __2printf
  [Calls]
  - >> Paint_SetPixel
  [Called By]
  - >> Touch_Draw

  Paint_DrawString_EN (Thumb, 122 bytes, Stack size 48 bytes, gui_paint.o(i.Paint_DrawString_EN))
  [Stack]

  - Max Depth = 136
  - Call Chain = Paint_DrawString_EN ⇒ Paint_DrawChar ⇒ Paint_SetPixel ⇒ __2printf
  [Calls]
  - >> __2printf
  - >> Paint_DrawChar
  [Called By]
  - >> Touch_Draw

  Paint_NewImage (Thumb, 68 bytes, Stack size 24 bytes, gui_paint.o(i.Paint_NewImage))
  [Stack]

  - Max Depth = 48
  - Call Chain = Paint_NewImage ⇒ __2printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> main

  Paint_SetPixel (Thumb, 228 bytes, Stack size 24 bytes, gui_paint.o(i.Paint_SetPixel))
  [Stack]

  - Max Depth = 48
  - Call Chain = Paint_SetPixel ⇒ __2printf
  [Calls]
  - >> __2printf
  - >> BSP_LCD_DrawPixel
  [Called By]
  - >> Paint_DrawString_CN
  - >> Paint_DrawPoint
  - >> Paint_DrawChar

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32h7xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32h7xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  SysTick_Handler (Thumb, 8 bytes, Stack size 8 bytes, stm32h7xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = SysTick_Handler
  [Calls]
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32h743xx.o(RESET)

  SystemClock_Config (Thumb, 266 bytes, Stack size 304 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 384
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> Error_Handler
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  SystemInit (Thumb, 130 bytes, Stack size 0 bytes, system_stm32h7xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(.text)

  TIM_Base_SetConfig (Thumb, 172 bytes, Stack size 8 bytes, stm32h7xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_Init

  TIM_CCxChannelCmd (Thumb, 28 bytes, Stack size 12 bytes, stm32h7xx_hal_tim.o(i.TIM_CCxChannelCmd))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_CCxChannelCmd
  [Called By]
  - >> HAL_TIM_PWM_Start

  TIM_OC1_SetConfig (Thumb, 152 bytes, Stack size 12 bytes, stm32h7xx_hal_tim.o(i.TIM_OC1_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC1_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  TIM_OC2_SetConfig (Thumb, 162 bytes, Stack size 12 bytes, stm32h7xx_hal_tim.o(i.TIM_OC2_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC2_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  TIM_OC3_SetConfig (Thumb, 160 bytes, Stack size 12 bytes, stm32h7xx_hal_tim.o(i.TIM_OC3_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC3_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  TIM_OC4_SetConfig (Thumb, 98 bytes, Stack size 12 bytes, stm32h7xx_hal_tim.o(i.TIM_OC4_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC4_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  Touch_Draw (Thumb, 252 bytes, Stack size 16 bytes, main.o(i.Touch_Draw))
  [Stack]

  - Max Depth = 264
  - Call Chain = Touch_Draw ⇒ GT7385_Init ⇒ GT7385_Scan ⇒ Paint_DrawLine ⇒ Paint_DrawPoint ⇒ Paint_SetPixel ⇒ __2printf
  [Calls]
  - >> Paint_DrawString_EN
  - >> Paint_DrawString_CN
  - >> Paint_DrawRectangle
  - >> Paint_DrawLine
  - >> Paint_DrawCircle
  - >> Paint_Clear
  - >> HAL_Delay
  - >> GT7385_Init
  [Called By]
  - >> main

  UART_AdvFeatureConfig (Thumb, 234 bytes, Stack size 0 bytes, stm32h7xx_hal_uart.o(i.UART_AdvFeatureConfig))
  [Called By]

  - >> HAL_UART_Init

  UART_CheckIdleState (Thumb, 116 bytes, Stack size 16 bytes, stm32h7xx_hal_uart.o(i.UART_CheckIdleState))
  [Stack]

  - Max Depth = 40
  - Call Chain = UART_CheckIdleState ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> HAL_UART_Init

  UART_SetConfig (Thumb, 2452 bytes, Stack size 72 bytes, stm32h7xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 112
  - Call Chain = UART_SetConfig ⇒ HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCCEx_GetD1SysClockFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  - >> HAL_RCCEx_GetPLL3ClockFreq
  - >> HAL_RCCEx_GetPLL2ClockFreq
  - >> HAL_RCCEx_GetD3PCLK1Freq
  - >> __aeabi_uldivmod
  [Called By]
  - >> HAL_UART_Init

  UART_WaitOnFlagUntilTimeout (Thumb, 108 bytes, Stack size 24 bytes, stm32h7xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_UART_Transmit
  - >> UART_CheckIdleState

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32h7xx_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32h743xx.o(RESET)

  __0printf$5 (Thumb, 22 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$5 (Thumb, 0 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> Paint_NewImage
  - >> Paint_DrawString_EN
  - >> Paint_DrawRectangle
  - >> Paint_DrawLine
  - >> Paint_DrawCircle
  - >> GT7385_Init
  - >> main
  - >> Error_Handler
  - >> GT7385_Scan
  - >> GT7385_Read_ID
  - >> GT7385_Read_FirmwareVersion
  - >> Paint_SetPixel
  - >> Paint_DrawChar

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  fputc (Thumb, 22 bytes, Stack size 16 bytes, usart.o(i.fputc))
  [Stack]

  - Max Depth = 72
  - Call Chain = fputc ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  [Address Reference Count : 1]
  - printf5.o(i.__0printf$5)

  main (Thumb, 120 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 384
  - Call Chain = main ⇒ SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> Paint_NewImage
  - >> Paint_Clear
  - >> MX_USART1_UART_Init
  - >> MX_TIM2_Init
  - >> MX_LTDC_Init
  - >> MX_GPIO_Init
  - >> MX_FMC_Init
  - >> MX_DMA2D_Init
  - >> MX_CRC_Init
  - >> HAL_TIM_PWM_Start
  - >> HAL_Init
  - >> HAL_GPIO_WritePin
  - >> HAL_Delay
  - >> BSP_LCD_Init
  - >> Touch_Draw
  - >> SystemClock_Config
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  HAL_FMC_MspInit (Thumb, 200 bytes, Stack size 32 bytes, fmc.o(i.HAL_FMC_MspInit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_FMC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_SDRAM_MspInit

  __NVIC_GetPriorityGrouping (Thumb, 10 bytes, Stack size 0 bytes, stm32h7xx_hal_cortex.o(i.__NVIC_GetPriorityGrouping))
  [Called By]

  - >> HAL_NVIC_SetPriority

  __NVIC_SetPriority (Thumb, 32 bytes, Stack size 8 bytes, stm32h7xx_hal_cortex.o(i.__NVIC_SetPriority))
  [Stack]

  - Max Depth = 8
  - Call Chain = __NVIC_SetPriority
  [Called By]
  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config

  DMA2D_SetConfig (Thumb, 258 bytes, Stack size 32 bytes, stm32h7xx_hal_dma2d.o(i.DMA2D_SetConfig))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA2D_SetConfig
  [Called By]
  - >> HAL_DMA2D_Start

  LTDC_SetConfig (Thumb, 530 bytes, Stack size 20 bytes, stm32h7xx_hal_ltdc.o(i.LTDC_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = LTDC_SetConfig
  [Called By]
  - >> HAL_LTDC_ConfigLayer

  TIM_OC5_SetConfig (Thumb, 92 bytes, Stack size 12 bytes, stm32h7xx_hal_tim.o(i.TIM_OC5_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC5_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  TIM_OC6_SetConfig (Thumb, 94 bytes, Stack size 12 bytes, stm32h7xx_hal_tim.o(i.TIM_OC6_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC6_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  RCCEx_PLL2_Config (Thumb, 300 bytes, Stack size 24 bytes, stm32h7xx_hal_rcc_ex.o(i.RCCEx_PLL2_Config))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCCEx_PLL2_Config
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RCCEx_PeriphCLKConfig

  RCCEx_PLL3_Config (Thumb, 300 bytes, Stack size 24 bytes, stm32h7xx_hal_rcc_ex.o(i.RCCEx_PLL3_Config))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCCEx_PLL3_Config
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RCCEx_PeriphCLKConfig

  LL_FillBuffer (Thumb, 144 bytes, Stack size 32 bytes, bsp_rgb_lcd.o(i.LL_FillBuffer))
  [Stack]

  - Max Depth = 104
  - Call Chain = LL_FillBuffer ⇒ HAL_DMA2D_Init ⇒ HAL_DMA2D_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_DMA2D_Init
  - >> HAL_DMA2D_ConfigLayer
  - >> HAL_DMA2D_Start
  - >> HAL_DMA2D_PollForTransfer
  [Called By]
  - >> BSP_LCD_Clear

  GT7385_RD_Reg (Thumb, 102 bytes, Stack size 24 bytes, gt7385.o(i.GT7385_RD_Reg))
  [Stack]

  - Max Depth = 112
  - Call Chain = GT7385_RD_Reg ⇒ I2C_Read_Byte ⇒ I2C_NAck ⇒ DEV_Set_GPIOMode ⇒ HAL_GPIO_Init
  [Calls]
  - >> I2C_Wait_Ack
  - >> I2C_Stop
  - >> I2C_Start
  - >> I2C_Send_Byte
  - >> I2C_Read_Byte
  [Called By]
  - >> GT7385_Scan
  - >> GT7385_Read_ID
  - >> GT7385_Read_FirmwareVersion

  GT7385_Read_FirmwareVersion (Thumb, 82 bytes, Stack size 16 bytes, gt7385.o(i.GT7385_Read_FirmwareVersion))
  [Stack]

  - Max Depth = 128
  - Call Chain = GT7385_Read_FirmwareVersion ⇒ GT7385_RD_Reg ⇒ I2C_Read_Byte ⇒ I2C_NAck ⇒ DEV_Set_GPIOMode ⇒ HAL_GPIO_Init
  [Calls]
  - >> __2printf
  - >> GT7385_RD_Reg
  [Called By]
  - >> GT7385_Init

  GT7385_Read_ID (Thumb, 68 bytes, Stack size 16 bytes, gt7385.o(i.GT7385_Read_ID))
  [Stack]

  - Max Depth = 128
  - Call Chain = GT7385_Read_ID ⇒ GT7385_RD_Reg ⇒ I2C_Read_Byte ⇒ I2C_NAck ⇒ DEV_Set_GPIOMode ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_Delay
  - >> __2printf
  - >> GT7385_WR_Reg
  - >> GT7385_RD_Reg
  [Called By]
  - >> GT7385_Init

  GT7385_Reset (Thumb, 92 bytes, Stack size 24 bytes, gt7385.o(i.GT7385_Reset))
  [Stack]

  - Max Depth = 88
  - Call Chain = GT7385_Reset ⇒ DEV_Set_GPIOMode ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> HAL_GPIO_WritePin
  - >> HAL_Delay
  - >> DEV_Set_GPIOMode
  [Called By]
  - >> GT7385_Init

  GT7385_WR_Reg (Thumb, 92 bytes, Stack size 24 bytes, gt7385.o(i.GT7385_WR_Reg))
  [Stack]

  - Max Depth = 104
  - Call Chain = GT7385_WR_Reg ⇒ I2C_Wait_Ack ⇒ I2C_Stop ⇒ DEV_Set_GPIOMode ⇒ HAL_GPIO_Init
  [Calls]
  - >> I2C_Wait_Ack
  - >> I2C_Stop
  - >> I2C_Start
  - >> I2C_Send_Byte
  [Called By]
  - >> GT7385_Scan
  - >> GT7385_Read_ID

  _printf_core (Thumb, 658 bytes, Stack size 104 bytes, printf5.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  [Called By]
  - >> __0printf$5

  ### Undefined Global Symbols