#MicroXplorer Configuration settings - do not modify
DMA2D.ColorMode=DMA2D_OUTPUT_RGB565
DMA2D.IPParameters=ColorMode
FMC.CASLatency1=FMC_SDRAM_CAS_LATENCY_3
FMC.ExitSelfRefreshDelay1=7
FMC.IPParameters=CASLatency1,SDClockPeriod1,ReadPipeDelay1,LoadToActiveDelay1,ExitSelfRefreshDelay1,SelfRefreshTime1,RowCycleDelay1,WriteRecoveryTime1,RPDelay1,RCDDelay1
FMC.LoadToActiveDelay1=2
FMC.RCDDelay1=2
FMC.RPDelay1=2
FMC.ReadPipeDelay1=FMC_SDRAM_RPIPE_DELAY_1
FMC.RowCycleDelay1=6
FMC.SDClockPeriod1=FMC_SDRAM_CLOCK_PERIOD_2
FMC.SelfRefreshTime1=4
FMC.WriteRecoveryTime1=2
File.Version=6
KeepUserPlacement=false
LTDC.ActiveH=600
LTDC.ActiveW=1024
LTDC.Alpha_L0=0xff
LTDC.FBStartAdress_L0=0xD0000000
LTDC.FBStartAdress_L1=0xD0200000
LTDC.HBP=46
LTDC.HSync=30
LTDC.IPParameters=HSync,HBP,ActiveW,VSync,VBP,VFP,WindowX1_L0,WindowY1_L0,WindowX1_L1,WindowY1_L1,PixelFormat_L0,PixelFormat_L1,Alpha_L0,FBStartAdress_L0,ImageWidth_L0,ImageHeight_L0,FBStartAdress_L1,ImageWidth_L1,ImageHeight_L1,ActiveH
LTDC.ImageHeight_L0=600
LTDC.ImageHeight_L1=600
LTDC.ImageWidth_L0=1024
LTDC.ImageWidth_L1=1024
LTDC.PixelFormat_L0=LTDC_PIXEL_FORMAT_RGB565
LTDC.PixelFormat_L1=LTDC_PIXEL_FORMAT_RGB565
LTDC.VBP=23
LTDC.VFP=22
LTDC.VSync=10
LTDC.WindowX1_L0=1024
LTDC.WindowX1_L1=1024
LTDC.WindowY1_L0=600
LTDC.WindowY1_L1=600
Mcu.Family=STM32H7
Mcu.IP0=CORTEX_M7
Mcu.IP1=CRC
Mcu.IP2=DMA2D
Mcu.IP3=FMC
Mcu.IP4=LTDC
Mcu.IP5=NVIC
Mcu.IP6=RCC
Mcu.IP7=SYS
Mcu.IP8=TIM2
Mcu.IP9=USART1
Mcu.IPNb=10
Mcu.Name=STM32H743IITx
Mcu.Package=LQFP176
Mcu.Pin0=PE4
Mcu.Pin1=PE5
Mcu.Pin10=PF4
Mcu.Pin11=PF5
Mcu.Pin12=PF6
Mcu.Pin13=PF7
Mcu.Pin14=PF8
Mcu.Pin15=PF10
Mcu.Pin16=PH0-OSC_IN (PH0)
Mcu.Pin17=PH1-OSC_OUT (PH1)
Mcu.Pin18=PC0
Mcu.Pin19=PH2
Mcu.Pin2=PE6
Mcu.Pin20=PH3
Mcu.Pin21=PH5
Mcu.Pin22=PA3
Mcu.Pin23=PB1
Mcu.Pin24=PF11
Mcu.Pin25=PF12
Mcu.Pin26=PF13
Mcu.Pin27=PF14
Mcu.Pin28=PF15
Mcu.Pin29=PG0
Mcu.Pin3=PI8
Mcu.Pin30=PG1
Mcu.Pin31=PE7
Mcu.Pin32=PE8
Mcu.Pin33=PE9
Mcu.Pin34=PE10
Mcu.Pin35=PE11
Mcu.Pin36=PE12
Mcu.Pin37=PE13
Mcu.Pin38=PE14
Mcu.Pin39=PE15
Mcu.Pin4=PI9
Mcu.Pin40=PH6
Mcu.Pin41=PH7
Mcu.Pin42=PH8
Mcu.Pin43=PH9
Mcu.Pin44=PH10
Mcu.Pin45=PD8
Mcu.Pin46=PD9
Mcu.Pin47=PD10
Mcu.Pin48=PD14
Mcu.Pin49=PD15
Mcu.Pin5=PI10
Mcu.Pin50=PG4
Mcu.Pin51=PG5
Mcu.Pin52=PG6
Mcu.Pin53=PG7
Mcu.Pin54=PG8
Mcu.Pin55=PA9
Mcu.Pin56=PA10
Mcu.Pin57=PA13 (JTMS/SWDIO)
Mcu.Pin58=PH13
Mcu.Pin59=PH15
Mcu.Pin6=PF0
Mcu.Pin60=PI0
Mcu.Pin61=PI1
Mcu.Pin62=PI2
Mcu.Pin63=PA14 (JTCK/SWCLK)
Mcu.Pin64=PA15 (JTDI)
Mcu.Pin65=PD0
Mcu.Pin66=PD1
Mcu.Pin67=PD6
Mcu.Pin68=PD7
Mcu.Pin69=PG10
Mcu.Pin7=PF1
Mcu.Pin70=PG11
Mcu.Pin71=PG12
Mcu.Pin72=PG15
Mcu.Pin73=PB3 (JTDO/TRACESWO)
Mcu.Pin74=PB4 (NJTRST)
Mcu.Pin75=PE0
Mcu.Pin76=PE1
Mcu.Pin77=PI4
Mcu.Pin78=PI5
Mcu.Pin79=PI6
Mcu.Pin8=PF2
Mcu.Pin80=PI7
Mcu.Pin81=VP_CRC_VS_CRC
Mcu.Pin82=VP_DMA2D_VS_DMA2D
Mcu.Pin83=VP_SYS_VS_Systick
Mcu.Pin9=PF3
Mcu.PinsNb=84
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32H743IITx
MxCube.Version=5.0.0
MxDb.Version=DB.5.0.0
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false
NVIC.DMA2D_IRQn=true\:0\:0\:false\:false\:true\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false
NVIC.EXTI9_5_IRQn=true\:6\:0\:true\:false\:true\:true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false
NVIC.PendSV_IRQn=true\:0\:0\:false\:false\:true\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:true\:false
NVIC.SysTick_IRQn=true\:0\:0\:false\:false\:true\:false
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false
PA10.Locked=true
PA10.Mode=Asynchronous
PA10.Signal=USART1_RX
PA13\ (JTMS/SWDIO).Mode=JTAG_5_pins
PA13\ (JTMS/SWDIO).Signal=SYS_JTMS-SWDIO
PA14\ (JTCK/SWCLK).Mode=JTAG_5_pins
PA14\ (JTCK/SWCLK).Signal=SYS_JTCK-SWCLK
PA15\ (JTDI).Mode=JTAG_5_pins
PA15\ (JTDI).Signal=SYS_JTDI
PA3.Locked=true
PA3.Signal=S_TIM2_CH4
PA9.Locked=true
PA9.Mode=Asynchronous
PA9.Signal=USART1_TX
PB1.GPIOParameters=GPIO_Speed
PB1.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PB1.Mode=RGB888
PB1.Signal=LTDC_R6
PB3\ (JTDO/TRACESWO).Mode=JTAG_5_pins
PB3\ (JTDO/TRACESWO).Signal=SYS_JTDO-SWO
PB4\ (NJTRST).Mode=JTAG_5_pins
PB4\ (NJTRST).Signal=SYS_JTRST
PC0.Mode=RGB888
PC0.Signal=LTDC_R5
PCC.Checker=false
PCC.Line=STM32H743/753
PCC.MCU=STM32H743IITx
PCC.PartNumber=STM32H743IITx
PCC.Seq0=0
PCC.Series=STM32H7
PCC.Temperature=25
PCC.Vdd=3.0
PD0.Signal=FMC_D2_DA2
PD1.Signal=FMC_D3_DA3
PD10.Signal=FMC_D15_DA15
PD14.Signal=FMC_D0_DA0
PD15.Signal=FMC_D1_DA1
PD6.Mode=RGB888
PD6.Signal=LTDC_B2
PD7.GPIOParameters=GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultEXTI
PD7.GPIO_Label=INT
PD7.GPIO_ModeDefaultEXTI=GPIO_MODE_IT_FALLING
PD7.GPIO_PuPd=GPIO_PULLUP
PD7.Locked=true
PD7.Signal=GPXTI7
PD8.Signal=FMC_D13_DA13
PD9.Signal=FMC_D14_DA14
PE0.Signal=FMC_NBL0
PE1.Signal=FMC_NBL1
PE10.Signal=FMC_D7_DA7
PE11.Signal=FMC_D8_DA8
PE12.Signal=FMC_D9_DA9
PE13.Signal=FMC_D10_DA10
PE14.Signal=FMC_D11_DA11
PE15.Signal=FMC_D12_DA12
PE4.Mode=RGB888
PE4.Signal=LTDC_B0
PE5.Mode=RGB888
PE5.Signal=LTDC_G0
PE6.Mode=RGB888
PE6.Signal=LTDC_G1
PE7.Signal=FMC_D4_DA4
PE8.Signal=FMC_D5_DA5
PE9.Signal=FMC_D6_DA6
PF0.Signal=FMC_A0
PF1.Signal=FMC_A1
PF10.Mode=RGB888
PF10.Signal=LTDC_DE
PF11.Signal=FMC_SDNRAS
PF12.Signal=FMC_A6
PF13.Signal=FMC_A7
PF14.Signal=FMC_A8
PF15.Signal=FMC_A9
PF2.Signal=FMC_A2
PF3.Signal=FMC_A3
PF4.Signal=FMC_A4
PF5.Signal=FMC_A5
PF6.GPIOParameters=PinState,GPIO_Label,GPIO_ModeDefaultOutputPP
PF6.GPIO_Label=RST
PF6.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_PP
PF6.Locked=true
PF6.PinState=GPIO_PIN_RESET
PF6.Signal=GPIO_Output
PF7.GPIOParameters=PinState,GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultOutputPP
PF7.GPIO_Label=SCL
PF7.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_PP
PF7.GPIO_PuPd=GPIO_PULLUP
PF7.Locked=true
PF7.PinState=GPIO_PIN_SET
PF7.Signal=GPIO_Output
PF8.GPIOParameters=PinState,GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultOutputPP
PF8.GPIO_Label=SDA
PF8.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_PP
PF8.GPIO_PuPd=GPIO_PULLUP
PF8.Locked=true
PF8.PinState=GPIO_PIN_SET
PF8.Signal=GPIO_Output
PG0.Signal=FMC_A10
PG1.Signal=FMC_A11
PG10.Locked=true
PG10.Mode=RGB888
PG10.Signal=LTDC_G3
PG11.Locked=true
PG11.Mode=RGB888
PG11.Signal=LTDC_B3
PG12.Mode=RGB888
PG12.Signal=LTDC_B1
PG15.Signal=FMC_SDNCAS
PG4.Signal=FMC_A14_BA0
PG5.Signal=FMC_A15_BA1
PG6.Mode=RGB888
PG6.Signal=LTDC_R7
PG7.GPIOParameters=GPIO_Speed
PG7.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PG7.Mode=RGB888
PG7.Signal=LTDC_CLK
PG8.Signal=FMC_SDCLK
PH0-OSC_IN\ (PH0).Mode=HSE-External-Oscillator
PH0-OSC_IN\ (PH0).Signal=RCC_OSC_IN
PH1-OSC_OUT\ (PH1).Mode=HSE-External-Oscillator
PH1-OSC_OUT\ (PH1).Signal=RCC_OSC_OUT
PH10.Locked=true
PH10.Mode=RGB888
PH10.Signal=LTDC_R4
PH13.Locked=true
PH13.Mode=RGB888
PH13.Signal=LTDC_G2
PH15.Locked=true
PH15.Mode=RGB888
PH15.Signal=LTDC_G4
PH2.Mode=RGB888
PH2.Signal=LTDC_R0
PH3.Locked=true
PH3.Mode=RGB888
PH3.Signal=LTDC_R1
PH5.Locked=true
PH5.Signal=FMC_SDNWE
PH6.Mode=SdramChipSelect2_1
PH6.Signal=FMC_SDNE1
PH7.Mode=SdramChipSelect2_1
PH7.Signal=FMC_SDCKE1
PH8.Locked=true
PH8.Mode=RGB888
PH8.Signal=LTDC_R2
PH9.Locked=true
PH9.Mode=RGB888
PH9.Signal=LTDC_R3
PI0.Locked=true
PI0.Mode=RGB888
PI0.Signal=LTDC_G5
PI1.Locked=true
PI1.Mode=RGB888
PI1.Signal=LTDC_G6
PI10.GPIOParameters=GPIO_Speed
PI10.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI10.Mode=RGB888
PI10.Signal=LTDC_HSYNC
PI2.Mode=RGB888
PI2.Signal=LTDC_G7
PI4.Locked=true
PI4.Mode=RGB888
PI4.Signal=LTDC_B4
PI5.Locked=true
PI5.Mode=RGB888
PI5.Signal=LTDC_B5
PI6.Locked=true
PI6.Mode=RGB888
PI6.Signal=LTDC_B6
PI7.Locked=true
PI7.Mode=RGB888
PI7.Signal=LTDC_B7
PI8.GPIOParameters=PinState,GPIO_Label
PI8.GPIO_Label=DISP
PI8.Locked=true
PI8.PinState=GPIO_PIN_SET
PI8.Signal=GPIO_Output
PI9.GPIOParameters=GPIO_Speed
PI9.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI9.Mode=RGB888
PI9.Signal=LTDC_VSYNC
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=true
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32H743IITx
ProjectManager.FirmwarePackage=STM32Cube FW_H7 V1.3.2
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x800
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=0
ProjectManager.MainLocation=Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=LCD.ioc
ProjectManager.ProjectName=LCD
ProjectManager.StackSize=0x1000
ProjectManager.TargetToolchain=MDK-ARM V5
ProjectManager.ToolChainLocation=
ProjectManager.UnderRoot=false
ProjectManager.functionlistsort=1-MX_GPIO_Init-GPIO-false-HAL-true,2-SystemClock_Config-RCC-false-HAL-false,3-MX_CORTEX_M7_Init-CORTEX_M7-false-HAL-true,4-MX_FMC_Init-FMC-false-HAL-true,5-MX_USART1_UART_Init-USART1-false-HAL-true,6-MX_LTDC_Init-LTDC-false-HAL-true,7-MX_DMA2D_Init-DMA2D-false-HAL-true,8-MX_TIM2_Init-TIM2-false-HAL-true,9-MX_CRC_Init-CRC-false-HAL-true
RCC.ADCFreq_Value=100000000
RCC.AHB12Freq_Value=200000000
RCC.AHB4Freq_Value=200000000
RCC.APB1Freq_Value=50000000
RCC.APB2Freq_Value=100000000
RCC.APB3Freq_Value=100000000
RCC.APB4Freq_Value=100000000
RCC.AXIClockFreq_Value=200000000
RCC.CECFreq_Value=32000
RCC.CKPERFreq_Value=64000000
RCC.CPU2Freq_Value=200000000
RCC.CPU2SystikFreq_Value=200000000
RCC.CortexFreq_Value=400000000
RCC.CpuClockFreq_Value=400000000
RCC.D1CPREFreq_Value=400000000
RCC.D1PPRE=RCC_APB3_DIV2
RCC.D2PPRE1=RCC_APB1_DIV4
RCC.D2PPRE2=RCC_APB2_DIV2
RCC.D3PPRE=RCC_APB4_DIV2
RCC.DFSDMACLkFreq_Value=400000000
RCC.DFSDMFreq_Value=100000000
RCC.DIVM1=4
RCC.DIVM2=4
RCC.DIVM3=4
RCC.DIVN1=400
RCC.DIVN2=100
RCC.DIVN3=44
RCC.DIVP1Freq_Value=400000000
RCC.DIVP2Freq_Value=100000000
RCC.DIVP3Freq_Value=44000000
RCC.DIVQ1Freq_Value=400000000
RCC.DIVQ2Freq_Value=100000000
RCC.DIVQ3Freq_Value=44000000
RCC.DIVR1Freq_Value=400000000
RCC.DIVR2Freq_Value=100000000
RCC.DIVR3=4
RCC.DIVR3Freq_Value=22000000
RCC.FDCANFreq_Value=400000000
RCC.FMCFreq_Value=200000000
RCC.FamilyName=M
RCC.HCLK3ClockFreq_Value=200000000
RCC.HCLKFreq_Value=200000000
RCC.HPRE=RCC_HCLK_DIV2
RCC.HRTIMFreq_Value=200000000
RCC.HSE_VALUE=8000000
RCC.I2C123Freq_Value=50000000
RCC.I2C4Freq_Value=100000000
RCC.IPParameters=ADCFreq_Value,AHB12Freq_Value,AHB4Freq_Value,APB1Freq_Value,APB2Freq_Value,APB3Freq_Value,APB4Freq_Value,AXIClockFreq_Value,CECFreq_Value,CKPERFreq_Value,CPU2Freq_Value,CPU2SystikFreq_Value,CortexFreq_Value,CpuClockFreq_Value,D1CPREFreq_Value,D1PPRE,D2PPRE1,D2PPRE2,D3PPRE,DFSDMACLkFreq_Value,DFSDMFreq_Value,DIVM1,DIVM2,DIVM3,DIVN1,DIVN2,DIVN3,DIVP1Freq_Value,DIVP2Freq_Value,DIVP3Freq_Value,DIVQ1Freq_Value,DIVQ2Freq_Value,DIVQ3Freq_Value,DIVR1Freq_Value,DIVR2Freq_Value,DIVR3,DIVR3Freq_Value,FDCANFreq_Value,FMCFreq_Value,FamilyName,HCLK3ClockFreq_Value,HCLKFreq_Value,HPRE,HRTIMFreq_Value,HSE_VALUE,I2C123Freq_Value,I2C4Freq_Value,LPTIM1Freq_Value,LPTIM2Freq_Value,LPTIM345Freq_Value,LPUART1Freq_Value,LTDCFreq_Value,MCO1PinFreq_Value,MCO2PinFreq_Value,PLLSourceVirtual,QSPIFreq_Value,RNGFreq_Value,RTCFreq_Value,SAI1Freq_Value,SAI23Freq_Value,SAI4AFreq_Value,SAI4BFreq_Value,SDMMCFreq_Value,SPDIFRXFreq_Value,SPI123Freq_Value,SPI45Freq_Value,SPI6Freq_Value,SWPMI1Freq_Value,SYSCLKFreq_VALUE,SYSCLKSource,Tim1OutputFreq_Value,Tim2OutputFreq_Value,TraceFreq_Value,USART16Freq_Value,USART234578Freq_Value,USBFreq_Value,VCO1OutputFreq_Value,VCO2OutputFreq_Value,VCO3OutputFreq_Value,VCOInput1Freq_Value,VCOInput2Freq_Value,VCOInput3Freq_Value
RCC.LPTIM1Freq_Value=50000000
RCC.LPTIM2Freq_Value=100000000
RCC.LPTIM345Freq_Value=100000000
RCC.LPUART1Freq_Value=100000000
RCC.LTDCFreq_Value=22000000
RCC.MCO1PinFreq_Value=64000000
RCC.MCO2PinFreq_Value=400000000
RCC.PLLSourceVirtual=RCC_PLLSOURCE_HSE
RCC.QSPIFreq_Value=200000000
RCC.RNGFreq_Value=48000000
RCC.RTCFreq_Value=32000
RCC.SAI1Freq_Value=400000000
RCC.SAI23Freq_Value=400000000
RCC.SAI4AFreq_Value=400000000
RCC.SAI4BFreq_Value=400000000
RCC.SDMMCFreq_Value=400000000
RCC.SPDIFRXFreq_Value=400000000
RCC.SPI123Freq_Value=400000000
RCC.SPI45Freq_Value=100000000
RCC.SPI6Freq_Value=100000000
RCC.SWPMI1Freq_Value=50000000
RCC.SYSCLKFreq_VALUE=400000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.Tim1OutputFreq_Value=100000000
RCC.Tim2OutputFreq_Value=200000000
RCC.TraceFreq_Value=400000000
RCC.USART16Freq_Value=100000000
RCC.USART234578Freq_Value=50000000
RCC.USBFreq_Value=400000000
RCC.VCO1OutputFreq_Value=800000000
RCC.VCO2OutputFreq_Value=200000000
RCC.VCO3OutputFreq_Value=88000000
RCC.VCOInput1Freq_Value=2000000
RCC.VCOInput2Freq_Value=2000000
RCC.VCOInput3Freq_Value=2000000
SH.FMC_A0.0=FMC_A0,12b-sda1
SH.FMC_A0.ConfNb=1
SH.FMC_A1.0=FMC_A1,12b-sda1
SH.FMC_A1.ConfNb=1
SH.FMC_A10.0=FMC_A10,12b-sda1
SH.FMC_A10.ConfNb=1
SH.FMC_A11.0=FMC_A11,12b-sda1
SH.FMC_A11.ConfNb=1
SH.FMC_A14_BA0.0=FMC_BA0,FourSdramBanks1
SH.FMC_A14_BA0.ConfNb=1
SH.FMC_A15_BA1.0=FMC_BA1,FourSdramBanks1
SH.FMC_A15_BA1.ConfNb=1
SH.FMC_A2.0=FMC_A2,12b-sda1
SH.FMC_A2.ConfNb=1
SH.FMC_A3.0=FMC_A3,12b-sda1
SH.FMC_A3.ConfNb=1
SH.FMC_A4.0=FMC_A4,12b-sda1
SH.FMC_A4.ConfNb=1
SH.FMC_A5.0=FMC_A5,12b-sda1
SH.FMC_A5.ConfNb=1
SH.FMC_A6.0=FMC_A6,12b-sda1
SH.FMC_A6.ConfNb=1
SH.FMC_A7.0=FMC_A7,12b-sda1
SH.FMC_A7.ConfNb=1
SH.FMC_A8.0=FMC_A8,12b-sda1
SH.FMC_A8.ConfNb=1
SH.FMC_A9.0=FMC_A9,12b-sda1
SH.FMC_A9.ConfNb=1
SH.FMC_D0_DA0.0=FMC_D0,sd-16b-d1
SH.FMC_D0_DA0.ConfNb=1
SH.FMC_D10_DA10.0=FMC_D10,sd-16b-d1
SH.FMC_D10_DA10.ConfNb=1
SH.FMC_D11_DA11.0=FMC_D11,sd-16b-d1
SH.FMC_D11_DA11.ConfNb=1
SH.FMC_D12_DA12.0=FMC_D12,sd-16b-d1
SH.FMC_D12_DA12.ConfNb=1
SH.FMC_D13_DA13.0=FMC_D13,sd-16b-d1
SH.FMC_D13_DA13.ConfNb=1
SH.FMC_D14_DA14.0=FMC_D14,sd-16b-d1
SH.FMC_D14_DA14.ConfNb=1
SH.FMC_D15_DA15.0=FMC_D15,sd-16b-d1
SH.FMC_D15_DA15.ConfNb=1
SH.FMC_D1_DA1.0=FMC_D1,sd-16b-d1
SH.FMC_D1_DA1.ConfNb=1
SH.FMC_D2_DA2.0=FMC_D2,sd-16b-d1
SH.FMC_D2_DA2.ConfNb=1
SH.FMC_D3_DA3.0=FMC_D3,sd-16b-d1
SH.FMC_D3_DA3.ConfNb=1
SH.FMC_D4_DA4.0=FMC_D4,sd-16b-d1
SH.FMC_D4_DA4.ConfNb=1
SH.FMC_D5_DA5.0=FMC_D5,sd-16b-d1
SH.FMC_D5_DA5.ConfNb=1
SH.FMC_D6_DA6.0=FMC_D6,sd-16b-d1
SH.FMC_D6_DA6.ConfNb=1
SH.FMC_D7_DA7.0=FMC_D7,sd-16b-d1
SH.FMC_D7_DA7.ConfNb=1
SH.FMC_D8_DA8.0=FMC_D8,sd-16b-d1
SH.FMC_D8_DA8.ConfNb=1
SH.FMC_D9_DA9.0=FMC_D9,sd-16b-d1
SH.FMC_D9_DA9.ConfNb=1
SH.FMC_NBL0.0=FMC_NBL0,Sd2ByteEnable1
SH.FMC_NBL0.ConfNb=1
SH.FMC_NBL1.0=FMC_NBL1,Sd2ByteEnable1
SH.FMC_NBL1.ConfNb=1
SH.FMC_SDCLK.0=FMC_SDCLK,12b-sda1
SH.FMC_SDCLK.ConfNb=1
SH.FMC_SDNCAS.0=FMC_SDNCAS,12b-sda1
SH.FMC_SDNCAS.ConfNb=1
SH.FMC_SDNRAS.0=FMC_SDNRAS,12b-sda1
SH.FMC_SDNRAS.ConfNb=1
SH.FMC_SDNWE.0=FMC_SDNWE,12b-sda1
SH.FMC_SDNWE.ConfNb=1
SH.GPXTI7.0=GPIO_EXTI7
SH.GPXTI7.ConfNb=1
SH.S_TIM2_CH4.0=TIM2_CH4,PWM Generation4 CH4
SH.S_TIM2_CH4.ConfNb=1
TIM2.AutoReloadPreload=TIM_AUTORELOAD_PRELOAD_ENABLE
TIM2.Channel-PWM\ Generation4\ CH4=TIM_CHANNEL_4
TIM2.IPParameters=Prescaler,Period,AutoReloadPreload,Channel-PWM Generation4 CH4,Pulse-PWM Generation4 CH4
TIM2.Period=1000-1
TIM2.Prescaler=100-1
TIM2.Pulse-PWM\ Generation4\ CH4=500
USART1.IPParameters=VirtualMode-Asynchronous
USART1.VirtualMode-Asynchronous=VM_ASYNC
VP_CRC_VS_CRC.Mode=CRC_Activate
VP_CRC_VS_CRC.Signal=CRC_VS_CRC
VP_DMA2D_VS_DMA2D.Mode=DMA2D_Activate
VP_DMA2D_VS_DMA2D.Signal=DMA2D_VS_DMA2D
VP_SYS_VS_Systick.Mode=SysTick
VP_SYS_VS_Systick.Signal=SYS_VS_Systick
board=custom
