#

##

##

##

    µVision Build Log
    Tool Versions:
    IDE-Version: ¦ÌVision V5.15
    Copyright (C) 2015 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: sky Sky123.Org, Sky123.Org, LIC=P6F63-A5JSF-NTD3G-V0HZ9-EFB8I-J7I5M

    Tool Versions:
    Toolchain:       MDK-ARM Professional  Version: 5.15.0
    Toolchain Path:  D:\Keil_v515\ARM\ARMCC\Bin
    C Compiler:      Armcc.exe V5.05 update 2 (build 169)
    Assembler:       Armasm.exe V5.05 update 2 (build 169)
    Linker/Locator:  ArmLink.exe V5.05 update 2 (build 169)
    Library Manager: ArmAr.exe V5.05 update 2 (build 169)
    Hex Converter:   FromElf.exe V5.05 update 2 (build 169)
    CPU DLL:         SARMCM3.DLL V5.15.0
    Dialog DLL:      DCM.DLL V1.13.2.0
    Target DLL:      UL2CM3.DLL V1.155.8.0
    Dialog DLL:      TCM.DLL V1.14.5.0

    Project:
    C:\Users\Administrator\Desktop\EVK407I-Demo\USB FS Examples\Project\USB_Host_Device_Examples\DRD\MDK-ARM\USB_Host_device.uvproj
    Project File Date:  09/07/2013

    Output:
    *** Using Compiler 'V5.05 update 2 (build 169)', folder: 'D:\Keil_v515\ARM\ARMCC\Bin'
    Build target 'Open407I'
    compiling stm324xg_eval_lcd.c...
    linking...
    Program Size: Code=39184 RO-data=10536 RW-data=740 ZI-data=11940
    FromELF: creating hex file...
    ".\STM324xG-EVAL\STM324xG-EVAL_FS.axf" - 0 Error(s), 0 Warning(s).