Static Call Graph - [.\STM324xG_EVAL\STM324xG_EVAL.axf]

# Static Call Graph for image .\STM324xG_EVAL\STM324xG_EVAL.axf

#<CALLGRAPH># ARM Linker, 5050169: Last Updated: Fri Mar 11 21:06:08 2016

### Maximum Stack Usage = 468 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

ethernet_input ⇒ ip_input ⇒ tcp_input ⇒ tcp_process ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(i.BusFault_Handler) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CRYP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f4xx.o(RESET)
  - ETH_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI15_10_IRQHandler from stm32f4xx_it.o(i.EXTI15_10_IRQHandler) referenced from startup_stm32f4xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - FPU_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - FSMC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(i.HardFault_Handler) referenced from startup_stm32f4xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(i.MemManage_Handler) referenced from startup_stm32f4xx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(i.NMI_Handler) referenced from startup_stm32f4xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(i.PendSV_Handler) referenced from startup_stm32f4xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - Reset_Handler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SDIO_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(i.SVC_Handler) referenced from startup_stm32f4xx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(i.SysTick_Handler) referenced from startup_stm32f4xx.o(RESET)
  - SystemInit from system_stm32f4xx.o(i.SystemInit) referenced from startup_stm32f4xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - UART4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - UART5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART6_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - UsageFault_Handler from stm32f4xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f4xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f4xx.o(.text)
  - _sputc from printf3.o(i._sputc) referenced from printf3.o(i.__0sprintf$3)
  - conn_err from httpserver.o(i.conn_err) referenced from httpserver.o(i.http_accept)
  - etharp_output from etharp.o(i.etharp_output) referenced from ethernetif.o(i.ethernetif_init)
  - ethernet_input from etharp.o(i.ethernet_input) referenced from netconf.o(i.LwIP_Init)
  - ethernetif_init from ethernetif.o(i.ethernetif_init) referenced from netconf.o(i.LwIP_Init)
  - http_accept from httpserver.o(i.http_accept) referenced from httpserver.o(i.IAP_httpd_init)
  - http_poll from httpserver.o(i.http_poll) referenced from httpserver.o(i.http_accept)
  - http_recv from httpserver.o(i.http_recv) referenced from httpserver.o(i.http_accept)
  - http_sent from httpserver.o(i.http_sent) referenced from httpserver.o(i.http_recv)
  - low_level_output from ethernetif.o(i.low_level_output) referenced from ethernetif.o(i.ethernetif_init)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)
  - tcp_accept_null from tcp.o(i.tcp_accept_null) referenced from tcp.o(i.tcp_listen_with_backlog)
  - tcp_recv_null from tcp.o(i.tcp_recv_null) referenced from tcp.o(i.tcp_alloc)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CRYP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> pbuf_copy
  - >> icmp_send_response
  - >> pbuf_copy_partial
  - >> ip_reass
  - >> ip_frag
  - >> ip_reass_free_complete_datagram
  - >> low_level_output
  - >> low_level_input
  - >> tcp_enqueue

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> ip_reass
  - >> tcp_alloc

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strcmp (Thumb, 28 bytes, Stack size 8 bytes, strcmp.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = strcmp
  [Called By]
  - >> fs_open

  memcmp (Thumb, 26 bytes, Stack size 12 bytes, memcmp.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = memcmp
  [Called By]
  - >> autoip_arp_reply

  strncmp (Thumb, 30 bytes, Stack size 12 bytes, strncmp.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = strncmp
  [Called By]
  - >> http_recv
  - >> Parse_Content_Length

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __decompress (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __decompress1 (Thumb, 86 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ETH_BSP_Config (Thumb, 134 bytes, Stack size 24 bytes, stm32f4x7_eth_bsp.o(i.ETH_BSP_Config))
  [Stack]

  - Max Depth = 288
  - Call Chain = ETH_BSP_Config ⇒ ETH_MACDMA_Config ⇒ ETH_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> SysTick_CLKSourceConfig
  - >> RCC_GetClocksFreq
  - >> Eth_Link_PHYITConfig
  - >> Eth_Link_EXTIConfig
  - >> ETH_MACDMA_Config
  - >> ETH_GPIO_Config
  - >> LCD_SetTextColor
  - >> LCD_GetFont
  - >> LCD_DisplayStringLine
  [Called By]
  - >> main

  ETH_CheckFrameReceived (Thumb, 96 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_CheckFrameReceived))
  [Called By]

  - >> main

  ETH_DMAReceptionCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_DMAReceptionCmd))
  [Called By]

  - >> ETH_Start

  ETH_DMARxDescChainInit (Thumb, 74 bytes, Stack size 20 bytes, stm32f4x7_eth.o(i.ETH_DMARxDescChainInit))
  [Stack]

  - Max Depth = 20
  - Call Chain = ETH_DMARxDescChainInit
  [Called By]
  - >> low_level_init

  ETH_DMATransmissionCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_DMATransmissionCmd))
  [Called By]

  - >> ETH_Start

  ETH_DMATxDescChainInit (Thumb, 62 bytes, Stack size 20 bytes, stm32f4x7_eth.o(i.ETH_DMATxDescChainInit))
  [Stack]

  - Max Depth = 20
  - Call Chain = ETH_DMATxDescChainInit
  [Called By]
  - >> low_level_init

  ETH_DMATxDescChecksumInsertionConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_DMATxDescChecksumInsertionConfig))
  [Called By]

  - >> low_level_init

  ETH_DeInit (Thumb, 24 bytes, Stack size 8 bytes, stm32f4x7_eth.o(i.ETH_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = ETH_DeInit
  [Calls]
  - >> RCC_AHB1PeriphResetCmd
  [Called By]
  - >> ETH_MACDMA_Config

  ETH_FlushTransmitFIFO (Thumb, 12 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_FlushTransmitFIFO))
  [Called By]

  - >> ETH_Start

  ETH_GetSoftwareResetStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_GetSoftwareResetStatus))
  [Called By]

  - >> ETH_MACDMA_Config

  ETH_Get_Received_Frame (Thumb, 42 bytes, Stack size 12 bytes, stm32f4x7_eth.o(i.ETH_Get_Received_Frame))
  [Stack]

  - Max Depth = 12
  - Call Chain = ETH_Get_Received_Frame
  [Called By]
  - >> low_level_input

  ETH_Init (Thumb, 520 bytes, Stack size 56 bytes, stm32f4x7_eth.o(i.ETH_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = ETH_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  - >> ETH_WritePHYRegister
  - >> ETH_ReadPHYRegister
  - >> ETH_Delay
  [Called By]
  - >> ETH_MACDMA_Config

  ETH_MACAddressConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_MACAddressConfig))
  [Called By]

  - >> low_level_init

  ETH_MACReceptionCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_MACReceptionCmd))
  [Called By]

  - >> ETH_Start

  ETH_MACTransmissionCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_MACTransmissionCmd))
  [Called By]

  - >> ETH_Start

  ETH_Prepare_Transmit_Descriptors (Thumb, 168 bytes, Stack size 20 bytes, stm32f4x7_eth.o(i.ETH_Prepare_Transmit_Descriptors))
  [Stack]

  - Max Depth = 20
  - Call Chain = ETH_Prepare_Transmit_Descriptors
  [Called By]
  - >> low_level_output

  ETH_ReadPHYRegister (Thumb, 80 bytes, Stack size 12 bytes, stm32f4x7_eth.o(i.ETH_ReadPHYRegister))
  [Stack]

  - Max Depth = 12
  - Call Chain = ETH_ReadPHYRegister
  [Called By]
  - >> ETH_Init
  - >> Eth_Link_PHYITConfig
  - >> Eth_Link_ITHandler

  ETH_SoftwareReset (Thumb, 12 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_SoftwareReset))
  [Called By]

  - >> ETH_MACDMA_Config

  ETH_Start (Thumb, 34 bytes, Stack size 4 bytes, stm32f4x7_eth.o(i.ETH_Start))
  [Stack]

  - Max Depth = 4
  - Call Chain = ETH_Start
  [Calls]
  - >> ETH_MACTransmissionCmd
  - >> ETH_MACReceptionCmd
  - >> ETH_FlushTransmitFIFO
  - >> ETH_DMATransmissionCmd
  - >> ETH_DMAReceptionCmd
  [Called By]
  - >> low_level_init

  ETH_StructInit (Thumb, 136 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_StructInit))
  [Called By]

  - >> ETH_MACDMA_Config

  ETH_WritePHYRegister (Thumb, 76 bytes, Stack size 16 bytes, stm32f4x7_eth.o(i.ETH_WritePHYRegister))
  [Stack]

  - Max Depth = 16
  - Call Chain = ETH_WritePHYRegister
  [Called By]
  - >> ETH_Init
  - >> Eth_Link_PHYITConfig

  EXTI15_10_IRQHandler (Thumb, 34 bytes, Stack size 8 bytes, stm32f4xx_it.o(i.EXTI15_10_IRQHandler))
  [Stack]

  - Max Depth = 72
  - Call Chain = EXTI15_10_IRQHandler ⇒ Eth_Link_ITHandler ⇒ LCD_DisplayStringLine ⇒ LCD_DisplayChar ⇒ LCD_DrawChar ⇒ LCD_SetCursor
  [Calls]
  - >> EXTI_GetITStatus
  - >> EXTI_ClearITPendingBit
  - >> Eth_Link_ITHandler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  EXTI_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_exti.o(i.EXTI_ClearITPendingBit))
  [Called By]

  - >> EXTI15_10_IRQHandler

  EXTI_GetITStatus (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_exti.o(i.EXTI_GetITStatus))
  [Called By]

  - >> EXTI15_10_IRQHandler

  EXTI_Init (Thumb, 108 bytes, Stack size 12 bytes, stm32f4xx_exti.o(i.EXTI_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = EXTI_Init
  [Called By]
  - >> Eth_Link_EXTIConfig
  - >> STM_EVAL_PBInit

  Eth_Link_EXTIConfig (Thumb, 110 bytes, Stack size 32 bytes, stm32f4x7_eth_bsp.o(i.Eth_Link_EXTIConfig))
  [Stack]

  - Max Depth = 52
  - Call Chain = Eth_Link_EXTIConfig ⇒ GPIO_Init
  [Calls]
  - >> SYSCFG_EXTILineConfig
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  - >> NVIC_PriorityGroupConfig
  - >> NVIC_Init
  - >> GPIO_Init
  - >> EXTI_Init
  [Called By]
  - >> ETH_BSP_Config

  Eth_Link_ITHandler (Thumb, 116 bytes, Stack size 8 bytes, stm32f4x7_eth_bsp.o(i.Eth_Link_ITHandler))
  [Stack]

  - Max Depth = 64
  - Call Chain = Eth_Link_ITHandler ⇒ LCD_DisplayStringLine ⇒ LCD_DisplayChar ⇒ LCD_DrawChar ⇒ LCD_SetCursor
  [Calls]
  - >> ETH_ReadPHYRegister
  - >> LCD_SetTextColor
  - >> LCD_GetFont
  - >> LCD_DisplayStringLine
  [Called By]
  - >> EXTI15_10_IRQHandler

  Eth_Link_PHYITConfig (Thumb, 54 bytes, Stack size 8 bytes, stm32f4x7_eth_bsp.o(i.Eth_Link_PHYITConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = Eth_Link_PHYITConfig ⇒ ETH_WritePHYRegister
  [Calls]
  - >> ETH_WritePHYRegister
  - >> ETH_ReadPHYRegister
  [Called By]
  - >> ETH_BSP_Config

  FLASH_EraseSector (Thumb, 104 bytes, Stack size 16 bytes, stm32f4xx_flash.o(i.FLASH_EraseSector))
  [Stack]

  - Max Depth = 24
  - Call Chain = FLASH_EraseSector ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_WaitForLastOperation
  [Called By]
  - >> FLASH_If_Erase

  FLASH_GetStatus (Thumb, 46 bytes, Stack size 0 bytes, stm32f4xx_flash.o(i.FLASH_GetStatus))
  [Called By]

  - >> FLASH_WaitForLastOperation

  FLASH_If_Erase (Thumb, 80 bytes, Stack size 8 bytes, flash_if.o(i.FLASH_If_Erase))
  [Stack]

  - Max Depth = 32
  - Call Chain = FLASH_If_Erase ⇒ FLASH_EraseSector ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_EraseSector
  [Called By]
  - >> http_recv

  FLASH_If_Init (Thumb, 4 bytes, Stack size 0 bytes, flash_if.o(i.FLASH_If_Init))
  [Calls]

  - >> FLASH_Unlock
  [Called By]
  - >> http_recv

  FLASH_If_Write (Thumb, 74 bytes, Stack size 24 bytes, flash_if.o(i.FLASH_If_Write))
  [Stack]

  - Max Depth = 48
  - Call Chain = FLASH_If_Write ⇒ FLASH_ProgramWord ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_ProgramWord
  [Called By]
  - >> IAP_HTTP_writedata

  FLASH_ProgramWord (Thumb, 56 bytes, Stack size 16 bytes, stm32f4xx_flash.o(i.FLASH_ProgramWord))
  [Stack]

  - Max Depth = 24
  - Call Chain = FLASH_ProgramWord ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_WaitForLastOperation
  [Called By]
  - >> FLASH_If_Write

  FLASH_Unlock (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_flash.o(i.FLASH_Unlock))
  [Called By]

  - >> FLASH_If_Init

  FLASH_WaitForLastOperation (Thumb, 30 bytes, Stack size 8 bytes, stm32f4xx_flash.o(i.FLASH_WaitForLastOperation))
  [Stack]

  - Max Depth = 8
  - Call Chain = FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_GetStatus
  [Called By]
  - >> FLASH_ProgramWord
  - >> FLASH_EraseSector

  FSMC_NORSRAMCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(i.FSMC_NORSRAMCmd))
  [Called By]

  - >> LCD_FSMCConfig

  FSMC_NORSRAMInit (Thumb, 200 bytes, Stack size 8 bytes, stm32f4xx_fsmc.o(i.FSMC_NORSRAMInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = FSMC_NORSRAMInit
  [Called By]
  - >> LCD_FSMCConfig

  GPIO_Init (Thumb, 162 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> Eth_Link_EXTIConfig
  - >> ETH_GPIO_Config
  - >> STM_EVAL_PBInit
  - >> STM_EVAL_LEDInit
  - >> LCD_CtrlLinesConfig

  GPIO_PinAFConfig (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(i.GPIO_PinAFConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = GPIO_PinAFConfig
  [Called By]
  - >> ETH_GPIO_Config
  - >> LCD_CtrlLinesConfig

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(i.GPIO_ReadInputDataBit))
  [Called By]

  - >> STM_EVAL_PBGetState

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  IAP_httpd_init (Thumb, 34 bytes, Stack size 8 bytes, httpserver.o(i.IAP_httpd_init))
  [Stack]

  - Max Depth = 372
  - Call Chain = IAP_httpd_init ⇒ tcp_new ⇒ tcp_alloc ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_new
  - >> tcp_listen_with_backlog
  - >> tcp_bind
  - >> tcp_accept
  [Called By]
  - >> main

  LCD_Clear (Thumb, 40 bytes, Stack size 12 bytes, stm324xg_eval_lcd.o(i.LCD_Clear))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_Clear ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_SetCursor
  [Called By]
  - >> LCD_LED_Init
  - >> http_recv

  LCD_CtrlLinesConfig (Thumb, 318 bytes, Stack size 16 bytes, stm324xg_eval_lcd.o(i.LCD_CtrlLinesConfig))
  [Stack]

  - Max Depth = 36
  - Call Chain = LCD_CtrlLinesConfig ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_AHB3PeriphClockCmd
  [Called By]
  - >> STM324xG_LCD_Init

  LCD_DisplayChar (Thumb, 26 bytes, Stack size 4 bytes, stm324xg_eval_lcd.o(i.LCD_DisplayChar))
  [Stack]

  - Max Depth = 36
  - Call Chain = LCD_DisplayChar ⇒ LCD_DrawChar ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_DrawChar
  [Called By]
  - >> LCD_DisplayStringLine

  LCD_DisplayStringLine (Thumb, 52 bytes, Stack size 20 bytes, stm324xg_eval_lcd.o(i.LCD_DisplayStringLine))
  [Stack]

  - Max Depth = 56
  - Call Chain = LCD_DisplayStringLine ⇒ LCD_DisplayChar ⇒ LCD_DrawChar ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_DisplayChar
  [Called By]
  - >> Eth_Link_ITHandler
  - >> LwIP_Init
  - >> ETH_BSP_Config
  - >> LCD_LED_Init
  - >> http_recv

  LCD_DrawChar (Thumb, 128 bytes, Stack size 28 bytes, stm324xg_eval_lcd.o(i.LCD_DrawChar))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_DrawChar ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_SetCursor
  [Called By]
  - >> LCD_DisplayChar

  LCD_FSMCConfig (Thumb, 78 bytes, Stack size 96 bytes, stm324xg_eval_lcd.o(i.LCD_FSMCConfig))
  [Stack]

  - Max Depth = 104
  - Call Chain = LCD_FSMCConfig ⇒ FSMC_NORSRAMInit
  [Calls]
  - >> FSMC_NORSRAMInit
  - >> FSMC_NORSRAMCmd
  [Called By]
  - >> STM324xG_LCD_Init

  LCD_GetFont (Thumb, 6 bytes, Stack size 0 bytes, stm324xg_eval_lcd.o(i.LCD_GetFont))
  [Called By]

  - >> Eth_Link_ITHandler
  - >> LwIP_Init
  - >> ETH_BSP_Config
  - >> LCD_LED_Init
  - >> http_recv

  LCD_LED_Init (Thumb, 114 bytes, Stack size 8 bytes, main.o(i.LCD_LED_Init))
  [Stack]

  - Max Depth = 144
  - Call Chain = LCD_LED_Init ⇒ STM324xG_LCD_Init ⇒ LCD_FSMCConfig ⇒ FSMC_NORSRAMInit
  [Calls]
  - >> STM_EVAL_LEDInit
  - >> STM324xG_LCD_Init
  - >> LCD_SetBackColor
  - >> LCD_SetTextColor
  - >> LCD_GetFont
  - >> LCD_DisplayStringLine
  - >> LCD_Clear
  [Called By]
  - >> main

  LCD_ReadReg (Thumb, 12 bytes, Stack size 0 bytes, stm324xg_eval_lcd.o(i.LCD_ReadReg))
  [Called By]

  - >> STM324xG_LCD_Init

  LCD_SetBackColor (Thumb, 12 bytes, Stack size 8 bytes, stm324xg_eval_lcd.o(i.LCD_SetBackColor))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_SetBackColor
  [Called By]
  - >> LCD_LED_Init

  LCD_SetCursor (Thumb, 58 bytes, Stack size 4 bytes, stm324xg_eval_lcd.o(i.LCD_SetCursor))
  [Stack]

  - Max Depth = 4
  - Call Chain = LCD_SetCursor
  [Calls]
  - >> LCD_WriteReg
  [Called By]
  - >> LCD_Clear
  - >> LCD_DrawChar

  LCD_SetTextColor (Thumb, 12 bytes, Stack size 8 bytes, stm324xg_eval_lcd.o(i.LCD_SetTextColor))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_SetTextColor
  [Called By]
  - >> Eth_Link_ITHandler
  - >> ETH_BSP_Config
  - >> LCD_LED_Init
  - >> http_recv

  LCD_WriteReg (Thumb, 12 bytes, Stack size 0 bytes, stm324xg_eval_lcd.o(i.LCD_WriteReg))
  [Called By]

  - >> STM324xG_LCD_Init
  - >> LCD_SetCursor

  LwIP_Init (Thumb, 136 bytes, Stack size 48 bytes, netconf.o(i.LwIP_Init))
  [Stack]

  - Max Depth = 444
  - Call Chain = LwIP_Init ⇒ netif_add ⇒ netif_set_addr ⇒ netif_set_ipaddr ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> netif_set_up
  - >> netif_set_default
  - >> netif_add
  - >> memp_init
  - >> mem_init
  - >> htonl
  - >> LCD_GetFont
  - >> LCD_DisplayStringLine
  - >> __2sprintf
  [Called By]
  - >> main

  LwIP_Periodic_Handle (Thumb, 50 bytes, Stack size 16 bytes, netconf.o(i.LwIP_Periodic_Handle))
  [Stack]

  - Max Depth = 348
  - Call Chain = LwIP_Periodic_Handle ⇒ tcp_tmr ⇒ tcp_fasttmr ⇒ tcp_recv_null ⇒ tcp_close ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_tmr
  - >> etharp_tmr
  [Called By]
  - >> main

  LwIP_Pkt_Handle (Thumb, 6 bytes, Stack size 0 bytes, netconf.o(i.LwIP_Pkt_Handle))
  [Stack]

  - Max Depth = 124
  - Call Chain = LwIP_Pkt_Handle ⇒ ethernetif_input ⇒ low_level_input ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ethernetif_input
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  NVIC_Init (Thumb, 96 bytes, Stack size 12 bytes, misc.o(i.NVIC_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = NVIC_Init
  [Called By]
  - >> Eth_Link_EXTIConfig
  - >> STM_EVAL_PBInit

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(i.NVIC_PriorityGroupConfig))
  [Called By]

  - >> Eth_Link_EXTIConfig

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RCC_AHB1PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_AHB1PeriphClockCmd))
  [Called By]

  - >> Eth_Link_EXTIConfig
  - >> ETH_MACDMA_Config
  - >> ETH_GPIO_Config
  - >> STM_EVAL_PBInit
  - >> STM_EVAL_LEDInit
  - >> LCD_CtrlLinesConfig

  RCC_AHB1PeriphResetCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_AHB1PeriphResetCmd))
  [Called By]

  - >> ETH_DeInit

  RCC_AHB3PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_AHB3PeriphClockCmd))
  [Called By]

  - >> LCD_CtrlLinesConfig

  RCC_APB2PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> Eth_Link_EXTIConfig
  - >> ETH_GPIO_Config
  - >> STM_EVAL_PBInit

  RCC_GetClocksFreq (Thumb, 132 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(i.RCC_GetClocksFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> ETH_Init
  - >> ETH_BSP_Config

  RCC_MCO1Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_MCO1Config))
  [Called By]

  - >> ETH_GPIO_Config

  STM324xG_LCD_Init (Thumb, 1154 bytes, Stack size 32 bytes, stm324xg_eval_lcd.o(i.STM324xG_LCD_Init))
  [Stack]

  - Max Depth = 136
  - Call Chain = STM324xG_LCD_Init ⇒ LCD_FSMCConfig ⇒ FSMC_NORSRAMInit
  [Calls]
  - >> delay_ms
  - >> LCD_WriteReg
  - >> LCD_ReadReg
  - >> LCD_FSMCConfig
  - >> LCD_CtrlLinesConfig
  [Called By]
  - >> LCD_LED_Init

  STM_EVAL_LEDInit (Thumb, 62 bytes, Stack size 16 bytes, stm324xg_eval.o(i.STM_EVAL_LEDInit))
  [Stack]

  - Max Depth = 36
  - Call Chain = STM_EVAL_LEDInit ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main
  - >> LCD_LED_Init

  STM_EVAL_LEDOn (Thumb, 16 bytes, Stack size 0 bytes, stm324xg_eval.o(i.STM_EVAL_LEDOn))
  [Called By]

  - >> main

  STM_EVAL_PBGetState (Thumb, 16 bytes, Stack size 0 bytes, stm324xg_eval.o(i.STM_EVAL_PBGetState))
  [Calls]

  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> main

  STM_EVAL_PBInit (Thumb, 156 bytes, Stack size 40 bytes, stm324xg_eval.o(i.STM_EVAL_PBInit))
  [Stack]

  - Max Depth = 60
  - Call Chain = STM_EVAL_PBInit ⇒ GPIO_Init
  [Calls]
  - >> SYSCFG_EXTILineConfig
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  - >> NVIC_Init
  - >> GPIO_Init
  - >> EXTI_Init
  [Called By]
  - >> main

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SYSCFG_ETH_MediaInterfaceConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_syscfg.o(i.SYSCFG_ETH_MediaInterfaceConfig))
  [Called By]

  - >> ETH_GPIO_Config

  SYSCFG_EXTILineConfig (Thumb, 42 bytes, Stack size 8 bytes, stm32f4xx_syscfg.o(i.SYSCFG_EXTILineConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = SYSCFG_EXTILineConfig
  [Called By]
  - >> Eth_Link_EXTIConfig
  - >> STM_EVAL_PBInit

  SysTick_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, misc.o(i.SysTick_CLKSourceConfig))
  [Called By]

  - >> ETH_BSP_Config

  SysTick_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SysTick_Handler))
  [Calls]

  - >> Time_Update
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  SystemInit (Thumb, 74 bytes, Stack size 8 bytes, system_stm32f4xx.o(i.SystemInit))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(.text)

  Time_Update (Thumb, 10 bytes, Stack size 0 bytes, main.o(i.Time_Update))
  [Called By]

  - >> SysTick_Handler

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  __0sprintf$3 (Thumb, 34 bytes, Stack size 24 bytes, printf3.o(i.__0sprintf$3), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf$3 (Thumb, 0 bytes, Stack size 24 bytes, printf3.o(i.__0sprintf$3), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printf3.o(i.__0sprintf$3))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> LwIP_Init
  - >> http_recv

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  autoip_arp_reply (Thumb, 158 bytes, Stack size 24 bytes, autoip.o(i.autoip_arp_reply))
  [Stack]

  - Max Depth = 156
  - Call Chain = autoip_arp_reply ⇒ autoip_arp_announce ⇒ etharp_raw ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> autoip_start
  - >> autoip_arp_announce
  - >> memcmp
  [Called By]
  - >> etharp_arp_input

  autoip_start (Thumb, 140 bytes, Stack size 24 bytes, autoip.o(i.autoip_start))
  [Stack]

  - Max Depth = 44
  - Call Chain = autoip_start ⇒ mem_malloc
  [Calls]
  - >> htonl
  - >> mem_malloc
  - >> ntohl
  - >> netif_set_down
  - >> netif_is_up
  - >> autoip_start_probing
  [Called By]
  - >> autoip_arp_reply

  delay_ms (Thumb, 28 bytes, Stack size 0 bytes, stm324xg_eval_lcd.o(i.delay_ms))
  [Called By]

  - >> STM324xG_LCD_Init

  etharp_arp_input (Thumb, 234 bytes, Stack size 32 bytes, etharp.o(i.etharp_arp_input))
  [Stack]

  - Max Depth = 188
  - Call Chain = etharp_arp_input ⇒ autoip_arp_reply ⇒ autoip_arp_announce ⇒ etharp_raw ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> autoip_arp_reply
  - >> htons
  - >> update_arp_entry
  [Called By]
  - >> ethernet_input

  etharp_ip_input (Thumb, 44 bytes, Stack size 8 bytes, etharp.o(i.etharp_ip_input))
  [Stack]

  - Max Depth = 132
  - Call Chain = etharp_ip_input ⇒ update_arp_entry ⇒ find_entry ⇒ free_etharp_q ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> update_arp_entry
  [Called By]
  - >> ethernet_input

  etharp_output (Thumb, 178 bytes, Stack size 32 bytes, etharp.o(i.etharp_output))
  [Stack]

  - Max Depth = 204
  - Call Chain = etharp_output ⇒ etharp_query ⇒ etharp_request ⇒ etharp_raw ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ip_addr_isbroadcast
  - >> ntohl
  - >> pbuf_header
  - >> etharp_query
  - >> etharp_send_ip
  [Address Reference Count : 1]
  - ethernetif.o(i.ethernetif_init)

  etharp_query (Thumb, 252 bytes, Stack size 40 bytes, etharp.o(i.etharp_query))
  [Stack]

  - Max Depth = 172
  - Call Chain = etharp_query ⇒ etharp_request ⇒ etharp_raw ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> etharp_request
  - >> pbuf_copy
  - >> ip_addr_isbroadcast
  - >> ntohl
  - >> pbuf_alloc
  - >> memp_malloc
  - >> find_entry
  - >> etharp_send_ip
  - >> pbuf_ref
  [Called By]
  - >> etharp_output

  etharp_raw (Thumb, 178 bytes, Stack size 40 bytes, etharp.o(i.etharp_raw))
  [Stack]

  - Max Depth = 108
  - Call Chain = etharp_raw ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> pbuf_alloc
  - >> htons
  [Called By]
  - >> etharp_request
  - >> autoip_arp_announce

  etharp_request (Thumb, 32 bytes, Stack size 24 bytes, etharp.o(i.etharp_request))
  [Stack]

  - Max Depth = 132
  - Call Chain = etharp_request ⇒ etharp_raw ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> etharp_raw
  [Called By]
  - >> netif_set_up
  - >> etharp_query

  etharp_tmr (Thumb, 80 bytes, Stack size 24 bytes, etharp.o(i.etharp_tmr))
  [Stack]

  - Max Depth = 68
  - Call Chain = etharp_tmr ⇒ free_etharp_q ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> free_etharp_q
  [Called By]
  - >> LwIP_Periodic_Handle

  ethernet_input (Thumb, 84 bytes, Stack size 16 bytes, etharp.o(i.ethernet_input))
  [Stack]

  - Max Depth = 468
  - Call Chain = ethernet_input ⇒ ip_input ⇒ tcp_input ⇒ tcp_process ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> ip_input
  - >> pbuf_header
  - >> htons
  - >> etharp_ip_input
  - >> etharp_arp_input
  [Address Reference Count : 1]
  - netconf.o(i.LwIP_Init)

  ethernetif_init (Thumb, 30 bytes, Stack size 8 bytes, ethernetif.o(i.ethernetif_init))
  [Stack]

  - Max Depth = 44
  - Call Chain = ethernetif_init ⇒ low_level_init ⇒ ETH_DMATxDescChainInit
  [Calls]
  - >> low_level_init
  [Address Reference Count : 1]
  - netconf.o(i.LwIP_Init)

  ethernetif_input (Thumb, 38 bytes, Stack size 16 bytes, ethernetif.o(i.ethernetif_input))
  [Stack]

  - Max Depth = 124
  - Call Chain = ethernetif_input ⇒ low_level_input ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> low_level_input
  [Called By]
  - >> LwIP_Pkt_Handle

  htonl (Thumb, 4 bytes, Stack size 0 bytes, inet.o(i.htonl))
  [Called By]

  - >> LwIP_Init
  - >> autoip_start
  - >> tcp_output_set_header
  - >> tcp_output_segment
  - >> tcp_send_empty_ack
  - >> tcp_rst
  - >> tcp_keepalive
  - >> tcp_enqueue

  htons (Thumb, 4 bytes, Stack size 0 bytes, inet.o(i.htons))
  [Called By]

  - >> ethernet_input
  - >> ip_input
  - >> lwip_standard_chksum
  - >> ip_output_if
  - >> icmp_input
  - >> etharp_raw
  - >> ip_reass
  - >> ip_frag
  - >> etharp_arp_input
  - >> etharp_send_ip
  - >> tcp_output_set_header
  - >> tcp_output_segment
  - >> tcp_receive
  - >> tcp_zero_window_probe
  - >> tcp_rst
  - >> tcp_output
  - >> tcp_enqueue

  icmp_dest_unreach (Thumb, 8 bytes, Stack size 0 bytes, icmp.o(i.icmp_dest_unreach))
  [Stack]

  - Max Depth = 252
  - Call Chain = icmp_dest_unreach ⇒ icmp_send_response ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> icmp_send_response
  [Called By]
  - >> udp_input
  - >> ip_input

  icmp_input (Thumb, 276 bytes, Stack size 48 bytes, icmp.o(i.icmp_input))
  [Stack]

  - Max Depth = 220
  - Call Chain = icmp_input ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> pbuf_copy
  - >> ip_output_if
  - >> ip_addr_isbroadcast
  - >> inet_chksum_pbuf
  - >> ntohl
  - >> pbuf_header
  - >> pbuf_alloc
  - >> ntohs
  - >> htons
  [Called By]
  - >> ip_input

  icmp_time_exceeded (Thumb, 8 bytes, Stack size 0 bytes, icmp.o(i.icmp_time_exceeded))
  [Stack]

  - Max Depth = 252
  - Call Chain = icmp_time_exceeded ⇒ icmp_send_response ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> icmp_send_response
  [Called By]
  - >> ip_reass_free_complete_datagram

  inet_chksum (Thumb, 12 bytes, Stack size 8 bytes, inet_chksum.o(i.inet_chksum))
  [Stack]

  - Max Depth = 16
  - Call Chain = inet_chksum ⇒ lwip_standard_chksum
  [Calls]
  - >> lwip_standard_chksum
  [Called By]
  - >> icmp_send_response
  - >> ip_reass
  - >> ip_frag

  inet_chksum_pbuf (Thumb, 72 bytes, Stack size 16 bytes, inet_chksum.o(i.inet_chksum_pbuf))
  [Stack]

  - Max Depth = 24
  - Call Chain = inet_chksum_pbuf ⇒ lwip_standard_chksum
  [Calls]
  - >> lwip_standard_chksum
  [Called By]
  - >> icmp_input

  ip_addr_isbroadcast (Thumb, 48 bytes, Stack size 0 bytes, ip_addr.o(i.ip_addr_isbroadcast))
  [Called By]

  - >> udp_input
  - >> tcp_input
  - >> ip_input
  - >> icmp_input
  - >> etharp_query
  - >> etharp_output
  - >> update_arp_entry

  ip_frag (Thumb, 294 bytes, Stack size 64 bytes, ip_frag.o(i.ip_frag))
  [Stack]

  - Max Depth = 132
  - Call Chain = ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> pbuf_realloc
  - >> pbuf_copy_partial
  - >> pbuf_chain
  - >> pbuf_alloc
  - >> ntohs
  - >> inet_chksum
  - >> htons
  - >> __aeabi_memcpy
  [Called By]
  - >> ip_output_if

  ip_input (Thumb, 348 bytes, Stack size 32 bytes, ip.o(i.ip_input))
  [Stack]

  - Max Depth = 452
  - Call Chain = ip_input ⇒ tcp_input ⇒ tcp_process ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> udp_input
  - >> tcp_input
  - >> raw_input
  - >> ip_addr_isbroadcast
  - >> icmp_input
  - >> icmp_dest_unreach
  - >> ntohl
  - >> netif_is_up
  - >> pbuf_realloc
  - >> ntohs
  - >> htons
  - >> ip_reass
  [Called By]
  - >> ethernet_input

  ip_output (Thumb, 52 bytes, Stack size 40 bytes, ip.o(i.ip_output))
  [Stack]

  - Max Depth = 212
  - Call Chain = ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ip_route
  - >> ip_output_if
  [Called By]
  - >> icmp_send_response
  - >> tcp_output_segment
  - >> tcp_send_empty_ack
  - >> tcp_zero_window_probe
  - >> tcp_rst
  - >> tcp_keepalive

  ip_output_if (Thumb, 200 bytes, Stack size 40 bytes, ip.o(i.ip_output_if))
  [Stack]

  - Max Depth = 172
  - Call Chain = ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_header
  - >> ntohs
  - >> htons
  - >> ip_frag
  [Called By]
  - >> ip_output
  - >> icmp_input

  ip_reass (Thumb, 406 bytes, Stack size 40 bytes, ip_frag.o(i.ip_reass))
  [Stack]

  - Max Depth = 340
  - Call Chain = ip_reass ⇒ ip_reass_remove_oldest_datagram ⇒ ip_reass_free_complete_datagram ⇒ icmp_time_exceeded ⇒ icmp_send_response ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> pbuf_header
  - >> pbuf_clen
  - >> pbuf_cat
  - >> ntohs
  - >> memp_malloc
  - >> inet_chksum
  - >> htons
  - >> ip_reass_remove_oldest_datagram
  - >> ip_reass_dequeue_datagram
  - >> ip_reass_chain_frag_into_datagram_and_validate
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy
  [Called By]
  - >> ip_input

  ip_route (Thumb, 62 bytes, Stack size 16 bytes, ip.o(i.ip_route))
  [Stack]

  - Max Depth = 16
  - Call Chain = ip_route
  [Calls]
  - >> netif_is_up
  [Called By]
  - >> ip_output
  - >> tcp_output_segment
  - >> tcp_eff_send_mss

  main (Thumb, 102 bytes, Stack size 8 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 452
  - Call Chain = main ⇒ LwIP_Init ⇒ netif_add ⇒ netif_set_addr ⇒ netif_set_ipaddr ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> STM_EVAL_PBInit
  - >> STM_EVAL_PBGetState
  - >> STM_EVAL_LEDOn
  - >> STM_EVAL_LEDInit
  - >> LwIP_Pkt_Handle
  - >> LwIP_Periodic_Handle
  - >> LwIP_Init
  - >> ETH_CheckFrameReceived
  - >> ETH_BSP_Config
  - >> LCD_LED_Init
  - >> IAP_httpd_init
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  mem_free (Thumb, 40 bytes, Stack size 0 bytes, mem.o(i.mem_free))
  [Stack]

  - Max Depth = 12
  - Call Chain = mem_free ⇒ plug_holes
  [Calls]
  - >> plug_holes
  [Called By]
  - >> pbuf_free
  - >> conn_err
  - >> close_conn

  mem_init (Thumb, 44 bytes, Stack size 8 bytes, mem.o(i.mem_init))
  [Stack]

  - Max Depth = 8
  - Call Chain = mem_init
  [Called By]
  - >> LwIP_Init

  mem_malloc (Thumb, 164 bytes, Stack size 20 bytes, mem.o(i.mem_malloc))
  [Stack]

  - Max Depth = 20
  - Call Chain = mem_malloc
  [Called By]
  - >> http_accept
  - >> autoip_start
  - >> pbuf_alloc

  mem_realloc (Thumb, 190 bytes, Stack size 36 bytes, mem.o(i.mem_realloc))
  [Stack]

  - Max Depth = 36
  - Call Chain = mem_realloc
  [Called By]
  - >> pbuf_realloc

  memp_free (Thumb, 18 bytes, Stack size 0 bytes, memp.o(i.memp_free))
  [Called By]

  - >> tcp_listen_with_backlog
  - >> tcp_close
  - >> pbuf_free
  - >> tcp_abandon
  - >> tcp_input
  - >> ip_reass_dequeue_datagram
  - >> update_arp_entry
  - >> free_etharp_q
  - >> tcp_enqueue
  - >> tcp_slowtmr
  - >> tcp_seg_free

  memp_init (Thumb, 78 bytes, Stack size 20 bytes, memp.o(i.memp_init))
  [Stack]

  - Max Depth = 20
  - Call Chain = memp_init
  [Called By]
  - >> LwIP_Init

  memp_malloc (Thumb, 28 bytes, Stack size 0 bytes, memp.o(i.memp_malloc))
  [Called By]

  - >> tcp_listen_with_backlog
  - >> pbuf_alloc
  - >> ip_reass
  - >> etharp_query
  - >> tcp_enqueue
  - >> tcp_alloc

  netif_add (Thumb, 70 bytes, Stack size 24 bytes, netif.o(i.netif_add))
  [Stack]

  - Max Depth = 396
  - Call Chain = netif_add ⇒ netif_set_addr ⇒ netif_set_ipaddr ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> netif_set_addr
  [Called By]
  - >> LwIP_Init

  netif_is_up (Thumb, 10 bytes, Stack size 0 bytes, netif.o(i.netif_is_up))
  [Called By]

  - >> ip_route
  - >> ip_input
  - >> autoip_start

  netif_set_addr (Thumb, 32 bytes, Stack size 16 bytes, netif.o(i.netif_set_addr))
  [Stack]

  - Max Depth = 372
  - Call Chain = netif_set_addr ⇒ netif_set_ipaddr ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> netif_set_netmask
  - >> netif_set_ipaddr
  - >> netif_set_gw
  [Called By]
  - >> netif_add

  netif_set_default (Thumb, 6 bytes, Stack size 0 bytes, netif.o(i.netif_set_default))
  [Called By]

  - >> LwIP_Init

  netif_set_down (Thumb, 18 bytes, Stack size 0 bytes, netif.o(i.netif_set_down))
  [Called By]

  - >> autoip_start

  netif_set_gw (Thumb, 8 bytes, Stack size 0 bytes, netif.o(i.netif_set_gw))
  [Called By]

  - >> netif_set_addr

  netif_set_ipaddr (Thumb, 96 bytes, Stack size 16 bytes, netif.o(i.netif_set_ipaddr))
  [Stack]

  - Max Depth = 356
  - Call Chain = netif_set_ipaddr ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_abandon
  [Called By]
  - >> netif_set_addr

  netif_set_netmask (Thumb, 8 bytes, Stack size 0 bytes, netif.o(i.netif_set_netmask))
  [Called By]

  - >> netif_set_addr

  netif_set_up (Thumb, 28 bytes, Stack size 0 bytes, netif.o(i.netif_set_up))
  [Stack]

  - Max Depth = 132
  - Call Chain = netif_set_up ⇒ etharp_request ⇒ etharp_raw ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> etharp_request
  [Called By]
  - >> LwIP_Init

  ntohl (Thumb, 4 bytes, Stack size 0 bytes, inet.o(i.ntohl))
  [Called By]

  - >> udp_input
  - >> tcp_input
  - >> ip_input
  - >> icmp_input
  - >> autoip_start
  - >> etharp_query
  - >> etharp_output
  - >> update_arp_entry
  - >> tcp_output_segment
  - >> tcp_rexmit
  - >> tcp_receive
  - >> tcp_process
  - >> tcp_output
  - >> tcp_enqueue

  ntohs (Thumb, 4 bytes, Stack size 0 bytes, inet.o(i.ntohs))
  [Called By]

  - >> udp_input
  - >> tcp_input
  - >> raw_input
  - >> ip_input
  - >> ip_output_if
  - >> icmp_input
  - >> ip_reass
  - >> ip_frag
  - >> ip_reass_chain_frag_into_datagram_and_validate
  - >> tcp_output_set_header
  - >> tcp_receive
  - >> tcp_parseopt
  - >> tcp_zero_window_probe
  - >> tcp_rst
  - >> tcp_output
  - >> tcp_enqueue

  pbuf_alloc (Thumb, 272 bytes, Stack size 40 bytes, pbuf.o(i.pbuf_alloc))
  [Stack]

  - Max Depth = 68
  - Call Chain = pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> mem_malloc
  - >> memp_malloc
  [Called By]
  - >> icmp_input
  - >> icmp_send_response
  - >> etharp_raw
  - >> ip_frag
  - >> low_level_input
  - >> etharp_query
  - >> tcp_send_empty_ack
  - >> tcp_zero_window_probe
  - >> tcp_rst
  - >> tcp_keepalive
  - >> tcp_enqueue

  pbuf_cat (Thumb, 40 bytes, Stack size 8 bytes, pbuf.o(i.pbuf_cat))
  [Stack]

  - Max Depth = 8
  - Call Chain = pbuf_cat
  [Called By]
  - >> pbuf_chain
  - >> ip_reass
  - >> tcp_enqueue

  pbuf_chain (Thumb, 18 bytes, Stack size 8 bytes, pbuf.o(i.pbuf_chain))
  [Stack]

  - Max Depth = 16
  - Call Chain = pbuf_chain ⇒ pbuf_cat
  [Calls]
  - >> pbuf_cat
  - >> pbuf_ref
  [Called By]
  - >> ip_frag

  pbuf_clen (Thumb, 18 bytes, Stack size 0 bytes, pbuf.o(i.pbuf_clen))
  [Called By]

  - >> ip_reass
  - >> ip_reass_free_complete_datagram
  - >> ip_reass_chain_frag_into_datagram_and_validate
  - >> tcp_receive
  - >> tcp_enqueue

  pbuf_copy (Thumb, 144 bytes, Stack size 32 bytes, pbuf.o(i.pbuf_copy))
  [Stack]

  - Max Depth = 32
  - Call Chain = pbuf_copy
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> icmp_input
  - >> etharp_query

  pbuf_copy_partial (Thumb, 104 bytes, Stack size 32 bytes, pbuf.o(i.pbuf_copy_partial))
  [Stack]

  - Max Depth = 32
  - Call Chain = pbuf_copy_partial
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> ip_frag

  pbuf_free (Thumb, 68 bytes, Stack size 16 bytes, pbuf.o(i.pbuf_free))
  [Stack]

  - Max Depth = 28
  - Call Chain = pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> mem_free
  - >> memp_free
  [Called By]
  - >> ethernetif_input
  - >> ethernet_input
  - >> http_recv
  - >> udp_input
  - >> tcp_input
  - >> ip_input
  - >> icmp_input
  - >> icmp_send_response
  - >> etharp_raw
  - >> pbuf_realloc
  - >> pbuf_alloc
  - >> ip_reass
  - >> ip_frag
  - >> ip_reass_free_complete_datagram
  - >> ip_reass_chain_frag_into_datagram_and_validate
  - >> etharp_query
  - >> etharp_arp_input
  - >> update_arp_entry
  - >> free_etharp_q
  - >> tcp_send_empty_ack
  - >> tcp_zero_window_probe
  - >> tcp_rst
  - >> tcp_keepalive
  - >> tcp_enqueue
  - >> tcp_seg_free
  - >> tcp_recv_null
  - >> tcp_pcb_purge

  pbuf_header (Thumb, 96 bytes, Stack size 8 bytes, pbuf.o(i.pbuf_header))
  [Stack]

  - Max Depth = 8
  - Call Chain = pbuf_header
  [Called By]
  - >> ethernet_input
  - >> udp_input
  - >> tcp_input
  - >> ip_output_if
  - >> icmp_input
  - >> ip_reass
  - >> etharp_output
  - >> tcp_receive
  - >> tcp_enqueue

  pbuf_realloc (Thumb, 78 bytes, Stack size 16 bytes, pbuf.o(i.pbuf_realloc))
  [Stack]

  - Max Depth = 52
  - Call Chain = pbuf_realloc ⇒ mem_realloc
  [Calls]
  - >> pbuf_free
  - >> mem_realloc
  [Called By]
  - >> ip_input
  - >> ip_frag
  - >> tcp_receive

  pbuf_ref (Thumb, 12 bytes, Stack size 0 bytes, pbuf.o(i.pbuf_ref))
  [Called By]

  - >> pbuf_chain
  - >> etharp_query

  raw_input (Thumb, 100 bytes, Stack size 32 bytes, raw.o(i.raw_input))
  [Stack]

  - Max Depth = 32
  - Call Chain = raw_input
  [Calls]
  - >> ntohs
  [Called By]
  - >> ip_input

  tcp_abandon (Thumb, 144 bytes, Stack size 56 bytes, tcp.o(i.tcp_abandon))
  [Stack]

  - Max Depth = 340
  - Call Chain = tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> memp_free
  - >> tcp_rst
  - >> tcp_segs_free
  - >> tcp_pcb_remove
  [Called By]
  - >> netif_set_ipaddr
  - >> tcp_process
  - >> tcp_listen_input
  - >> tcp_alloc

  tcp_accept (Thumb, 4 bytes, Stack size 0 bytes, tcp.o(i.tcp_accept))
  [Called By]

  - >> IAP_httpd_init

  tcp_alloc (Thumb, 250 bytes, Stack size 24 bytes, tcp.o(i.tcp_alloc))
  [Stack]

  - Max Depth = 364
  - Call Chain = tcp_alloc ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_abandon
  - >> memp_malloc
  - >> tcp_next_iss
  - >> __aeabi_memclr4
  [Called By]
  - >> tcp_new
  - >> tcp_listen_input

  tcp_arg (Thumb, 4 bytes, Stack size 0 bytes, tcp.o(i.tcp_arg))
  [Called By]

  - >> http_accept
  - >> close_conn

  tcp_bind (Thumb, 182 bytes, Stack size 24 bytes, tcp.o(i.tcp_bind))
  [Stack]

  - Max Depth = 44
  - Call Chain = tcp_bind ⇒ tcp_new_port
  [Calls]
  - >> tcp_new_port
  [Called By]
  - >> IAP_httpd_init

  tcp_close (Thumb, 152 bytes, Stack size 16 bytes, tcp.o(i.tcp_close))
  [Stack]

  - Max Depth = 300
  - Call Chain = tcp_close ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> memp_free
  - >> tcp_send_ctrl
  - >> tcp_output
  - >> tcp_pcb_remove
  [Called By]
  - >> http_poll
  - >> close_conn
  - >> tcp_recv_null

  tcp_eff_send_mss (Thumb, 32 bytes, Stack size 8 bytes, tcp.o(i.tcp_eff_send_mss))
  [Stack]

  - Max Depth = 24
  - Call Chain = tcp_eff_send_mss ⇒ ip_route
  [Calls]
  - >> ip_route
  [Called By]
  - >> tcp_process
  - >> tcp_listen_input

  tcp_enqueue (Thumb, 830 bytes, Stack size 96 bytes, tcp_out.o(i.tcp_enqueue))
  [Stack]

  - Max Depth = 164
  - Call Chain = tcp_enqueue ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> htonl
  - >> pbuf_free
  - >> ntohl
  - >> pbuf_header
  - >> pbuf_clen
  - >> pbuf_cat
  - >> pbuf_alloc
  - >> ntohs
  - >> memp_malloc
  - >> memp_free
  - >> htons
  - >> tcp_segs_free
  - >> __aeabi_memcpy
  [Called By]
  - >> tcp_write
  - >> tcp_listen_input
  - >> tcp_send_ctrl

  tcp_err (Thumb, 6 bytes, Stack size 0 bytes, tcp.o(i.tcp_err))
  [Called By]

  - >> http_accept

  tcp_fasttmr (Thumb, 86 bytes, Stack size 16 bytes, tcp.o(i.tcp_fasttmr))
  [Stack]

  - Max Depth = 324
  - Call Chain = tcp_fasttmr ⇒ tcp_recv_null ⇒ tcp_close ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_output
  - >> tcp_recv_null
  [Called By]
  - >> tcp_tmr

  tcp_input (Thumb, 732 bytes, Stack size 32 bytes, tcp_in.o(i.tcp_input))
  [Stack]

  - Max Depth = 420
  - Call Chain = tcp_input ⇒ tcp_process ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> ip_addr_isbroadcast
  - >> ntohl
  - >> pbuf_header
  - >> ntohs
  - >> memp_free
  - >> tcp_timewait_input
  - >> tcp_process
  - >> tcp_listen_input
  - >> tcp_rst
  - >> tcp_output
  - >> tcp_recv_null
  - >> tcp_pcb_remove
  [Called By]
  - >> ip_input

  tcp_keepalive (Thumb, 70 bytes, Stack size 24 bytes, tcp_out.o(i.tcp_keepalive))
  [Stack]

  - Max Depth = 236
  - Call Chain = tcp_keepalive ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> htonl
  - >> pbuf_free
  - >> ip_output
  - >> pbuf_alloc
  - >> tcp_output_set_header
  [Called By]
  - >> tcp_slowtmr

  tcp_listen_with_backlog (Thumb, 118 bytes, Stack size 16 bytes, tcp.o(i.tcp_listen_with_backlog))
  [Stack]

  - Max Depth = 16
  - Call Chain = tcp_listen_with_backlog
  [Calls]
  - >> memp_malloc
  - >> memp_free
  [Called By]
  - >> IAP_httpd_init

  tcp_new (Thumb, 6 bytes, Stack size 0 bytes, tcp.o(i.tcp_new))
  [Stack]

  - Max Depth = 364
  - Call Chain = tcp_new ⇒ tcp_alloc ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_alloc
  [Called By]
  - >> IAP_httpd_init

  tcp_next_iss (Thumb, 12 bytes, Stack size 0 bytes, tcp.o(i.tcp_next_iss))
  [Called By]

  - >> tcp_alloc

  tcp_output (Thumb, 424 bytes, Stack size 32 bytes, tcp_out.o(i.tcp_output))
  [Stack]

  - Max Depth = 268
  - Call Chain = tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ntohl
  - >> ntohs
  - >> htons
  - >> tcp_output_segment
  - >> tcp_send_empty_ack
  - >> tcp_seg_free
  [Called By]
  - >> tcp_recved
  - >> tcp_close
  - >> tcp_input
  - >> tcp_timewait_input
  - >> tcp_receive
  - >> tcp_process
  - >> tcp_listen_input
  - >> tcp_rexmit_rto
  - >> tcp_slowtmr
  - >> tcp_pcb_remove
  - >> tcp_fasttmr

  tcp_pcb_purge (Thumb, 48 bytes, Stack size 16 bytes, tcp.o(i.tcp_pcb_purge))
  [Stack]

  - Max Depth = 76
  - Call Chain = tcp_pcb_purge ⇒ tcp_segs_free ⇒ tcp_seg_free ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> tcp_segs_free
  [Called By]
  - >> tcp_process
  - >> tcp_slowtmr
  - >> tcp_pcb_remove

  tcp_pcb_remove (Thumb, 86 bytes, Stack size 16 bytes, tcp.o(i.tcp_pcb_remove))
  [Stack]

  - Max Depth = 284
  - Call Chain = tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_output
  - >> tcp_pcb_purge
  [Called By]
  - >> tcp_close
  - >> tcp_abandon
  - >> tcp_input

  tcp_poll (Thumb, 10 bytes, Stack size 0 bytes, tcp.o(i.tcp_poll))
  [Called By]

  - >> http_accept

  tcp_recv (Thumb, 6 bytes, Stack size 0 bytes, tcp.o(i.tcp_recv))
  [Called By]

  - >> http_accept
  - >> close_conn

  tcp_recv_null (Thumb, 36 bytes, Stack size 8 bytes, tcp.o(i.tcp_recv_null))
  [Stack]

  - Max Depth = 308
  - Call Chain = tcp_recv_null ⇒ tcp_close ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_recved
  - >> tcp_close
  - >> pbuf_free
  [Called By]
  - >> tcp_input
  - >> tcp_fasttmr
  [Address Reference Count : 1]
  - tcp.o(i.tcp_alloc)

  tcp_recved (Thumb, 60 bytes, Stack size 8 bytes, tcp.o(i.tcp_recved))
  [Stack]

  - Max Depth = 276
  - Call Chain = tcp_recved ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_output
  - >> tcp_update_rcv_ann_wnd
  [Called By]
  - >> http_recv
  - >> tcp_recv_null

  tcp_rexmit (Thumb, 74 bytes, Stack size 24 bytes, tcp_out.o(i.tcp_rexmit))
  [Stack]

  - Max Depth = 24
  - Call Chain = tcp_rexmit
  [Calls]
  - >> ntohl
  [Called By]
  - >> tcp_rexmit_fast
  - >> tcp_process

  tcp_rexmit_fast (Thumb, 92 bytes, Stack size 8 bytes, tcp_out.o(i.tcp_rexmit_fast))
  [Stack]

  - Max Depth = 32
  - Call Chain = tcp_rexmit_fast ⇒ tcp_rexmit
  [Calls]
  - >> tcp_rexmit
  [Called By]
  - >> tcp_receive

  tcp_rexmit_rto (Thumb, 46 bytes, Stack size 0 bytes, tcp_out.o(i.tcp_rexmit_rto))
  [Stack]

  - Max Depth = 268
  - Call Chain = tcp_rexmit_rto ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_output
  [Called By]
  - >> tcp_slowtmr

  tcp_rst (Thumb, 156 bytes, Stack size 48 bytes, tcp_out.o(i.tcp_rst))
  [Stack]

  - Max Depth = 260
  - Call Chain = tcp_rst ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> htonl
  - >> pbuf_free
  - >> ip_output
  - >> pbuf_alloc
  - >> ntohs
  - >> htons
  [Called By]
  - >> tcp_abandon
  - >> tcp_input
  - >> tcp_timewait_input
  - >> tcp_process
  - >> tcp_listen_input
  - >> tcp_slowtmr

  tcp_seg_free (Thumb, 32 bytes, Stack size 16 bytes, tcp.o(i.tcp_seg_free))
  [Stack]

  - Max Depth = 44
  - Call Chain = tcp_seg_free ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> memp_free
  [Called By]
  - >> tcp_receive
  - >> tcp_process
  - >> tcp_output
  - >> tcp_segs_free

  tcp_segs_free (Thumb, 26 bytes, Stack size 16 bytes, tcp.o(i.tcp_segs_free))
  [Stack]

  - Max Depth = 60
  - Call Chain = tcp_segs_free ⇒ tcp_seg_free ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_seg_free
  [Called By]
  - >> tcp_abandon
  - >> tcp_enqueue
  - >> tcp_pcb_purge

  tcp_send_ctrl (Thumb, 22 bytes, Stack size 16 bytes, tcp_out.o(i.tcp_send_ctrl))
  [Stack]

  - Max Depth = 180
  - Call Chain = tcp_send_ctrl ⇒ tcp_enqueue ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_enqueue
  [Called By]
  - >> tcp_close

  tcp_send_empty_ack (Thumb, 86 bytes, Stack size 24 bytes, tcp_out.o(i.tcp_send_empty_ack))
  [Stack]

  - Max Depth = 236
  - Call Chain = tcp_send_empty_ack ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> htonl
  - >> pbuf_free
  - >> ip_output
  - >> pbuf_alloc
  - >> tcp_output_set_header
  [Called By]
  - >> tcp_receive
  - >> tcp_output

  tcp_sent (Thumb, 6 bytes, Stack size 0 bytes, tcp.o(i.tcp_sent))
  [Called By]

  - >> http_recv
  - >> close_conn

  tcp_slowtmr (Thumb, 540 bytes, Stack size 40 bytes, tcp.o(i.tcp_slowtmr))
  [Stack]

  - Max Depth = 308
  - Call Chain = tcp_slowtmr ⇒ tcp_rexmit_rto ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> memp_free
  - >> tcp_zero_window_probe
  - >> tcp_rst
  - >> tcp_rexmit_rto
  - >> tcp_output
  - >> tcp_keepalive
  - >> tcp_pcb_purge
  [Called By]
  - >> tcp_tmr

  tcp_tmr (Thumb, 28 bytes, Stack size 8 bytes, tcp.o(i.tcp_tmr))
  [Stack]

  - Max Depth = 332
  - Call Chain = tcp_tmr ⇒ tcp_fasttmr ⇒ tcp_recv_null ⇒ tcp_close ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_slowtmr
  - >> tcp_fasttmr
  [Called By]
  - >> LwIP_Periodic_Handle

  tcp_update_rcv_ann_wnd (Thumb, 52 bytes, Stack size 16 bytes, tcp.o(i.tcp_update_rcv_ann_wnd))
  [Stack]

  - Max Depth = 16
  - Call Chain = tcp_update_rcv_ann_wnd
  [Called By]
  - >> tcp_recved
  - >> tcp_receive

  tcp_write (Thumb, 46 bytes, Stack size 16 bytes, tcp_out.o(i.tcp_write))
  [Stack]

  - Max Depth = 180
  - Call Chain = tcp_write ⇒ tcp_enqueue ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_enqueue
  [Called By]
  - >> send_data

  tcp_zero_window_probe (Thumb, 144 bytes, Stack size 32 bytes, tcp_out.o(i.tcp_zero_window_probe))
  [Stack]

  - Max Depth = 244
  - Call Chain = tcp_zero_window_probe ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> ip_output
  - >> pbuf_alloc
  - >> ntohs
  - >> htons
  - >> tcp_output_set_header
  [Called By]
  - >> tcp_slowtmr

  udp_input (Thumb, 336 bytes, Stack size 48 bytes, udp.o(i.udp_input))
  [Stack]

  - Max Depth = 300
  - Call Chain = udp_input ⇒ icmp_dest_unreach ⇒ icmp_send_response ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> ip_addr_isbroadcast
  - >> icmp_dest_unreach
  - >> ntohl
  - >> pbuf_header
  - >> ntohs
  [Called By]
  - >> ip_input

  ### Local Symbols

  SetSysClock (Thumb, 162 bytes, Stack size 12 bytes, system_stm32f4xx.o(i.SetSysClock))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClock
  [Called By]
  - >> SystemInit

  IAP_HTTP_writedata (Thumb, 130 bytes, Stack size 32 bytes, httpserver.o(i.IAP_HTTP_writedata))
  [Stack]

  - Max Depth = 80
  - Call Chain = IAP_HTTP_writedata ⇒ FLASH_If_Write ⇒ FLASH_ProgramWord ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_If_Write
  [Called By]
  - >> http_recv

  Parse_Content_Length (Thumb, 102 bytes, Stack size 40 bytes, httpserver.o(i.Parse_Content_Length))
  [Stack]

  - Max Depth = 52
  - Call Chain = Parse_Content_Length ⇒ strncmp
  [Calls]
  - >> strncmp
  [Called By]
  - >> http_recv

  close_conn (Thumb, 44 bytes, Stack size 16 bytes, httpserver.o(i.close_conn))
  [Stack]

  - Max Depth = 316
  - Call Chain = close_conn ⇒ tcp_close ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_sent
  - >> tcp_recv
  - >> tcp_close
  - >> tcp_arg
  - >> mem_free
  [Called By]
  - >> http_sent
  - >> http_recv

  conn_err (Thumb, 4 bytes, Stack size 0 bytes, httpserver.o(i.conn_err))
  [Stack]

  - Max Depth = 12
  - Call Chain = conn_err ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> mem_free
  [Address Reference Count : 1]
  - httpserver.o(i.http_accept)

  fs_open (Thumb, 42 bytes, Stack size 16 bytes, httpserver.o(i.fs_open))
  [Stack]

  - Max Depth = 24
  - Call Chain = fs_open ⇒ strcmp
  [Calls]
  - >> strcmp
  [Called By]
  - >> http_recv

  http_accept (Thumb, 62 bytes, Stack size 8 bytes, httpserver.o(i.http_accept))
  [Stack]

  - Max Depth = 28
  - Call Chain = http_accept ⇒ mem_malloc
  [Calls]
  - >> tcp_recv
  - >> tcp_poll
  - >> tcp_err
  - >> tcp_arg
  - >> mem_malloc
  [Address Reference Count : 1]
  - httpserver.o(i.IAP_httpd_init)

  http_poll (Thumb, 26 bytes, Stack size 8 bytes, httpserver.o(i.http_poll))
  [Stack]

  - Max Depth = 308
  - Call Chain = http_poll ⇒ tcp_close ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_close
  - >> send_data
  [Address Reference Count : 1]
  - httpserver.o(i.http_accept)

  http_recv (Thumb, 1452 bytes, Stack size 152 bytes, httpserver.o(i.http_recv))
  [Stack]

  - Max Depth = 468
  - Call Chain = http_recv ⇒ close_conn ⇒ tcp_close ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_sent
  - >> tcp_recved
  - >> pbuf_free
  - >> LCD_SetTextColor
  - >> LCD_GetFont
  - >> LCD_DisplayStringLine
  - >> LCD_Clear
  - >> send_data
  - >> fs_open
  - >> close_conn
  - >> Parse_Content_Length
  - >> IAP_HTTP_writedata
  - >> FLASH_If_Init
  - >> FLASH_If_Erase
  - >> __2sprintf
  - >> strncmp
  [Address Reference Count : 1]
  - httpserver.o(i.http_accept)

  http_sent (Thumb, 60 bytes, Stack size 8 bytes, httpserver.o(i.http_sent))
  [Stack]

  - Max Depth = 324
  - Call Chain = http_sent ⇒ close_conn ⇒ tcp_close ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> send_data
  - >> close_conn
  [Address Reference Count : 1]
  - httpserver.o(i.http_recv)

  send_data (Thumb, 44 bytes, Stack size 16 bytes, httpserver.o(i.send_data))
  [Stack]

  - Max Depth = 196
  - Call Chain = send_data ⇒ tcp_write ⇒ tcp_enqueue ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_write
  [Called By]
  - >> http_sent
  - >> http_recv
  - >> http_poll

  ETH_GPIO_Config (Thumb, 194 bytes, Stack size 16 bytes, stm32f4x7_eth_bsp.o(i.ETH_GPIO_Config))
  [Stack]

  - Max Depth = 36
  - Call Chain = ETH_GPIO_Config ⇒ GPIO_Init
  [Calls]
  - >> SYSCFG_ETH_MediaInterfaceConfig
  - >> RCC_MCO1Config
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  [Called By]
  - >> ETH_BSP_Config

  ETH_MACDMA_Config (Thumb, 116 bytes, Stack size 192 bytes, stm32f4x7_eth_bsp.o(i.ETH_MACDMA_Config))
  [Stack]

  - Max Depth = 264
  - Call Chain = ETH_MACDMA_Config ⇒ ETH_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> ETH_StructInit
  - >> ETH_SoftwareReset
  - >> ETH_Init
  - >> ETH_GetSoftwareResetStatus
  - >> ETH_DeInit
  [Called By]
  - >> ETH_BSP_Config

  ip_reass_chain_frag_into_datagram_and_validate (Thumb, 236 bytes, Stack size 32 bytes, ip_frag.o(i.ip_reass_chain_frag_into_datagram_and_validate))
  [Stack]

  - Max Depth = 60
  - Call Chain = ip_reass_chain_frag_into_datagram_and_validate ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> pbuf_clen
  - >> ntohs
  [Called By]
  - >> ip_reass

  ip_reass_dequeue_datagram (Thumb, 30 bytes, Stack size 8 bytes, ip_frag.o(i.ip_reass_dequeue_datagram))
  [Stack]

  - Max Depth = 8
  - Call Chain = ip_reass_dequeue_datagram
  [Calls]
  - >> memp_free
  [Called By]
  - >> ip_reass
  - >> ip_reass_free_complete_datagram

  ip_reass_free_complete_datagram (Thumb, 106 bytes, Stack size 24 bytes, ip_frag.o(i.ip_reass_free_complete_datagram))
  [Stack]

  - Max Depth = 276
  - Call Chain = ip_reass_free_complete_datagram ⇒ icmp_time_exceeded ⇒ icmp_send_response ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> pbuf_clen
  - >> icmp_time_exceeded
  - >> ip_reass_dequeue_datagram
  - >> __aeabi_memcpy
  [Called By]
  - >> ip_reass_remove_oldest_datagram

  ip_reass_remove_oldest_datagram (Thumb, 104 bytes, Stack size 24 bytes, ip_frag.o(i.ip_reass_remove_oldest_datagram))
  [Stack]

  - Max Depth = 300
  - Call Chain = ip_reass_remove_oldest_datagram ⇒ ip_reass_free_complete_datagram ⇒ icmp_time_exceeded ⇒ icmp_send_response ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ip_reass_free_complete_datagram
  [Called By]
  - >> ip_reass

  autoip_arp_announce (Thumb, 32 bytes, Stack size 24 bytes, autoip.o(i.autoip_arp_announce))
  [Stack]

  - Max Depth = 132
  - Call Chain = autoip_arp_announce ⇒ etharp_raw ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> etharp_raw
  [Called By]
  - >> autoip_arp_reply

  autoip_start_probing (Thumb, 68 bytes, Stack size 8 bytes, autoip.o(i.autoip_start_probing))
  [Stack]

  - Max Depth = 8
  - Call Chain = autoip_start_probing
  [Called By]
  - >> autoip_start

  icmp_send_response (Thumb, 102 bytes, Stack size 40 bytes, icmp.o(i.icmp_send_response))
  [Stack]

  - Max Depth = 252
  - Call Chain = icmp_send_response ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> ip_output
  - >> pbuf_alloc
  - >> inet_chksum
  - >> __aeabi_memcpy
  [Called By]
  - >> icmp_dest_unreach
  - >> icmp_time_exceeded

  lwip_standard_chksum (Thumb, 62 bytes, Stack size 8 bytes, inet_chksum.o(i.lwip_standard_chksum))
  [Stack]

  - Max Depth = 8
  - Call Chain = lwip_standard_chksum
  [Calls]
  - >> htons
  [Called By]
  - >> inet_chksum_pbuf
  - >> inet_chksum

  plug_holes (Thumb, 78 bytes, Stack size 12 bytes, mem.o(i.plug_holes))
  [Stack]

  - Max Depth = 12
  - Call Chain = plug_holes
  [Called By]
  - >> mem_free

  tcp_accept_null (Thumb, 6 bytes, Stack size 0 bytes, tcp.o(i.tcp_accept_null))
  [Address Reference Count : 1]

  - tcp.o(i.tcp_listen_with_backlog)

  tcp_new_port (Thumb, 92 bytes, Stack size 20 bytes, tcp.o(i.tcp_new_port))
  [Stack]

  - Max Depth = 20
  - Call Chain = tcp_new_port
  [Called By]
  - >> tcp_bind

  tcp_listen_input (Thumb, 222 bytes, Stack size 24 bytes, tcp_in.o(i.tcp_listen_input))
  [Stack]

  - Max Depth = 388
  - Call Chain = tcp_listen_input ⇒ tcp_alloc ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_abandon
  - >> tcp_parseopt
  - >> tcp_rst
  - >> tcp_output
  - >> tcp_enqueue
  - >> tcp_eff_send_mss
  - >> tcp_alloc
  [Called By]
  - >> tcp_input

  tcp_parseopt (Thumb, 122 bytes, Stack size 16 bytes, tcp_in.o(i.tcp_parseopt))
  [Stack]

  - Max Depth = 16
  - Call Chain = tcp_parseopt
  [Calls]
  - >> ntohs
  [Called By]
  - >> tcp_process
  - >> tcp_listen_input

  tcp_process (Thumb, 812 bytes, Stack size 48 bytes, tcp_in.o(i.tcp_process))
  [Stack]

  - Max Depth = 388
  - Call Chain = tcp_process ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_abandon
  - >> ntohl
  - >> tcp_rexmit
  - >> tcp_receive
  - >> tcp_parseopt
  - >> tcp_rst
  - >> tcp_output
  - >> tcp_seg_free
  - >> tcp_pcb_purge
  - >> tcp_eff_send_mss
  [Called By]
  - >> tcp_input

  tcp_receive (Thumb, 1082 bytes, Stack size 24 bytes, tcp_in.o(i.tcp_receive))
  [Stack]

  - Max Depth = 292
  - Call Chain = tcp_receive ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ntohl
  - >> pbuf_realloc
  - >> pbuf_header
  - >> pbuf_clen
  - >> ntohs
  - >> htons
  - >> tcp_send_empty_ack
  - >> tcp_rexmit_fast
  - >> tcp_output
  - >> tcp_update_rcv_ann_wnd
  - >> tcp_seg_free
  [Called By]
  - >> tcp_process

  tcp_timewait_input (Thumb, 100 bytes, Stack size 16 bytes, tcp_in.o(i.tcp_timewait_input))
  [Stack]

  - Max Depth = 284
  - Call Chain = tcp_timewait_input ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_rst
  - >> tcp_output
  [Called By]
  - >> tcp_input

  tcp_output_segment (Thumb, 168 bytes, Stack size 24 bytes, tcp_out.o(i.tcp_output_segment))
  [Stack]

  - Max Depth = 236
  - Call Chain = tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> htonl
  - >> ip_route
  - >> ip_output
  - >> ntohl
  - >> htons
  [Called By]
  - >> tcp_output

  tcp_output_set_header (Thumb, 124 bytes, Stack size 24 bytes, tcp_out.o(i.tcp_output_set_header))
  [Stack]

  - Max Depth = 24
  - Call Chain = tcp_output_set_header
  [Calls]
  - >> htonl
  - >> ntohs
  - >> htons
  [Called By]
  - >> tcp_send_empty_ack
  - >> tcp_zero_window_probe
  - >> tcp_keepalive

  etharp_send_ip (Thumb, 54 bytes, Stack size 24 bytes, etharp.o(i.etharp_send_ip))
  [Stack]

  - Max Depth = 24
  - Call Chain = etharp_send_ip
  [Calls]
  - >> htons
  [Called By]
  - >> etharp_query
  - >> etharp_output
  - >> update_arp_entry

  find_entry (Thumb, 326 bytes, Stack size 48 bytes, etharp.o(i.find_entry))
  [Stack]

  - Max Depth = 92
  - Call Chain = find_entry ⇒ free_etharp_q ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> free_etharp_q
  [Called By]
  - >> etharp_query
  - >> update_arp_entry

  free_etharp_q (Thumb, 30 bytes, Stack size 16 bytes, etharp.o(i.free_etharp_q))
  [Stack]

  - Max Depth = 44
  - Call Chain = free_etharp_q ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> memp_free
  [Called By]
  - >> etharp_tmr
  - >> find_entry

  update_arp_entry (Thumb, 162 bytes, Stack size 32 bytes, etharp.o(i.update_arp_entry))
  [Stack]

  - Max Depth = 124
  - Call Chain = update_arp_entry ⇒ find_entry ⇒ free_etharp_q ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> ip_addr_isbroadcast
  - >> ntohl
  - >> memp_free
  - >> find_entry
  - >> etharp_send_ip
  [Called By]
  - >> etharp_ip_input
  - >> etharp_arp_input

  low_level_init (Thumb, 112 bytes, Stack size 16 bytes, ethernetif.o(i.low_level_init))
  [Stack]

  - Max Depth = 36
  - Call Chain = low_level_init ⇒ ETH_DMATxDescChainInit
  [Calls]
  - >> ETH_Start
  - >> ETH_MACAddressConfig
  - >> ETH_DMATxDescChecksumInsertionConfig
  - >> ETH_DMATxDescChainInit
  - >> ETH_DMARxDescChainInit
  [Called By]
  - >> ethernetif_init

  low_level_input (Thumb, 120 bytes, Stack size 40 bytes, ethernetif.o(i.low_level_input))
  [Stack]

  - Max Depth = 108
  - Call Chain = low_level_input ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_alloc
  - >> ETH_Get_Received_Frame
  - >> __aeabi_memcpy
  [Called By]
  - >> ethernetif_input

  low_level_output (Thumb, 44 bytes, Stack size 16 bytes, ethernetif.o(i.low_level_output))
  [Stack]

  - Max Depth = 36
  - Call Chain = low_level_output ⇒ ETH_Prepare_Transmit_Descriptors
  [Calls]
  - >> ETH_Prepare_Transmit_Descriptors
  - >> __aeabi_memcpy
  [Address Reference Count : 1]
  - ethernetif.o(i.ethernetif_init)

  ETH_Delay (Thumb, 18 bytes, Stack size 12 bytes, stm32f4x7_eth.o(i.ETH_Delay))
  [Stack]

  - Max Depth = 12
  - Call Chain = ETH_Delay
  [Called By]
  - >> ETH_Init

  _printf_core (Thumb, 436 bytes, Stack size 96 bytes, printf3.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uidivmod
  [Called By]
  - >> __0sprintf$3

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printf3.o(i._sputc))
  [Called By]

  - >> __0sprintf$3
  [Address Reference Count : 1]
  - printf3.o(i.__0sprintf$3)

  ### Undefined Global Symbols