nRF51 SDK: GAP Advertising timeout values

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Advertising timeout values
Defines

## Macros

#define | BLE_GAP_ADV_TIMEOUT_LIMITED_MAX 180
#define | BLE_GAP_ADV_TIMEOUT_GENERAL_UNLIMITED 0

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_ADV_TIMEOUT_GENERAL_UNLIMITED 0

Unlimited advertising in general discoverable mode.

#define BLE_GAP_ADV_TIMEOUT_LIMITED_MAX 180

Maximum advertising time in limited discoverable mode (TGAP(lim_adv_timeout) = 180s in spec (Addendum 2)).