nRF51 SDK: Cycling Speed and Cadence Service

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Cycling Speed and Cadence Service

This module implements the Cycling Speed and Cadence Service. If enabled, notification of the Cycling Speead and Candence Measurement is performed when the application calls ble_cscs_measurement_send().

If an event handler is supplied by the application, the Cycling Speed and Cadence Service will generate Cycling Speed and Cadence Service events to the application.

Note
  The application must propagate BLE stack events to the Cycling Speead and Candence Service module by calling ble_cscs_on_ble_evt() from the from the ble_stack_handler function.