nRF51 SDK: SVC return values specific to GAP

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
SVC return values specific to GAP
Defines

## Macros

#define | BLE_ERROR_GAP_UUID_LIST_MISMATCH (NRF_GAP_ERR_BASE + 0x000)
#define | BLE_ERROR_GAP_DISCOVERABLE_WITH_WHITELIST (NRF_GAP_ERR_BASE + 0x001)
#define | BLE_ERROR_GAP_INVALID_BLE_ADDR (NRF_GAP_ERR_BASE + 0x002)

## Detailed Description

## Macro Definition Documentation

#define BLE_ERROR_GAP_DISCOVERABLE_WITH_WHITELIST (NRF_GAP_ERR_BASE + 0x001)

Use of Whitelist not permitted with discoverable advertising.

#define BLE_ERROR_GAP_INVALID_BLE_ADDR (NRF_GAP_ERR_BASE + 0x002)

The upper two bits of the address do not correspond to the specified address type.

#define BLE_ERROR_GAP_UUID_LIST_MISMATCH (NRF_GAP_ERR_BASE + 0x000)

UUID list does not contain an integral number of UUIDs.