nRF51 SDK: Types

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Typedefs
Types
SoftDevice Manager API

## Typedefs

typedef uint32_t | nrf_clock_lfclksrc_t
| Type representing lfclk oscillator source.
typedef void(* | softdevice_assertion_handler_t )(uint32_t pc, uint16_t line_number, const uint8_t *p_file_name)
| SoftDevice Assertion Handler type. More...

## Detailed Description

## Typedef Documentation

typedef void(* softdevice_assertion_handler_t)(uint32_t pc, uint16_t line_number, const uint8_t *p_file_name)

SoftDevice Assertion Handler type.

When an unexpected error occurs within the SoftDevice it will call the SoftDevice assertion handler callback. The protocol stack will be in an undefined state when this happens and the only way to recover will be to perform a reset, using e.g. CMSIS NVIC_SystemReset().

Note
  This callback is executed in HardFault context, thus SVC functions cannot be called from the SoftDevice assert callback.

Parameters

  [in] | pc | The program counter of the failed assert.
  [in] | line_number | Line number where the assert failed.
  [in] | file_name | File name where the assert failed.