nRF51 SDK: Temperature Example

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Temperature Example

The Temperature Example project uses a temperature sensor, displaying the measurement on Port 1 GPIO (LEDs). It uses the hardware delivered in the nRF51822 Development Kit.

Note
  Port 1 only has 8 bits, so only positive temperatures are displayed.

The application starts with configuring the temperature module and the GPIO. The main loop reads the temperature sensor and updates the LEDs every 500ms.

# Setup

Instructions on how to set up the nRFgo Motherboard: nRFgo Motherboard Setup (nRF6310).

LED assignments:

- LED 0-7 is used to show the measured temperature.

# Testing

The Temperature Example Application can be tested as follows:

1. Compile and program the application.
2. The LEDs should show a binary value that is close to the real temperature.