nRF51 SDK: Definitions for the Alert Level characteristic values

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
Definitions for the Alert Level characteristic values
'Common service definitions'

## Macros

#define | BLE_CHAR_ALERT_LEVEL_NO_ALERT 0x00
#define | BLE_CHAR_ALERT_LEVEL_MILD_ALERT 0x01
#define | BLE_CHAR_ALERT_LEVEL_HIGH_ALERT 0x02

## Detailed Description

## Macro Definition Documentation

#define BLE_CHAR_ALERT_LEVEL_HIGH_ALERT 0x02

High Alert.

#define BLE_CHAR_ALERT_LEVEL_MILD_ALERT 0x01

Mild Alert.

#define BLE_CHAR_ALERT_LEVEL_NO_ALERT 0x00

No Alert.