nRF51 SDK: Structures

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Structures
Structures
Generic Access Profile (GAP)

## Data Structures

struct | ble_gap_addr_t
| Bluetooth Low Energy address. More...
struct | ble_gap_conn_params_t
| GAP connection parameters. More...
struct | ble_gap_conn_sec_mode_t
| GAP link requirements. More...
struct | ble_gap_conn_sec_t
| GAP connection security status. More...
struct | ble_gap_irk_t
| Identity Resolving Key. More...
struct | ble_gap_whitelist_t
| Whitelist structure. More...
struct | ble_gap_adv_params_t
| GAP advertising parameters. More...
struct | ble_gap_scan_params_t
| GAP scanning parameters. More...
struct | ble_gap_sec_kdist_t
| Keys that can be exchanged. More...
struct | ble_gap_sec_params_t
| GAP security parameters. More...
struct | ble_gap_enc_info_t
| GAP Encryption Information. More...
struct | ble_gap_master_id_t
| GAP Master Identification. More...
struct | ble_gap_sign_info_t
| GAP Signing Information. More...
struct | ble_gap_evt_connected_t
| Event data for connected event. More...
struct | ble_gap_evt_disconnected_t
| Event data for disconnected event. More...
struct | ble_gap_evt_conn_param_update_t
| Event data for connection parameter update event. More...
struct | ble_gap_evt_sec_params_request_t
| Event data for security parameters request event. More...
struct | ble_gap_evt_sec_info_request_t
| Event data for securito info request event. More...
struct | ble_gap_evt_passkey_display_t
| Event data for passkey display event. More...
struct | ble_gap_evt_auth_key_request_t
| Event data for authentication key request event. More...
struct | ble_gap_sec_levels_t
| Security levels supported. More...
struct | ble_gap_enc_key_t
| Encryption Key. More...
struct | ble_gap_id_key_t
| Identity Key. More...
struct | ble_gap_sec_keys_t
| Keys that have been exchanged. More...
struct | ble_gap_sec_keyset_t
| Security key set (both Peripheral and Central keys). Note that when distributing Bluetooth addresses pertaining to the local device those will have to be filled in by the user. More...
struct | ble_gap_evt_auth_status_t
| Event data for authentication status event. More...
struct | ble_gap_evt_conn_sec_update_t
| Event data for connection security update event. More...
struct | ble_gap_evt_timeout_t
| Event data for timeout event. More...
struct | ble_gap_evt_rssi_changed_t
| Event data for advertisement report event. More...
struct | ble_gap_evt_adv_report_t
| Event data for advertising report event. More...
struct | ble_gap_evt_sec_request_t
| Event data for security request event. More...
struct | ble_gap_evt_conn_param_update_request_t
| Event data for connection parameter update request event. More...
struct | ble_gap_evt_t
| GAP event callback event structure. More...
struct | ble_gap_opt_ch_map_t
| Channel Map option. More...
union | ble_gap_opt_t
| Option structure for GAP options. More...

## Detailed Description