nRF51 SDK: ble_rscs_meas_s Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_rscs_meas_s Struct Reference
Running Speed and Cadence Service

Running Speed and Cadence Service measurement structure. This contains a Running Speed and Cadence measurement. More...

`#include <ble_rscs.h>`

## Data Fields

bool | is_inst_stride_len_present
bool | is_total_distance_present
bool | is_running
uint16_t | inst_speed
uint8_t | inst_cadence
uint16_t | inst_stride_length
uint32_t | total_distance

## Detailed Description

Running Speed and Cadence Service measurement structure. This contains a Running Speed and Cadence measurement.

## Field Documentation

uint8_t ble_rscs_meas_s::inst_cadence

Instantaneous Cadence.

uint16_t ble_rscs_meas_s::inst_speed

Instantaneous Speed.

uint16_t ble_rscs_meas_s::inst_stride_length

Instantaneous Stride Length.

bool ble_rscs_meas_s::is_inst_stride_len_present

True if Instantaneous Stride Length is present in the measurement.

bool ble_rscs_meas_s::is_running

True if running, False if walking.

bool ble_rscs_meas_s::is_total_distance_present

True if Total Distance is present in the measurement.

uint32_t ble_rscs_meas_s::total_distance

Total Distance.