nRF51 SDK: Advertising Application Serialized

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Advertising Application Serialized

# Advertising Application Serialized

The Serialized Advertising Application is a firmware prototype using serialized SoftDevice commands to connect to a connectivity chip using the hardware delivered in the nRF51822 Development Kit.

The source code and project file can be found in the `<InstallFolder>\Nordic\nrf51\Board\nrf6310\ble_s110_serialization\ble_app_advertising` folder.

# Setup

Instructions on how to set up the nRFgo Motherboard for serialization: nRFgo Motherboard Setup - Serialization.

LED assignments:

- LED 0: Advertising
- LED 1: Connected
- LED 2: Running
- LED 7: Asserted (for example an assert check in the application has failed)

# Testing

The Serialized Advertising Application can be tested using the Master Control Panel as follows:

1. Compile and program the application. Observe that the Advertising LED (LED 0) is lit.
2. Locate and connect to the Application using Master Control Panel. The application will be advertising as 'BLE_Connectivity'.
3. Observe that the Connected LED is lit, and the Advertising LED is off.
4. Disconnect, and observe that the Advertising LED (LED 0) is lit, the Connected LED (LED 1) is off.