nRF51 SDK: Enumerations

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Enumerations
Enumerations
Events, type definitions and API calls

## Enumerations

enum

BLE_COMMON_SVCS {
SD_BLE_EVT_GET = 0x60, SD_BLE_TX_BUFFER_COUNT_GET, SD_BLE_UUID_VS_ADD, SD_BLE_UUID_DECODE,
SD_BLE_UUID_ENCODE, SD_BLE_VERSION_GET, SD_BLE_USER_MEM_REPLY, SD_BLE_EVT_GET = 0x60,
SD_BLE_TX_BUFFER_COUNT_GET, SD_BLE_UUID_VS_ADD, SD_BLE_UUID_DECODE, SD_BLE_UUID_ENCODE,
SD_BLE_VERSION_GET, SD_BLE_USER_MEM_REPLY, SD_BLE_OPT_SET, SD_BLE_OPT_GET,
SD_BLE_EVT_GET = 0x60, SD_BLE_TX_BUFFER_COUNT_GET, SD_BLE_UUID_VS_ADD, SD_BLE_UUID_DECODE,
SD_BLE_UUID_ENCODE, SD_BLE_VERSION_GET, SD_BLE_USER_MEM_REPLY
}

| Common API SVC numbers. More...

enum

BLE_COMMON_EVTS {
BLE_EVT_TX_COMPLETE = 0x01, BLE_EVT_USER_MEM_REQUEST, BLE_EVT_USER_MEM_RELEASE, BLE_EVT_TX_COMPLETE = 0x01,
BLE_EVT_USER_MEM_REQUEST, BLE_EVT_USER_MEM_RELEASE, BLE_EVT_TX_COMPLETE = 0x01, BLE_EVT_USER_MEM_REQUEST,
BLE_EVT_USER_MEM_RELEASE
}

| BLE Module Independent Event IDs. More...

## Detailed Description

## Enumeration Type Documentation

enum BLE_COMMON_EVTS

BLE Module Independent Event IDs.

Enumerator
BLE_EVT_TX_COMPLETE | Transmission Complete.
BLE_EVT_USER_MEM_REQUEST | User Memory request.
BLE_EVT_USER_MEM_RELEASE | User Memory release.
BLE_EVT_TX_COMPLETE | Common BLE Event base. Transmission Complete.
BLE_EVT_USER_MEM_REQUEST | User Memory request.
BLE_EVT_USER_MEM_RELEASE | User Memory release.
BLE_EVT_TX_COMPLETE | Transmission Complete.
BLE_EVT_USER_MEM_REQUEST | User Memory request.
BLE_EVT_USER_MEM_RELEASE | User Memory release.

enum BLE_COMMON_SVCS

Common API SVC numbers.

Enumerator
SD_BLE_EVT_GET | Get an event from the pending events queue.
SD_BLE_TX_BUFFER_COUNT_GET | Get the total number of available application transmission buffers from the stack.
SD_BLE_UUID_VS_ADD | Add a Vendor Specific UUID.
SD_BLE_UUID_DECODE | Decode UUID bytes.
SD_BLE_UUID_ENCODE | Encode UUID bytes.
SD_BLE_VERSION_GET | Get the local version information (company id, LMP Version, LMP Subversion).
SD_BLE_USER_MEM_REPLY | User Memory Reply.
SD_BLE_EVT_GET | Common BLE SVC base. Get an event from the pending events queue.
SD_BLE_TX_BUFFER_COUNT_GET | Get the total number of available application transmission buffers from the stack.
SD_BLE_UUID_VS_ADD | Add a Vendor Specific UUID.
SD_BLE_UUID_DECODE | Decode UUID bytes.
SD_BLE_UUID_ENCODE | Encode UUID bytes.
SD_BLE_VERSION_GET | Get the local version information (company id, LMP Version, LMP Subversion).
SD_BLE_USER_MEM_REPLY | User Memory Reply.
SD_BLE_OPT_SET | Set a BLE option.
SD_BLE_OPT_GET | Get a BLE option.
SD_BLE_EVT_GET | Get an event from the pending events queue.
SD_BLE_TX_BUFFER_COUNT_GET | Get the total number of available application transmission buffers from the stack.
SD_BLE_UUID_VS_ADD | Add a Vendor Specific UUID.
SD_BLE_UUID_DECODE | Decode UUID bytes.
SD_BLE_UUID_ENCODE | Encode UUID bytes.
SD_BLE_VERSION_GET | Get the local version information (company id, LMP Version, LMP Subversion).
SD_BLE_USER_MEM_REPLY | User Memory Reply.