nRF51 SDK: ble_sensorsim_cfg_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_sensorsim_cfg_t Struct Reference
Sensor Data Simulator

Triangular waveform sensor simulator configuration. More...

`#include <ble_sensorsim.h>`

## Data Fields

uint32_t | min
uint32_t | max
uint32_t | incr
bool | start_at_max

## Detailed Description

Triangular waveform sensor simulator configuration.

## Field Documentation

uint32_t ble_sensorsim_cfg_t::incr

Increment between each measurement.

uint32_t ble_sensorsim_cfg_t::max

Maximum simulated value.

uint32_t ble_sensorsim_cfg_t::min

Minimum simulated value.

bool ble_sensorsim_cfg_t::start_at_max

TRUE is measurement is to start at the maximum value, FALSE if it is to start at the minimum.