nRF51 SDK: GAP Scan window max and min

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Scan window max and min
Defines

## Macros

#define | BLE_GAP_SCAN_WINDOW_MIN 0x0004
#define | BLE_GAP_SCAN_WINDOW_MAX 0x4000

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_SCAN_WINDOW_MAX 0x4000

Maximum Scan window in 625 us units, i.e. 10.24 s.

#define BLE_GAP_SCAN_WINDOW_MIN 0x0004

Minimum Scan window in 625 us units, i.e. 2.5 ms.