nRF51 SDK: ble_ans_c_evt_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_ans_c_evt_t Struct Reference
Alert Notification Service Client

Alert Notification Event structure. More...

`#include <ble_ans_c.h>`

## Data Fields

ble_ans_c_evt_type_t | evt_type
ble_uuid_t | uuid
union {
ble_ans_alert_settings_t settings
ble_ans_alert_notification_t alert
uint32_t error_code
} | data

## Detailed Description

Alert Notification Event structure.

The structure contains the event that should be handled, as well as additional information.

## Field Documentation

ble_ans_alert_notification_t ble_ans_c_evt_t::alert

Alert Notification data sent by the server.

uint32_t ble_ans_c_evt_t::error_code

Additional status/error code if the event was caused by a stack error or gatt status, e.g. during service discovery.

ble_ans_c_evt_type_t ble_ans_c_evt_t::evt_type

Type of event.

ble_ans_alert_settings_t ble_ans_c_evt_t::settings

Setting returned from server on read request.

ble_uuid_t ble_ans_c_evt_t::uuid

UUID of the event in case of an alert or notification.