Static Call Graph - [.\_build\ble_app_hrs.axf]

# Static Call Graph for image .\_build\ble_app_hrs.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 76]: Last Updated: Tue Aug 26 15:28:32 2014

### Maximum Stack Usage = 336 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ ble_bondmngr_init ⇒ pstorage_clear ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ swap_state_process

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- SVC_Handler ⇒ SVC_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- CCM_AAR_IRQHandler ⇒ CCM_AAR_IRQHandler
- __asm___11_app_timer_c_cd27f9c3__nrf_delay_us ⇒ __asm___11_app_timer_c_cd27f9c3__nrf_delay_us

  ### Function Pointers

  - ADC_IRQHandler from battery.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - CCM_AAR_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - ECB_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - GPIOTE_IRQHandler from app_gpiote.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - HardFault_Handler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - LPCOMP_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - NMI_Handler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - POWER_CLOCK_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - PendSV_Handler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - QDEC_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - RADIO_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - RNG_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - RTC0_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - RTC1_IRQHandler from app_timer.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - Reset_Handler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SPI0_TWI0_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SPI1_TWI1_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SVC_Handler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SWI0_IRQHandler from app_timer.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SWI1_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SWI2_IRQHandler from softdevice_handler.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SWI3_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SWI4_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SWI5_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SysTick_Handler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SystemInit from system_nrf51.o(.text) referenced from arm_startup_nrf51.o(.text)
  - TEMP_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - TIMER0_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - TIMER1_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - TIMER2_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - UART0_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - WDT_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - __main from __main.o(!!!main) referenced from arm_startup_nrf51.o(.text)
  - battery_level_meas_timeout_handler from main.o(.text) referenced from main.o(.text)
  - ble_evt_dispatch from main.o(.text) referenced from main.o(.text)
  - bm_pstorage_cb_handler from ble_bondmngr.o(.text) referenced from ble_bondmngr.o(.text)
  - bond_manager_error_handler from main.o(.text) referenced from main.o(.text)
  - button_event_handler from main.o(.text) referenced 2 times from main.o(.data)
  - conn_params_error_handler from main.o(.text) referenced from main.o(.text)
  - detection_delay_timeout_handler from app_button.o(.text) referenced from app_button.o(.text)
  - gpiote_event_handler from app_button.o(.text) referenced from app_button.o(.text)
  - heart_rate_meas_timeout_handler from main.o(.text) referenced from main.o(.text)
  - softdevice_assertion_handler from softdevice_handler.o(.text) referenced from softdevice_handler.o(.text)
  - sys_evt_dispatch from main.o(.text) referenced from main.o(.text)
  - update_timeout_handler from ble_conn_params.o(.text) referenced from ble_conn_params.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 52 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000001))

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000031))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 336 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ ble_bondmngr_init ⇒ pstorage_clear ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ swap_state_process
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  __asm___11_app_timer_c_cd27f9c3__nrf_delay_us (Thumb, 30 bytes, Stack size 0 bytes, app_timer.o(.emb_text))
  [Calls]

  - >> __asm___11_app_timer_c_cd27f9c3__nrf_delay_us
  [Called By]
  - >> __asm___11_app_timer_c_cd27f9c3__nrf_delay_us
  - >> timer_list_handler
  - >> app_timer_init

  __aeabi_memcpy4 (Thumb, 56 bytes, Stack size 0 bytes, rt_memcpy.o(.emb_text))
  [Called By]

  - >> ble_bondmngr_on_ble_evt
  - >> ble_bondmngr_init
  - >> ble_bondmngr_bonded_centrals_store
  - >> __aeabi_memmove4
  - >> __aeabi_memcpy
  - >> ble_bondmngr_bonded_central_delete

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, rt_memcpy.o(.emb_text), UNUSED)

  Reset_Handler (Thumb, 18 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  CCM_AAR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Calls]

  - >> CCM_AAR_IRQHandler
  [Called By]
  - >> CCM_AAR_IRQHandler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  ECB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  LPCOMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  POWER_CLOCK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  QDEC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  RADIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  RTC0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  SPI0_TWI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  SPI1_TWI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  SWI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  SWI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  SWI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  SWI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  TEMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, arm_startup_nrf51.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  SystemCoreClockUpdate (Thumb, 8 bytes, Stack size 0 bytes, system_nrf51.o(.text), UNUSED)

  SystemInit (Thumb, 108 bytes, Stack size 0 bytes, system_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(.text)

  app_error_handler (Thumb, 16 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> char_add
  - >> ADC_IRQHandler
  - >> led_start
  - >> battery_start
  - >> detection_delay_timeout_handler
  - >> SWI2_IRQHandler
  - >> intern_softdevice_events_execute
  - >> RTC1_IRQHandler

  assert_nrf_callback (Thumb, 16 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> softdevice_assertion_handler

  main (Thumb, 956 bytes, Stack size 112 bytes, main.o(.text))
  [Stack]

  - Max Depth = 336
  - Call Chain = main ⇒ ble_bondmngr_init ⇒ pstorage_clear ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ swap_state_process
  [Calls]
  - >> softdevice_sys_evt_handler_set
  - >> softdevice_handler_init
  - >> softdevice_ble_evt_handler_set
  - >> pstorage_init
  - >> led_start
  - >> ble_srv_ascii_to_utf8
  - >> ble_hrs_init
  - >> ble_dis_init
  - >> ble_conn_params_init
  - >> ble_bondmngr_init
  - >> ble_bas_init
  - >> ble_advdata_set
  - >> app_timer_init
  - >> app_timer_create
  - >> app_gpiote_init
  - >> app_button_is_pushed
  - >> app_button_init
  - >> __aeabi_memclr4
  [Called By]
  - >> __rt_entry_main

  ADC_IRQHandler (Thumb, 206 bytes, Stack size 8 bytes, battery.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = ADC_IRQHandler ⇒ ble_bas_battery_level_update
  [Calls]
  - >> ble_bas_battery_level_update
  - >> app_error_handler
  - >> __aeabi_idivmod
  - >> __aeabi_uidivmod
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  battery_start (Thumb, 80 bytes, Stack size 16 bytes, battery.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = battery_start
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> battery_level_meas_timeout_handler

  led_start (Thumb, 108 bytes, Stack size 16 bytes, led.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = led_start
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> main

  led_stop (Thumb, 20 bytes, Stack size 0 bytes, led.o(.text))
  [Called By]

  - >> ble_evt_dispatch

  ble_dis_init (Thumb, 358 bytes, Stack size 32 bytes, ble_dis.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = ble_dis_init ⇒ char_add
  [Calls]
  - >> char_add
  [Called By]
  - >> main

  ble_bas_on_ble_evt (Thumb, 86 bytes, Stack size 8 bytes, ble_bas.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = ble_bas_on_ble_evt
  [Called By]
  - >> ble_evt_dispatch

  ble_bas_init (Thumb, 330 bytes, Stack size 96 bytes, ble_bas.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = ble_bas_init
  [Calls]
  - >> ble_srv_report_ref_encode
  [Called By]
  - >> main

  ble_bas_battery_level_update (Thumb, 102 bytes, Stack size 40 bytes, ble_bas.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = ble_bas_battery_level_update
  [Called By]
  - >> ADC_IRQHandler

  ble_hrs_on_ble_evt (Thumb, 80 bytes, Stack size 8 bytes, ble_hrs.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = ble_hrs_on_ble_evt
  [Called By]
  - >> ble_evt_dispatch

  ble_hrs_init (Thumb, 320 bytes, Stack size 112 bytes, ble_hrs.o(.text))
  [Stack]

  - Max Depth = 192
  - Call Chain = ble_hrs_init ⇒ hrm_encode ⇒ __aeabi_memmove ⇒ __aeabi_memcpy
  [Calls]
  - >> hrm_encode
  [Called By]
  - >> main

  ble_hrs_heart_rate_measurement_send (Thumb, 84 bytes, Stack size 56 bytes, ble_hrs.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = ble_hrs_heart_rate_measurement_send ⇒ hrm_encode ⇒ __aeabi_memmove ⇒ __aeabi_memcpy
  [Calls]
  - >> hrm_encode
  [Called By]
  - >> heart_rate_meas_timeout_handler

  ble_hrs_rr_interval_add (Thumb, 46 bytes, Stack size 16 bytes, ble_hrs.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memmove

  ble_hrs_rr_interval_buffer_is_full (Thumb, 16 bytes, Stack size 0 bytes, ble_hrs.o(.text), UNUSED)

  ble_hrs_sensor_contact_supported_set (Thumb, 18 bytes, Stack size 0 bytes, ble_hrs.o(.text), UNUSED)

  ble_hrs_sensor_contact_detected_update (Thumb, 6 bytes, Stack size 0 bytes, ble_hrs.o(.text), UNUSED)

  ble_hrs_body_sensor_location_set (Thumb, 22 bytes, Stack size 16 bytes, ble_hrs.o(.text), UNUSED)

  ble_conn_params_init (Thumb, 90 bytes, Stack size 16 bytes, ble_conn_params.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = ble_conn_params_init ⇒ app_timer_create
  [Calls]
  - >> app_timer_create
  [Called By]
  - >> main

  ble_conn_params_stop (Thumb, 12 bytes, Stack size 8 bytes, ble_conn_params.o(.text), UNUSED)
  [Calls]

  - >> app_timer_stop

  ble_conn_params_on_ble_evt (Thumb, 164 bytes, Stack size 24 bytes, ble_conn_params.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = ble_conn_params_on_ble_evt ⇒ conn_params_negotiation ⇒ app_timer_start
  [Calls]
  - >> app_timer_stop
  - >> conn_params_negotiation
  [Called By]
  - >> ble_evt_dispatch

  ble_conn_params_change_conn_params (Thumb, 80 bytes, Stack size 24 bytes, ble_conn_params.o(.text), UNUSED)

  ble_advdata_set (Thumb, 104 bytes, Stack size 88 bytes, ble_advdata.o(.text))
  [Stack]

  - Max Depth = 184
  - Call Chain = ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode
  [Calls]
  - >> adv_data_encode
  [Called By]
  - >> main

  ble_srv_report_ref_encode (Thumb, 12 bytes, Stack size 0 bytes, ble_srv_common.o(.text))
  [Called By]

  - >> ble_bas_init

  ble_srv_ascii_to_utf8 (Thumb, 18 bytes, Stack size 16 bytes, ble_srv_common.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = ble_srv_ascii_to_utf8 ⇒ strlen
  [Calls]
  - >> strlen
  [Called By]
  - >> main

  RTC1_IRQHandler (Thumb, 140 bytes, Stack size 24 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = RTC1_IRQHandler
  [Calls]
  - >> app_error_handler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  SWI0_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = SWI0_IRQHandler ⇒ timer_list_handler
  [Calls]
  - >> timer_list_handler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  app_timer_init (Thumb, 234 bytes, Stack size 40 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = app_timer_init
  [Calls]
  - >> __asm___11_app_timer_c_cd27f9c3__nrf_delay_us
  [Called By]
  - >> main

  app_timer_create (Thumb, 82 bytes, Stack size 12 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = app_timer_create
  [Called By]
  - >> ble_conn_params_init
  - >> app_button_init
  - >> main

  app_timer_start (Thumb, 212 bytes, Stack size 16 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = app_timer_start
  [Called By]
  - >> conn_params_negotiation
  - >> ble_evt_dispatch
  - >> gpiote_event_handler

  app_timer_stop (Thumb, 180 bytes, Stack size 16 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = app_timer_stop
  [Called By]
  - >> ble_conn_params_stop
  - >> ble_conn_params_on_ble_evt
  - >> app_button_disable
  - >> gpiote_event_handler

  app_timer_stop_all (Thumb, 272 bytes, Stack size 12 bytes, app_timer.o(.text), UNUSED)

  app_timer_cnt_get (Thumb, 10 bytes, Stack size 0 bytes, app_timer.o(.text), UNUSED)

  app_timer_cnt_diff_compute (Thumb, 12 bytes, Stack size 0 bytes, app_timer.o(.text), UNUSED)

  softdevice_assertion_handler (Thumb, 12 bytes, Stack size 8 bytes, softdevice_handler.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = softdevice_assertion_handler
  [Calls]
  - >> assert_nrf_callback
  [Address Reference Count : 1]
  - softdevice_handler.o(.text)

  intern_softdevice_events_execute (Thumb, 124 bytes, Stack size 24 bytes, softdevice_handler.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = intern_softdevice_events_execute
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> SWI2_IRQHandler

  softdevice_handler_init (Thumb, 48 bytes, Stack size 8 bytes, softdevice_handler.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = softdevice_handler_init
  [Called By]
  - >> main

  softdevice_handler_sd_disable (Thumb, 18 bytes, Stack size 0 bytes, softdevice_handler.o(.text), UNUSED)

  softdevice_ble_evt_handler_set (Thumb, 16 bytes, Stack size 0 bytes, softdevice_handler.o(.text))
  [Called By]

  - >> main

  softdevice_sys_evt_handler_set (Thumb, 16 bytes, Stack size 0 bytes, softdevice_handler.o(.text))
  [Called By]

  - >> main

  SWI2_IRQHandler (Thumb, 34 bytes, Stack size 8 bytes, softdevice_handler.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = SWI2_IRQHandler ⇒ intern_softdevice_events_execute
  [Calls]
  - >> app_error_handler
  - >> intern_softdevice_events_execute
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  ble_bondmngr_on_ble_evt (Thumb, 982 bytes, Stack size 32 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 168
  - Call Chain = ble_bondmngr_on_ble_evt ⇒ bond_info_store ⇒ pstorage_store ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ swap_state_process
  [Calls]
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy
  - >> __aeabi_memcpy4
  - >> memcmp
  - >> update_whitelist
  - >> bond_info_store
  [Called By]
  - >> ble_evt_dispatch

  ble_bondmngr_bonded_centrals_store (Thumb, 478 bytes, Stack size 32 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 168
  - Call Chain = ble_bondmngr_bonded_centrals_store ⇒ bond_info_store ⇒ pstorage_store ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ swap_state_process
  [Calls]
  - >> __aeabi_memcpy4
  - >> pstorage_store
  - >> pstorage_clear
  - >> pstorage_block_identifier_get
  - >> crc16_compute
  - >> update_whitelist
  - >> bond_info_store
  [Called By]
  - >> ble_evt_dispatch

  ble_bondmngr_sys_attr_store (Thumb, 84 bytes, Stack size 24 bytes, ble_bondmngr.o(.text), UNUSED)
  [Calls]

  - >> sys_attr_store

  ble_bondmngr_bonded_centrals_delete (Thumb, 52 bytes, Stack size 8 bytes, ble_bondmngr.o(.text), UNUSED)
  [Calls]

  - >> pstorage_clear

  ble_bondmngr_central_addr_get (Thumb, 54 bytes, Stack size 8 bytes, ble_bondmngr.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memcpy

  ble_bondmngr_whitelist_get (Thumb, 386 bytes, Stack size 24 bytes, ble_bondmngr.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_uidivmod

  ble_bondmngr_init (Thumb, 602 bytes, Stack size 120 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 224
  - Call Chain = ble_bondmngr_init ⇒ pstorage_clear ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ swap_state_process
  [Calls]
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy4
  - >> pstorage_register
  - >> pstorage_load
  - >> pstorage_clear
  - >> pstorage_block_identifier_get
  - >> crc16_compute
  - >> update_whitelist
  [Called By]
  - >> main

  ble_bondmngr_central_ids_get (Thumb, 72 bytes, Stack size 8 bytes, ble_bondmngr.o(.text), UNUSED)

  ble_bondmngr_bonded_central_delete (Thumb, 400 bytes, Stack size 32 bytes, ble_bondmngr.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memclr4
  - >> __aeabi_memcpy4
  - >> pstorage_store
  - >> pstorage_clear
  - >> pstorage_block_identifier_get
  - >> crc16_compute
  - >> update_whitelist
  - >> bond_info_store

  ble_bondmngr_is_link_encrypted (Thumb, 24 bytes, Stack size 0 bytes, ble_bondmngr.o(.text), UNUSED)

  pstorage_sys_event_handler (Thumb, 268 bytes, Stack size 24 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = pstorage_sys_event_handler ⇒ cmd_process ⇒ swap_state_process
  [Calls]
  - >> app_notify
  - >> cmd_process
  [Called By]
  - >> sys_evt_dispatch

  pstorage_init (Thumb, 160 bytes, Stack size 24 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = pstorage_init
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> main

  pstorage_register (Thumb, 228 bytes, Stack size 24 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = pstorage_register
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> ble_bondmngr_init

  pstorage_block_identifier_get (Thumb, 84 bytes, Stack size 12 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = pstorage_block_identifier_get
  [Called By]
  - >> ble_bondmngr_init
  - >> ble_bondmngr_bonded_centrals_store
  - >> ble_bondmngr_bonded_central_delete
  - >> sys_attr_store
  - >> bond_info_store

  pstorage_store (Thumb, 110 bytes, Stack size 24 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = pstorage_store ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ swap_state_process
  [Calls]
  - >> cmd_queue_enqueue
  [Called By]
  - >> ble_bondmngr_bonded_centrals_store
  - >> ble_bondmngr_bonded_central_delete
  - >> sys_attr_store
  - >> bond_info_store

  pstorage_update (Thumb, 110 bytes, Stack size 24 bytes, pstorage.o(.text), UNUSED)
  [Calls]

  - >> cmd_queue_enqueue

  pstorage_load (Thumb, 104 bytes, Stack size 16 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = pstorage_load ⇒ __aeabi_memcpy
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> ble_bondmngr_init

  pstorage_clear (Thumb, 100 bytes, Stack size 16 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = pstorage_clear ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ swap_state_process
  [Calls]
  - >> __aeabi_uidivmod
  - >> cmd_queue_enqueue
  [Called By]
  - >> ble_bondmngr_init
  - >> ble_bondmngr_bonded_centrals_store
  - >> ble_bondmngr_bonded_central_delete
  - >> ble_bondmngr_bonded_centrals_delete

  pstorage_access_status_get (Thumb, 30 bytes, Stack size 0 bytes, pstorage.o(.text))
  [Called By]

  - >> sys_evt_dispatch

  crc16_compute (Thumb, 120 bytes, Stack size 0 bytes, crc16.o(.text))
  [Called By]

  - >> ble_bondmngr_init
  - >> ble_bondmngr_bonded_centrals_store
  - >> ble_bondmngr_bonded_central_delete
  - >> sys_attr_store
  - >> bond_info_store

  app_button_init (Thumb, 98 bytes, Stack size 24 bytes, app_button.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = app_button_init ⇒ app_gpiote_user_register
  [Calls]
  - >> app_timer_create
  - >> app_gpiote_user_register
  [Called By]
  - >> main

  app_button_enable (Thumb, 22 bytes, Stack size 8 bytes, app_button.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = app_button_enable ⇒ app_gpiote_user_enable
  [Calls]
  - >> app_gpiote_user_enable
  [Called By]
  - >> ble_evt_dispatch

  app_button_disable (Thumb, 32 bytes, Stack size 8 bytes, app_button.o(.text), UNUSED)
  [Calls]

  - >> app_timer_stop
  - >> app_gpiote_user_disable

  app_button_is_pushed (Thumb, 80 bytes, Stack size 24 bytes, app_button.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = app_button_is_pushed
  [Calls]
  - >> app_gpiote_pins_state_get
  [Called By]
  - >> main

  GPIOTE_IRQHandler (Thumb, 270 bytes, Stack size 32 bytes, app_gpiote.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = GPIOTE_IRQHandler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  app_gpiote_init (Thumb, 76 bytes, Stack size 8 bytes, app_gpiote.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = app_gpiote_init
  [Calls]
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  app_gpiote_user_register (Thumb, 118 bytes, Stack size 16 bytes, app_gpiote.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = app_gpiote_user_register
  [Called By]
  - >> app_button_init

  app_gpiote_user_enable (Thumb, 138 bytes, Stack size 16 bytes, app_gpiote.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = app_gpiote_user_enable
  [Called By]
  - >> app_button_enable

  app_gpiote_user_disable (Thumb, 98 bytes, Stack size 16 bytes, app_gpiote.o(.text), UNUSED)
  [Called By]

  - >> app_button_disable

  app_gpiote_pins_state_get (Thumb, 42 bytes, Stack size 0 bytes, app_gpiote.o(.text))
  [Called By]

  - >> app_button_is_pushed
  - >> detection_delay_timeout_handler

  memcmp (Thumb, 90 bytes, Stack size 8 bytes, memcmp.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = memcmp
  [Called By]
  - >> ble_bondmngr_on_ble_evt

  strlen (Thumb, 62 bytes, Stack size 12 bytes, strlen.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = strlen
  [Called By]
  - >> ble_srv_ascii_to_utf8

  __aeabi_memcpy (Thumb, 130 bytes, Stack size 24 bytes, rt_memcpy.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = __aeabi_memcpy
  [Calls]
  - >> __aeabi_memcpy4
  [Called By]
  - >> adv_data_encode
  - >> ble_bondmngr_on_ble_evt
  - >> __aeabi_memmove
  - >> pstorage_load
  - >> ble_bondmngr_central_addr_get

  __rt_memcpy (Thumb, 0 bytes, Stack size 24 bytes, rt_memcpy.o(.text), UNUSED)

  __aeabi_memmove4 (Thumb, 70 bytes, Stack size 16 bytes, rt_memmove.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_memmove4
  [Calls]
  - >> __aeabi_memcpy4
  [Called By]
  - >> __aeabi_memmove

  __aeabi_memmove8 (Thumb, 0 bytes, Stack size 16 bytes, rt_memmove.o(.text), UNUSED)

  __aeabi_memmove (Thumb, 80 bytes, Stack size 24 bytes, rt_memmove.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = __aeabi_memmove ⇒ __aeabi_memcpy
  [Calls]
  - >> __aeabi_memmove4
  - >> __aeabi_memcpy
  [Called By]
  - >> ble_hrs_rr_interval_add
  - >> hrm_encode

  __rt_memmove (Thumb, 0 bytes, Stack size 24 bytes, rt_memmove.o(.text), UNUSED)

  _memset_w (Thumb, 26 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)
  [Called By]

  - >> __rt_memclr_w
  - >> _memset

  _memset (Thumb, 30 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)
  [Calls]

  - >> _memset_w
  [Called By]
  - >> __aeabi_memclr

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)
  [Calls]

  - >> _memset

  __rt_memclr (Thumb, 0 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, rt_memclr.o(.text))
  [Called By]

  - >> ble_bondmngr_on_ble_evt
  - >> ble_bondmngr_init
  - >> app_gpiote_init
  - >> main
  - >> ble_bondmngr_bonded_central_delete

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)

  __rt_memclr_w (Thumb, 4 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)
  [Calls]

  - >> _memset_w

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 0 bytes, aeabi_sdivfast.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 28 bytes, Stack size 0 bytes, aeabi_sdivfast.o(.text))
  [Called By]

  - >> ADC_IRQHandler
  - >> pstorage_init
  - >> cmd_process
  - >> swap_state_process
  - >> pstorage_register
  - >> pstorage_clear
  - >> ble_bondmngr_whitelist_get

  __aeabi_idiv (Thumb, 0 bytes, Stack size 8 bytes, aeabi_sdivfast.o(.text), UNUSED)

  __aeabi_idivmod (Thumb, 460 bytes, Stack size 8 bytes, aeabi_sdivfast.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_idivmod
  [Called By]
  - >> ADC_IRQHandler

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 62 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  - >> _call_atexit_fns (Weak Reference)
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  ### Local Symbols

  conn_params_error_handler (Thumb, 16 bytes, Stack size 0 bytes, main.o(.text))
  [Address Reference Count : 1]

  - main.o(.text)

  bond_manager_error_handler (Thumb, 16 bytes, Stack size 0 bytes, main.o(.text))
  [Address Reference Count : 1]

  - main.o(.text)

  battery_level_meas_timeout_handler (Thumb, 8 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = battery_level_meas_timeout_handler ⇒ battery_start
  [Calls]
  - >> battery_start
  [Address Reference Count : 1]
  - main.o(.text)

  heart_rate_meas_timeout_handler (Thumb, 50 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = heart_rate_meas_timeout_handler ⇒ ble_hrs_heart_rate_measurement_send ⇒ hrm_encode ⇒ __aeabi_memmove ⇒ __aeabi_memcpy
  [Calls]
  - >> ble_hrs_heart_rate_measurement_send
  [Address Reference Count : 1]
  - main.o(.text)

  button_event_handler (Thumb, 68 bytes, Stack size 0 bytes, main.o(.text))
  [Address Reference Count : 1]

  - main.o(.data)

  sys_evt_dispatch (Thumb, 54 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = sys_evt_dispatch ⇒ pstorage_sys_event_handler ⇒ cmd_process ⇒ swap_state_process
  [Calls]
  - >> pstorage_sys_event_handler
  - >> pstorage_access_status_get
  [Address Reference Count : 1]
  - main.o(.text)

  ble_evt_dispatch (Thumb, 242 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 192
  - Call Chain = ble_evt_dispatch ⇒ ble_bondmngr_on_ble_evt ⇒ bond_info_store ⇒ pstorage_store ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ swap_state_process
  [Calls]
  - >> led_stop
  - >> ble_hrs_on_ble_evt
  - >> ble_conn_params_on_ble_evt
  - >> ble_bondmngr_on_ble_evt
  - >> ble_bondmngr_bonded_centrals_store
  - >> ble_bas_on_ble_evt
  - >> app_timer_start
  - >> app_button_enable
  [Address Reference Count : 1]
  - main.o(.text)

  char_add (Thumb, 142 bytes, Stack size 80 bytes, ble_dis.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = char_add
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> ble_dis_init

  hrm_encode (Thumb, 140 bytes, Stack size 32 bytes, ble_hrs.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = hrm_encode ⇒ __aeabi_memmove ⇒ __aeabi_memcpy
  [Calls]
  - >> __aeabi_memmove
  [Called By]
  - >> ble_hrs_init
  - >> ble_hrs_heart_rate_measurement_send

  update_timeout_handler (Thumb, 86 bytes, Stack size 16 bytes, ble_conn_params.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = update_timeout_handler
  [Address Reference Count : 1]
  - ble_conn_params.o(.text)

  conn_params_negotiation (Thumb, 96 bytes, Stack size 24 bytes, ble_conn_params.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = conn_params_negotiation ⇒ app_timer_start
  [Calls]
  - >> app_timer_start
  [Called By]
  - >> ble_conn_params_on_ble_evt

  uuid_list_encode (Thumb, 328 bytes, Stack size 56 bytes, ble_advdata.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = uuid_list_encode
  [Called By]
  - >> adv_data_encode

  adv_data_encode (Thumb, 742 bytes, Stack size 40 bytes, ble_advdata.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = adv_data_encode ⇒ uuid_list_encode
  [Calls]
  - >> uuid_list_encode
  - >> __aeabi_memcpy
  [Called By]
  - >> ble_advdata_set

  timer_list_handler (Thumb, 894 bytes, Stack size 104 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = timer_list_handler
  [Calls]
  - >> __asm___11_app_timer_c_cd27f9c3__nrf_delay_us
  [Called By]
  - >> SWI0_IRQHandler

  bond_info_store (Thumb, 118 bytes, Stack size 24 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = bond_info_store ⇒ pstorage_store ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ swap_state_process
  [Calls]
  - >> pstorage_store
  - >> pstorage_block_identifier_get
  - >> crc16_compute
  [Called By]
  - >> ble_bondmngr_on_ble_evt
  - >> ble_bondmngr_bonded_centrals_store
  - >> ble_bondmngr_bonded_central_delete

  update_whitelist (Thumb, 94 bytes, Stack size 16 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = update_whitelist
  [Called By]
  - >> ble_bondmngr_on_ble_evt
  - >> ble_bondmngr_init
  - >> ble_bondmngr_bonded_centrals_store
  - >> ble_bondmngr_bonded_central_delete

  bm_pstorage_cb_handler (Thumb, 12 bytes, Stack size 0 bytes, ble_bondmngr.o(.text))
  [Address Reference Count : 1]

  - ble_bondmngr.o(.text)

  sys_attr_store (Thumb, 118 bytes, Stack size 24 bytes, ble_bondmngr.o(.text), UNUSED)
  [Calls]

  - >> pstorage_store
  - >> pstorage_block_identifier_get
  - >> crc16_compute
  [Called By]
  - >> ble_bondmngr_sys_attr_store

  swap_state_process (Thumb, 384 bytes, Stack size 40 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = swap_state_process
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> cmd_process

  cmd_process (Thumb, 232 bytes, Stack size 24 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = cmd_process ⇒ swap_state_process
  [Calls]
  - >> __aeabi_uidivmod
  - >> swap_state_process
  [Called By]
  - >> pstorage_sys_event_handler
  - >> cmd_queue_enqueue

  cmd_queue_enqueue (Thumb, 78 bytes, Stack size 24 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = cmd_queue_enqueue ⇒ cmd_process ⇒ swap_state_process
  [Calls]
  - >> cmd_process
  [Called By]
  - >> pstorage_update
  - >> pstorage_store
  - >> pstorage_clear

  app_notify (Thumb, 36 bytes, Stack size 16 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = app_notify
  [Called By]
  - >> pstorage_sys_event_handler

  detection_delay_timeout_handler (Thumb, 196 bytes, Stack size 24 bytes, app_button.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = detection_delay_timeout_handler
  [Calls]
  - >> app_error_handler
  - >> app_gpiote_pins_state_get
  [Address Reference Count : 1]
  - app_button.o(.text)

  gpiote_event_handler (Thumb, 38 bytes, Stack size 16 bytes, app_button.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = gpiote_event_handler ⇒ app_timer_stop
  [Calls]
  - >> app_timer_stop
  - >> app_timer_start
  [Address Reference Count : 1]
  - app_button.o(.text)

  ### Undefined Global Symbols

  _call_atexit_fns (ARM, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> exit