nRF51 SDK: ble_gattc_write_params_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gattc_write_params_t Struct Reference
Generic Attribute Profile (GATT) Client | Structures | Generic Attribute Profile (GATT) Client

Write Parameters. More...

`#include <ble_gattc.h>`

## Data Fields

uint8_t | write_op
uint16_t | handle
uint16_t | offset
uint16_t | len
uint8_t * | p_value
uint8_t | flags

## Detailed Description

Write Parameters.

## Field Documentation

uint8_t ble_gattc_write_params_t::flags

Flags, see BLE_GATT_EXEC_WRITE_FLAGS.

uint16_t ble_gattc_write_params_t::handle

Handle to the attribute to be written.

uint16_t ble_gattc_write_params_t::len

Length of data in bytes.

uint16_t ble_gattc_write_params_t::offset

Offset in bytes.

Offset in bytes.

Note
  For WRITE_CMD and WRITE_REQ, offset must be 0.

uint8_t * ble_gattc_write_params_t::p_value

Pointer to the value data.

uint8_t ble_gattc_write_params_t::write_op

Write Operation to be performed, see BLE_GATT_WRITE_OPS.

Write Operation to be performed, see BLE_GATT_WRITE_OPS.