nRF51 SDK: nrf_gzll_device_tx_info_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_gzll_device_tx_info_t Struct Reference
Gazell Link Layer

Data structure containing information about the last packet transmission. More...

`#include <nrf_gzll.h>`

## Data Fields

bool | payload_received_in_ack
| A payload was received in the ACK.
uint16_t | num_tx_attempts
| Number of attempts used on previous Device packet transmission.
uint16_t | num_channel_switches
| Number of channel switches needed during previous packet transmission.
int16_t | rssi
| Received signal strength indicator in dBm. More...

## Detailed Description

Data structure containing information about the last packet transmission.

## Field Documentation

int16_t nrf_gzll_device_tx_info_t::rssi

Received signal strength indicator in dBm.

See Also
  nrf_gzll_enable_rssi().