nRF51 SDK: Record Access Control Point

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Structures | Macros | Functions
Record Access Control Point
BLE Libraries

Record Access Control Point library. More...

## Data Structures

struct | ble_racp_value_t
| Record Access Control Point value structure. More...

## Macros

#define | RACP_OPCODE_RESERVED 0
| Record Access Control Point opcodes. More...
#define | RACP_OPCODE_REPORT_RECS 1
#define | RACP_OPCODE_DELETE_RECS 2
#define | RACP_OPCODE_ABORT_OPERATION 3
#define | RACP_OPCODE_REPORT_NUM_RECS 4
#define | RACP_OPCODE_NUM_RECS_RESPONSE 5
#define | RACP_OPCODE_RESPONSE_CODE 6
#define | RACP_OPERATOR_NULL 0
| Record Access Control Point operators. More...
#define | RACP_OPERATOR_ALL 1
#define | RACP_OPERATOR_LESS_OR_EQUAL 2
#define | RACP_OPERATOR_GREATER_OR_EQUAL 3
#define | RACP_OPERATOR_RANGE 4
#define | RACP_OPERATOR_FIRST 5
#define | RACP_OPERATOR_LAST 6
#define | RACP_OPERATOR_RFU_START 7
#define | RACP_RESPONSE_RESERVED 0
| Record Access Control Point response codes. More...
#define | RACP_RESPONSE_SUCCESS 1
#define | RACP_RESPONSE_OPCODE_UNSUPPORTED 2
#define | RACP_RESPONSE_INVALID_OPERATOR 3
#define | RACP_RESPONSE_OPERATOR_UNSUPPORTED 4
#define | RACP_RESPONSE_INVALID_OPERAND 5
#define | RACP_RESPONSE_NO_RECORDS_FOUND 6
#define | RACP_RESPONSE_ABORT_FAILED 7
#define | RACP_RESPONSE_PROCEDURE_NOT_DONE 8
#define | RACP_RESPONSE_OPERAND_UNSUPPORTED 9

## Functions

void | ble_racp_decode (uint8_t data_len, uint8_t *p_data, ble_racp_value_t *p_racp_val)
| Function for decoding a Record Access Control Point write. More...
uint8_t | ble_racp_encode (const ble_racp_value_t *p_racp_val, uint8_t *p_data)
| Function for encoding a Record Access Control Point response. More...

## Detailed Description

Record Access Control Point library.

## Macro Definition Documentation

#define RACP_OPCODE_ABORT_OPERATION 3

Record Access Control Point opcode - Abort operation.

#define RACP_OPCODE_DELETE_RECS 2

Record Access Control Point opcode - Delete stored records.

#define RACP_OPCODE_NUM_RECS_RESPONSE 5

Record Access Control Point opcode - Number of stored records response.

#define RACP_OPCODE_REPORT_NUM_RECS 4

Record Access Control Point opcode - Report number of stored records.

#define RACP_OPCODE_REPORT_RECS 1

Record Access Control Point opcode - Report stored records.

#define RACP_OPCODE_RESERVED 0

Record Access Control Point opcodes.

Record Access Control Point opcode - Reserved for future use.

#define RACP_OPCODE_RESPONSE_CODE 6

Record Access Control Point opcode - Response code.

#define RACP_OPERATOR_ALL 1

Record Access Control Point operator - All records.

#define RACP_OPERATOR_FIRST 5

Record Access Control Point operator - First record (i.e. oldest record).

#define RACP_OPERATOR_GREATER_OR_EQUAL 3

Record Access Control Point operator - Greater than or equal to.

#define RACP_OPERATOR_LAST 6

Record Access Control Point operator - Last record (i.e. most recent record).

#define RACP_OPERATOR_LESS_OR_EQUAL 2

Record Access Control Point operator - Less than or equal to.

#define RACP_OPERATOR_NULL 0

Record Access Control Point operators.

Record Access Control Point operator - Null.

#define RACP_OPERATOR_RANGE 4

Record Access Control Point operator - Within range of (inclusive).

#define RACP_OPERATOR_RFU_START 7

Record Access Control Point operator - Start of Reserved for Future Use area.

#define RACP_RESPONSE_ABORT_FAILED 7

Record Access Control Point response code - Abort could not be completed.

#define RACP_RESPONSE_INVALID_OPERAND 5

Record Access Control Point response code - Operand not valid for service.

#define RACP_RESPONSE_INVALID_OPERATOR 3

Record Access Control Point response code - Operator not valid for service.

#define RACP_RESPONSE_NO_RECORDS_FOUND 6

Record Access Control Point response code - No matching records found.

#define RACP_RESPONSE_OPCODE_UNSUPPORTED 2

Record Access Control Point response code - Unsupported op code received.

#define RACP_RESPONSE_OPERAND_UNSUPPORTED 9

Record Access Control Point response code - Unsupported operand.

#define RACP_RESPONSE_OPERATOR_UNSUPPORTED 4

Record Access Control Point response code - Unsupported operator.

#define RACP_RESPONSE_PROCEDURE_NOT_DONE 8

Record Access Control Point response code - Procedure could not be completed.

#define RACP_RESPONSE_RESERVED 0

Record Access Control Point response codes.

Record Access Control Point response code - Reserved for future use.

#define RACP_RESPONSE_SUCCESS 1

Record Access Control Point response code - Successful operation.

## Function Documentation

void ble_racp_decode | ( | uint8_t | data_len,
|  | uint8_t * | p_data,
|  | ble_racp_value_t * | p_racp_val
| ) |  |

Function for decoding a Record Access Control Point write.

This call decodes a write to the Record Access Control Point.

Parameters

  [in] | data_len | Length of data in received write.
  [in] | p_data | Pointer to received data.
  [out] | p_racp_val | Pointer to decoded Record Access Control Point write.

Note
  This does not do a data copy. It assumes the data pointed to by p_data is persistant until no longer needed.

uint8_t ble_racp_encode | ( | const ble_racp_value_t * | p_racp_val,
|  | uint8_t * | p_data
| ) |  |

Function for encoding a Record Access Control Point response.

This call encodes a response from the Record Access Control Point response.

Parameters

  [in] | p_racp_val | Pointer to Record Access Control Point to encode.
  [out] | p_data | Pointer to where encoded data is written. NOTE! It is calling routines respsonsibility to make sure.

Returns
  Length of encoded data.