nRF51 SDK: Module specific SVC and event number subranges

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
Module specific SVC and event number subranges
BLE SoftDevice Common

Definition of SVC and event number subranges for each API module. More...

## Macros

#define | BLE_SVC_BASE 0x60
#define | BLE_SVC_LAST 0x6B /* Total: 12. */
#define | BLE_RESERVED_SVC_BASE 0x6C
#define | BLE_RESERVED_SVC_LAST 0x6F /* Total: 4. */
#define | BLE_GAP_SVC_BASE 0x70
#define | BLE_GAP_SVC_LAST 0x8F /* Total: 32. */
#define | BLE_GATTC_SVC_BASE 0x90
#define | BLE_GATTC_SVC_LAST 0x9F /* Total: 16. */
#define | BLE_GATTS_SVC_BASE 0xA0
#define | BLE_GATTS_SVC_LAST 0xAF /* Total: 16. */
#define | BLE_L2CAP_SVC_BASE 0xB0
#define | BLE_L2CAP_SVC_LAST 0xBF /* Total: 16. */
#define | BLE_EVT_INVALID 0x00
#define | BLE_EVT_BASE 0x01
#define | BLE_EVT_LAST 0x0F /* Total: 15. */
#define | BLE_GAP_EVT_BASE 0x10
#define | BLE_GAP_EVT_LAST 0x2F /* Total: 32. */
#define | BLE_GATTC_EVT_BASE 0x30
#define | BLE_GATTC_EVT_LAST 0x4F /* Total: 32. */
#define | BLE_GATTS_EVT_BASE 0x50
#define | BLE_GATTS_EVT_LAST 0x6F /* Total: 32. */
#define | BLE_L2CAP_EVT_BASE 0x70
#define | BLE_L2CAP_EVT_LAST 0x8F /* Total: 32. */

## Detailed Description

Definition of SVC and event number subranges for each API module.

Note
  SVCs and event numbers are split into subranges for each API module. Each module receives its entire allocated range of SVC calls, whether implemented or not, but return BLE_ERROR_NOT_SUPPORTED for unimplemented or undefined calls in its range.

Note that the symbols BLE_<module>_SVC_LAST is the end of the allocated SVC range, rather than the last SVC function call actually defined and implemented.

Specific SVC and event values are defined in each module's ble_<module>.h file, which defines names of each individual SVC code based on the range start value.