#

##

##

    礦ision Build Log
    Project:
    F:\资料包\code\BLE4.0\nrf51822\Board\pca10001\06 s110\ble_app_proximity\arm\ble_app_proximity.uvproj
    Project File Date:  07/16/2014

    Output:
    Build target 'nrf51822_xxaa_s110 (256K)'
    linking...
    Program Size: Code=16860 RO-data=236 RW-data=228 ZI-data=6876
    FromELF: creating hex file...
    ".\_build\ble_app_proximity.axf" - 0 Errors, 0 Warning(s).
    Load "F:\\资料包\\code\\BLE4.0\\nrf51822\\Board\\pca10001\\06 s110\\ble_app_proximity\\arm\\_build\\ble_app_proximity.axf"
    Set JLink Project File to "F:\资料包\code\BLE4.0\nrf51822\Board\pca10001\06 s110\ble_app_proximity\arm\JLinkSettings.ini"
    * JLink Info: Device "NRF51822_XXAA" selected (257 KB flash, 8 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 235586136
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x0BB11477
    * JLink Info: FPUnit: 4 code (BP) slots and 0 literal slots
    * JLink Info: Found Cortex-M0 r0p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: nRF51822_xxAA
    VTarget = 3.384V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 8192
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'nrf51822_xxaa_s110 (256K)'
    linking...
    Program Size: Code=16860 RO-data=236 RW-data=228 ZI-data=6876
    FromELF: creating hex file...
    ".\_build\ble_app_proximity.axf" - 0 Errors, 0 Warning(s).
    Load "F:\\资料包\\code\\BLE4.0\\nrf51822\\Board\\pca10001\\06 s110\\ble_app_proximity\\arm\\_build\\ble_app_proximity.axf"
    Set JLink Project File to "F:\资料包\code\BLE4.0\nrf51822\Board\pca10001\06 s110\ble_app_proximity\arm\JLinkSettings.ini"
    * JLink Info: Device "NRF51822_XXAA" selected (257 KB flash, 8 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 235586136
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x0BB11477
    * JLink Info: FPUnit: 4 code (BP) slots and 0 literal slots
    * JLink Info: Found Cortex-M0 r0p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: nRF51822_xxAA
    VTarget = 3.384V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 8192
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Load "F:\\资料包\\code\\BLE4.0\\nrf51822\\Board\\pca10001\\06 s110\\ble_app_proximity\\arm\\_build\\ble_app_proximity.axf"
    Set JLink Project File to "F:\资料包\code\BLE4.0\nrf51822\Board\pca10001\06 s110\ble_app_proximity\arm\JLinkSettings.ini"
    * JLink Info: Device "NRF51822_XXAA" selected (257 KB flash, 8 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 235586136
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x0BB11477
    * JLink Info: FPUnit: 4 code (BP) slots and 0 literal slots
    * JLink Info: Found Cortex-M0 r0p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: nRF51822_xxAA
    VTarget = 3.338V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 0, TMS: 1, TRES: 1, TRST: 0
    Hardware-Breakpoints: 4
    Software-Breakpoints: 8192
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Load "F:\\资料包\\code\\BLE4.0\\nrf51822\\Board\\pca10001\\06 s110\\ble_app_proximity\\arm\\_build\\ble_app_proximity.axf"
    Set JLink Project File to "F:\资料包\code\BLE4.0\nrf51822\Board\pca10001\06 s110\ble_app_proximity\arm\JLinkSettings.ini"
    * JLink Info: Device "NRF51822_XXAA" selected (257 KB flash, 8 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 235586136
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x0BB11477
    * JLink Info: FPUnit: 4 code (BP) slots and 0 literal slots
    * JLink Info: Found Cortex-M0 r0p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: nRF51822_xxAA
    VTarget = 3.338V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 0, TMS: 1, TRES: 1, TRST: 0
    Hardware-Breakpoints: 4
    Software-Breakpoints: 8192
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Load "F:\\资料包\\code\\BLE4.0\\nrf51822\\Board\\pca10001\\06 s110\\ble_app_proximity\\arm\\_build\\ble_app_proximity.axf"
    Set JLink Project File to "F:\资料包\code\BLE4.0\nrf51822\Board\pca10001\06 s110\ble_app_proximity\arm\JLinkSettings.ini"
    * JLink Info: Device "NRF51822_XXAA" selected (257 KB flash, 8 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 235586136
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x0BB11477
    * JLink Info: FPUnit: 4 code (BP) slots and 0 literal slots
    * JLink Info: Found Cortex-M0 r0p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: nRF51822_xxAA
    VTarget = 3.377V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 8192
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...