nRF51 SDK: ble_advdata_conn_int_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_advdata_conn_int_t Struct Reference
Advertising Data Encoder

Connection interval range structure. More...

`#include <ble_advdata.h>`

## Data Fields

uint16_t | min_conn_interval
uint16_t | max_conn_interval

## Detailed Description

Connection interval range structure.

## Field Documentation

uint16_t ble_advdata_conn_int_t::max_conn_interval

Maximum Connection Interval, in units of 1.25ms, range 6 to 3200 (i.e. 7.5ms to 4s). Value of 0xFFFF indicates no specific maximum.

uint16_t ble_advdata_conn_int_t::min_conn_interval

Minimum Connection Interval, in units of 1.25ms, range 6 to 3200 (i.e. 7.5ms to 4s).