nRF51 SDK: ble_gattc_handle_value_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gattc_handle_value_t Struct Reference
Generic Attribute Profile (GATT) Client | Structures | Generic Attribute Profile (GATT) Client

GATT read by UUID handle value pair. More...

`#include <ble_gattc.h>`

## Data Fields

uint16_t | handle
uint8_t * | p_value

## Detailed Description

GATT read by UUID handle value pair.

## Field Documentation

uint16_t ble_gattc_handle_value_t::handle

Attribute Handle.

uint8_t * ble_gattc_handle_value_t::p_value

           Pointer to value, variable length (length available as value_len in ble_gattc_evt_read_by_uuid_rsp_t).

Please note that this pointer is absolute to the memory provided by the user when retrieving the event, so it will effectively point to a location inside the handle_value array.