nRF51 SDK: TX Power Service

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
TX Power Service

This module implements the TX Power Service with the TX Power Level characteristic. During initialization it adds the TX Power Service and TX Power Level characteristic with the specified initial value to the BLE stack database.

It provides a function for letting the application update the TX Power Level characteristic.