nRF51 SDK: ble_gap_evt_sec_info_request_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_evt_sec_info_request_t Struct Reference
Generic Access Profile (GAP) | Structures | Generic Access Profile (GAP)

Event data for securito info request event. More...

`#include <ble_gap.h>`

## Data Fields

ble_gap_addr_t | peer_addr
uint16_t | div
uint8_t | enc_info: 1
uint8_t | id_info: 1
uint8_t | sign_info: 1
ble_gap_master_id_t | master_id

## Detailed Description

Event data for securito info request event.

Event data for security info request event.

## Field Documentation

uint16_t ble_gap_evt_sec_info_request_t::div

Encryption diversifier for LTK lookup.

uint8_t ble_gap_evt_sec_info_request_t::enc_info

If 1, Encryption Information required.

uint8_t ble_gap_evt_sec_info_request_t::id_info

If 1, Identity Information required.

ble_gap_master_id_t ble_gap_evt_sec_info_request_t::master_id

Master Identification for LTK lookup.

ble_gap_addr_t ble_gap_evt_sec_info_request_t::peer_addr

Bluetooth address of the peer device.

uint8_t ble_gap_evt_sec_info_request_t::sign_info

If 1, Signing Information required.