nRF51 SDK: GAP Advertising interval max and min

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Advertising interval max and min
Defines

## Macros

#define | BLE_GAP_ADV_INTERVAL_MIN 0x0020
#define | BLE_GAP_ADV_NONCON_INTERVAL_MIN 0x00A0
#define | BLE_GAP_ADV_INTERVAL_MAX 0x4000

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_ADV_INTERVAL_MAX 0x4000

Maximum Advertising interval in 625 us units, i.e. 10.24 s.

#define BLE_GAP_ADV_INTERVAL_MIN 0x0020

Minimum Advertising interval in 625 us units, i.e. 20 ms.

#define BLE_GAP_ADV_NONCON_INTERVAL_MIN 0x00A0

Minimum Advertising interval in 625 us units for non connectable mode, i.e. 100 ms.