nRF51 SDK: ble_gap_whitelist_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_whitelist_t Struct Reference
Generic Access Profile (GAP) | Structures | Generic Access Profile (GAP)

Whitelist structure. More...

`#include <ble_gap.h>`

## Data Fields

ble_gap_addr_t ** | pp_addrs
uint8_t | addr_count
ble_gap_irk_t ** | pp_irks
uint8_t | irk_count

## Detailed Description

Whitelist structure.

## Field Documentation

uint8_t ble_gap_whitelist_t::addr_count

Count of device addresses in array, up to BLE_GAP_WHITELIST_ADDR_MAX_COUNT.

uint8_t ble_gap_whitelist_t::irk_count

Count of IRKs in array, up to BLE_GAP_WHITELIST_IRK_MAX_COUNT.

ble_gap_addr_t ** ble_gap_whitelist_t::pp_addrs

Pointer to array of device address pointers, pointing to addresses to be used in whitelist. NULL if none are given.

ble_gap_irk_t ** ble_gap_whitelist_t::pp_irks

Pointer to array of Identity Resolving Key (IRK) pointers, each pointing to an IRK in the whitelist. NULL if none are given.