nRF51 SDK: ble_gap_conn_sec_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_conn_sec_t Struct Reference
Generic Access Profile (GAP) | Structures | Generic Access Profile (GAP)

GAP connection security status. More...

`#include <ble_gap.h>`

## Data Fields

ble_gap_conn_sec_mode_t | sec_mode
uint8_t | encr_key_size

## Detailed Description

GAP connection security status.

## Field Documentation

uint8_t ble_gap_conn_sec_t::encr_key_size

Length of currently active encryption key, 7 to 16 octets.

ble_gap_conn_sec_mode_t ble_gap_conn_sec_t::sec_mode

Currently active security mode for this connection.