#

##

##

    礦ision Build Log
    Project:
    F:\资料包\code\BLE4.0\nrf51822\Board\pca10001\03 at45dbxx_example\arm\uart_example.uvproj
    Project File Date:  08/23/2014

    Output:
    Build target 'nrf51822_xxaa (256K)'
    Clean started - Project: 'uart_example'
       deleting intermediate output files for target 'nrf51822_xxaa (256K)'
    compiling main.c...
    compiling AT45DBXX.c...
    compiling system_nrf51.c...
    assembling startup_arm_nrf51.s...
    compiling simple_uart.c...
    compiling spi_master.c...
    compiling nrf_delay.c...
    linking...
    Program Size: Code=1220 RO-data=208 RW-data=4 ZI-data=2052
    ".\_build\uart_example_arm.axf" - 0 Errors, 0 Warning(s).

    *** Performing Cross-Module-Optimization:
    compiling main.c...
    compiling system_nrf51.c...
    compiling simple_uart.c...
    compiling spi_master.c...
    compiling nrf_delay.c...
    linking...
    Program Size: Code=1220 RO-data=208 RW-data=4 ZI-data=2052
    FromELF: creating hex file...
    ".\_build\uart_example_arm.axf" - 0 Errors, 0 Warning(s).
    *** Completed Cross-Module-Optimization after 2 iteration(s).
    Load "F:\\资料包\\code\\BLE4.0\\nrf51822\\Board\\pca10001\\03 at45dbxx_example\\arm\\_build\\uart_example_arm.axf"
    Set JLink Project File to "F:\资料包\code\BLE4.0\nrf51822\Board\pca10001\03 at45dbxx_example\arm\JLinkSettings.ini"
    * JLink Info: Device "NRF51822_XXAA" selected (257 KB flash, 8 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 235586136
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x0BB11477
    * JLink Info: FPUnit: 4 code (BP) slots and 0 literal slots
    * JLink Info: Found Cortex-M0 r0p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: nRF51822_xxAA
    VTarget = 3.384V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 8192
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...