nRF51 SDK: Running Speed and Cadence Service

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Running Speed and Cadence Service

This module implements the Running Speed and Cadence Service. If enabled, notification of the Running Speead and Candence Measurement is performed when the application calls ble_rscs_measurement_send().

If an event handler is supplied by the application, the Running Speed and Cadence Service will generate Running Speed and Cadence Service events to the application.

Note
  The application must propagate BLE stack events to the Running Speead and Candence Service module by calling ble_rscs_on_ble_evt() from the from the ble_stack_handler function.