nRF51 SDK: Defines

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Modules | Macros
Defines
Generic Access Profile (GAP)

## Modules

| SVC return values specific to GAP
| GAP Roles
| GAP Timeout sources
| GAP Address types
| GAP Advertising and Scan Response Data format
| GAP Advertisement Flags
| GAP Advertising interval max and min
| GAP Advertising types
| GAP Advertising filter policies
| GAP Advertising timeout values
| GAP Discovery modes
| GAP IO Capabilities
| GAP Authentication Key Types
| GAP Security status
| GAP Security status sources
| GAP Connection Parameters Limits
| GAP attribute security requirement setters
| GAP Security Modes

## Macros

#define | BLE_GAP_ADDR_LEN 6
| BLE address length.
#define | BLE_GAP_ADV_MAX_SIZE 31
| Maximum size of advertising data in octets.
#define | BLE_GAP_DEVNAME_MAX_LEN 31
| GAP device name maximum length.
#define | BLE_GAP_SEC_KEY_LEN 16
| GAP Security Key Length.
#define | BLE_GAP_WHITELIST_ADDR_MAX_COUNT (8)
| Maximum amount of addresses in a whitelist.
#define | BLE_GAP_WHITELIST_IRK_MAX_COUNT (8)
| Maximum amount of IRKs in a whitelist. More...

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_WHITELIST_IRK_MAX_COUNT (8)

Maximum amount of IRKs in a whitelist.

Note
  The number of IRKs is limited to 8, even if the hardware supports more.