nRF51 SDK: GAP Security status

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Security status
Defines

## Macros

#define | BLE_GAP_SEC_STATUS_SUCCESS 0x00
#define | BLE_GAP_SEC_STATUS_TIMEOUT 0x01
#define | BLE_GAP_SEC_STATUS_PDU_INVALID 0x02
#define | BLE_GAP_SEC_STATUS_PASSKEY_ENTRY_FAILED 0x81
#define | BLE_GAP_SEC_STATUS_OOB_NOT_AVAILABLE 0x82
#define | BLE_GAP_SEC_STATUS_AUTH_REQ 0x83
#define | BLE_GAP_SEC_STATUS_CONFIRM_VALUE 0x84
#define | BLE_GAP_SEC_STATUS_PAIRING_NOT_SUPP 0x85
#define | BLE_GAP_SEC_STATUS_ENC_KEY_SIZE 0x86
#define | BLE_GAP_SEC_STATUS_SMP_CMD_UNSUPPORTED 0x87
#define | BLE_GAP_SEC_STATUS_UNSPECIFIED 0x88
#define | BLE_GAP_SEC_STATUS_REPEATED_ATTEMPTS 0x89
#define | BLE_GAP_SEC_STATUS_INVALID_PARAMS 0x8A

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_SEC_STATUS_AUTH_REQ 0x83

Authentication requirements not met.

#define BLE_GAP_SEC_STATUS_CONFIRM_VALUE 0x84

Confirm value failed.

#define BLE_GAP_SEC_STATUS_ENC_KEY_SIZE 0x86

Encryption key size.

#define BLE_GAP_SEC_STATUS_INVALID_PARAMS 0x8A

Invalid parameters.

#define BLE_GAP_SEC_STATUS_OOB_NOT_AVAILABLE 0x82

Out of Band Key not available.

#define BLE_GAP_SEC_STATUS_PAIRING_NOT_SUPP 0x85

Pairing not supported.

#define BLE_GAP_SEC_STATUS_PASSKEY_ENTRY_FAILED 0x81

Passkey entry failed (user cancelled or other).

#define BLE_GAP_SEC_STATUS_PDU_INVALID 0x02

Invalid PDU received.

#define BLE_GAP_SEC_STATUS_REPEATED_ATTEMPTS 0x89

Too little time elapsed since last attempt.

#define BLE_GAP_SEC_STATUS_SMP_CMD_UNSUPPORTED 0x87

Unsupported SMP command.

#define BLE_GAP_SEC_STATUS_SUCCESS 0x00

Procedure completed with success.

#define BLE_GAP_SEC_STATUS_TIMEOUT 0x01

Procedure timed out.

#define BLE_GAP_SEC_STATUS_UNSPECIFIED 0x88

Unspecified reason.