nRF51 SDK: SLIP handling library

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
SLIP handling library

SLIP layer for supporting packet framing in HCI transport.

This module implements SLIP packet framing as described in the Bluetooth Core Specification 4.0, Volume 4, Part D, Chapter 3 SLIP Layer.

SLIP framing ensures that all packets sent on the UART are framed as: <0xC0> SLIP packet 1 <0xC0> <0xC0> SLIP packet 2 <0xC0>.

The SLIP layer uses events to notify the upper layer when data transmission is complete and when a SLIP packet is received.