nRF51 SDK: ble_bas_s Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_bas_s Struct Reference
Battery Service

Battery Service structure. This contains various status information for the service. More...

`#include <ble_bas.h>`

## Data Fields

ble_bas_evt_handler_t | evt_handler
uint16_t | service_handle
ble_gatts_char_handles_t | battery_level_handles
uint16_t | report_ref_handle
uint8_t | battery_level_last
uint16_t | conn_handle
bool | is_notification_supported

## Detailed Description

Battery Service structure. This contains various status information for the service.

## Field Documentation

ble_gatts_char_handles_t ble_bas_s::battery_level_handles

Handles related to the Battery Level characteristic.

uint8_t ble_bas_s::battery_level_last

Last Battery Level measurement passed to the Battery Service.

uint16_t ble_bas_s::conn_handle

Handle of the current connection (as provided by the BLE stack, is BLE_CONN_HANDLE_INVALID if not in a connection).

ble_bas_evt_handler_t ble_bas_s::evt_handler

Event handler to be called for handling events in the Battery Service.

bool ble_bas_s::is_notification_supported

TRUE if notification of Battery Level is supported.

uint16_t ble_bas_s::report_ref_handle

Handle of the Report Reference descriptor.

uint16_t ble_bas_s::service_handle

Handle of Battery Service (as provided by the BLE stack).