nRF51 SDK: Defines

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Modules | Macros
Defines
Logical Link Control and Adaptation Protocol (L2CAP)

## Modules

| SVC return values specific to L2CAP

## Macros

#define | BLE_L2CAP_MTU_DEF (23)
| Default L2CAP MTU.
#define | BLE_L2CAP_CID_INVALID (0x0000)
| Invalid Channel Identifier.
#define | BLE_L2CAP_CID_DYN_BASE (0x0040)
| Dynamic Channel Identifier base.
#define | BLE_L2CAP_CID_DYN_MAX (8)
| Maximum amount of dynamic CIDs.

## Detailed Description