nRF51 SDK: ble_lls_init_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_lls_init_t Struct Reference
Link Loss Service

Link Loss Service init structure. This contains all options and data needed for initialization of the service. More...

`#include <ble_lls.h>`

## Data Fields

ble_lls_evt_handler_t | evt_handler
ble_srv_error_handler_t | error_handler
uint8_t | initial_alert_level
ble_srv_security_mode_t | lls_attr_md

## Detailed Description

Link Loss Service init structure. This contains all options and data needed for initialization of the service.

## Field Documentation

ble_srv_error_handler_t ble_lls_init_t::error_handler

Function to be called in case of an error.

ble_lls_evt_handler_t ble_lls_init_t::evt_handler

Event handler to be called for handling events in the Link Loss Service.

uint8_t ble_lls_init_t::initial_alert_level

Initial value of the Alert Level characteristic.

ble_srv_security_mode_t ble_lls_init_t::lls_attr_md

Initial Security Setting for Link Loss Service Characteristics.