Configuration	TCS34725_Color_Sensoc
STM32CubeMX 	4.22.1
Date	01/18/2019
MCU	STM32F103RBTx



PERIPHERALS	MODES	FUNCTIONS	PINS
I2C1	I2C	I2C1_SCL	PB8
I2C1	I2C	I2C1_SDA	PB9
RCC	Crystal/Ceramic Resonator	RCC_OSC_IN	PD0-OSC_IN
RCC	Crystal/Ceramic Resonator	RCC_OSC_OUT	PD1-OSC_OUT
SYS	Serial Wire	SYS_JTCK-SWCLK	PA14
SYS	Serial Wire	SYS_JTMS-SWDIO	PA13
SYS	SysTick	SYS_VS_Systick	VP_SYS_VS_Systick
TIM3	PWM Generation CH4	TIM3_CH4	PC9
USART2	Asynchronous	USART2_RX	PA3
USART2	Asynchronous	USART2_TX	PA2



Pin Nb	PINs	FUNCTIONs	LABELs
5	PD0-OSC_IN	RCC_OSC_IN	
6	PD1-OSC_OUT	RCC_OSC_OUT	
16	PA2	USART2_TX	
17	PA3	USART2_RX	
40	PC9	TIM3_CH4	
46	PA13	SYS_JTMS-SWDIO	
49	PA14	SYS_JTCK-SWCLK	
61	PB8	I2C1_SCL	
62	PB9	I2C1_SDA	



SOFTWARE PROJECT

Project Settings : 
Project Name : TCS34725_Color_Sensoc
Project Folder : E:\Project\TCS34725 Color Sensor\code\STM32\STM32F103RBT6
Toolchain / IDE : MDK-ARM V5
Firmware Package Name and Version : STM32Cube FW_F1 V1.6.1


Code Generation Settings : 
STM32Cube Firmware Library Package : Copy all used libraries into the project folder
Generate peripheral initialization as a pair of '.c/.h' files per peripheral : Yes
Backup previously generated files when re-generating : No
Delete previously generated files when not re-generated : Yes
Set all free pins as analog (to optimize the power consumption) : No


Toolchains Settings : 
Compiler Optimizations : Balanced Size/Speed






