Static Call Graph - [TCS34725_Color_Sensoc\TCS34725_Color_Sensoc.axf]

# Static Call Graph for image TCS34725_Color_Sensoc\TCS34725_Color_Sensoc.axf

#<CALLGRAPH># ARM Linker, 5060960: Last Updated: Wed Feb 23 11:10:23 2022

### Maximum Stack Usage = 200 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ TCS34725_Init ⇒ TCS34725_Set_Interrupt_Threshold ⇒ TCS34725_WriteByte ⇒ DEV_I2C_WriteByte ⇒ HAL_I2C_Mem_Write ⇒ I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- _Error_Handler ⇒ _Error_Handler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - BusFault_Handler from stm32f1xx_it.o(i.BusFault_Handler) referenced from startup_stm32f103xb.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DebugMon_Handler from stm32f1xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f103xb.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - FLASH_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - HardFault_Handler from stm32f1xx_it.o(i.HardFault_Handler) referenced from startup_stm32f103xb.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - MemManage_Handler from stm32f1xx_it.o(i.MemManage_Handler) referenced from startup_stm32f103xb.o(RESET)
  - NMI_Handler from stm32f1xx_it.o(i.NMI_Handler) referenced from startup_stm32f103xb.o(RESET)
  - PVD_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - PendSV_Handler from stm32f1xx_it.o(i.PendSV_Handler) referenced from startup_stm32f103xb.o(RESET)
  - RCC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - RTC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - Reset_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SPI1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SPI2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SVC_Handler from stm32f1xx_it.o(i.SVC_Handler) referenced from startup_stm32f103xb.o(RESET)
  - SysTick_Handler from stm32f1xx_it.o(i.SysTick_Handler) referenced from startup_stm32f103xb.o(RESET)
  - SystemInit from system_stm32f1xx.o(i.SystemInit) referenced from startup_stm32f103xb.o(.text)
  - TAMPER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USART1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USART2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USART3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - UsageFault_Handler from stm32f1xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f103xb.o(RESET)
  - WWDG_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f103xb.o(.text)
  - fputc from dev_config.o(i.fputc) referenced from printf5.o(i.__0printf$5)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_lib_shutdown_fini (Thumb, 0 bytes, Stack size unknown bytes, entry12b.o(.ARM.Collect$$$$0000000E))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000F))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$00000011))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __aeabi_fdiv (Thumb, 124 bytes, Stack size 8 bytes, fdiv.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_fdiv
  [Calls]
  - >> _float_round
  [Called By]
  - >> TCS34725_GetRGB888
  - >> TCS34725_GetRGB565

  __aeabi_ui2f (Thumb, 10 bytes, Stack size 0 bytes, ffltui.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_ui2f ⇒ _float_epilogue
  [Calls]
  - >> _float_epilogue
  [Called By]
  - >> TCS34725_GetRGB888
  - >> TCS34725_GetRGB565

  __aeabi_f2uiz (Thumb, 40 bytes, Stack size 0 bytes, ffixui.o(.text))
  [Called By]

  - >> TCS34725_GetRGB888
  - >> TCS34725_GetRGB565

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __I$use$fp (Thumb, 0 bytes, Stack size 0 bytes, iusefp.o(.text), UNUSED)

  _float_round (Thumb, 18 bytes, Stack size 0 bytes, fepilogue.o(.text))
  [Called By]

  - >> __aeabi_fdiv

  _float_epilogue (Thumb, 92 bytes, Stack size 4 bytes, fepilogue.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = _float_epilogue
  [Called By]
  - >> __aeabi_ui2f

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  DEV_I2C_ReadByte (Thumb, 38 bytes, Stack size 24 bytes, dev_config.o(i.DEV_I2C_ReadByte))
  [Stack]

  - Max Depth = 160
  - Call Chain = DEV_I2C_ReadByte ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_I2C_Mem_Read
  [Called By]
  - >> TCS34725_ReadByte

  DEV_I2C_ReadWord (Thumb, 38 bytes, Stack size 24 bytes, dev_config.o(i.DEV_I2C_ReadWord))
  [Stack]

  - Max Depth = 160
  - Call Chain = DEV_I2C_ReadWord ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_I2C_Mem_Read
  [Called By]
  - >> TCS34725_ReadWord

  DEV_I2C_WriteByte (Thumb, 36 bytes, Stack size 24 bytes, dev_config.o(i.DEV_I2C_WriteByte))
  [Stack]

  - Max Depth = 152
  - Call Chain = DEV_I2C_WriteByte ⇒ HAL_I2C_Mem_Write ⇒ I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_I2C_Mem_Write
  [Called By]
  - >> TCS34725_WriteByte

  DEV_Set_I2CAddress (Thumb, 6 bytes, Stack size 0 bytes, dev_config.o(i.DEV_Set_I2CAddress))
  [Called By]

  - >> TCS34725_Init

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  HAL_Delay (Thumb, 32 bytes, Stack size 16 bytes, stm32f1xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> TCS34725_Init
  - >> TCS34725_Get_RGBData

  HAL_GPIO_Init (Thumb, 408 bytes, Stack size 40 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> HAL_TIM_MspPostInit
  - >> HAL_I2C_MspInit
  - >> MX_GPIO_Init
  - >> HAL_UART_MspInit

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> I2C_WaitOnTXEFlagUntilTimeout
  - >> I2C_WaitOnRXNEFlagUntilTimeout
  - >> I2C_WaitOnMasterAddressFlagUntilTimeout
  - >> I2C_WaitOnFlagUntilTimeout
  - >> I2C_WaitOnBTFFlagUntilTimeout
  - >> HAL_Delay
  - >> HAL_UART_Transmit
  - >> HAL_I2C_Mem_Write
  - >> HAL_I2C_Mem_Read
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> UART_WaitOnFlagUntilTimeout

  HAL_I2C_Init (Thumb, 302 bytes, Stack size 16 bytes, stm32f1xx_hal_i2c.o(i.HAL_I2C_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_I2C_Init ⇒ HAL_I2C_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_RCC_GetPCLK1Freq
  - >> HAL_I2C_MspInit
  [Called By]
  - >> MX_I2C1_Init

  HAL_I2C_Mem_Read (Thumb, 530 bytes, Stack size 64 bytes, stm32f1xx_hal_i2c.o(i.HAL_I2C_Mem_Read))
  [Stack]

  - Max Depth = 136
  - Call Chain = HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> I2C_WaitOnRXNEFlagUntilTimeout
  - >> I2C_WaitOnFlagUntilTimeout
  - >> I2C_RequestMemoryRead
  [Called By]
  - >> DEV_I2C_ReadWord
  - >> DEV_I2C_ReadByte

  HAL_I2C_Mem_Write (Thumb, 306 bytes, Stack size 64 bytes, stm32f1xx_hal_i2c.o(i.HAL_I2C_Mem_Write))
  [Stack]

  - Max Depth = 128
  - Call Chain = HAL_I2C_Mem_Write ⇒ I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> I2C_WaitOnTXEFlagUntilTimeout
  - >> I2C_WaitOnFlagUntilTimeout
  - >> I2C_WaitOnBTFFlagUntilTimeout
  - >> I2C_RequestMemoryWrite
  [Called By]
  - >> DEV_I2C_WriteByte

  HAL_I2C_MspInit (Thumb, 70 bytes, Stack size 24 bytes, i2c.o(i.HAL_I2C_MspInit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_I2C_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_I2C_Init

  HAL_IncTick (Thumb, 12 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 32 bytes, Stack size 8 bytes, stm32f1xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_InitTick
  - >> HAL_MspInit
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 54 bytes, Stack size 16 bytes, stm32f1xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 118 bytes, Stack size 8 bytes, stm32f1xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_Init

  HAL_NVIC_SetPriority (Thumb, 60 bytes, Stack size 16 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> SystemClock_Config
  - >> HAL_MspInit

  HAL_NVIC_SetPriorityGrouping (Thumb, 26 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_MspInit
  - >> HAL_Init

  HAL_RCC_ClockConfig (Thumb, 322 bytes, Stack size 32 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_GetTick
  - >> HAL_InitTick
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Called By]

  - >> SystemClock_Config

  HAL_RCC_GetPCLK1Freq (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Called By]

  - >> HAL_I2C_Init
  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Called By]

  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 74 bytes, Stack size 20 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_ClockConfig

  HAL_RCC_OscConfig (Thumb, 750 bytes, Stack size 40 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SYSTICK_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_CLKSourceConfig))
  [Called By]

  - >> SystemClock_Config

  HAL_SYSTICK_Callback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Callback))
  [Called By]

  - >> HAL_SYSTICK_IRQHandler

  HAL_SYSTICK_Config (Thumb, 40 bytes, Stack size 8 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_Config
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> SystemClock_Config

  HAL_SYSTICK_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_Callback
  [Called By]
  - >> SysTick_Handler

  HAL_TIMEx_MasterConfigSynchronization (Thumb, 80 bytes, Stack size 12 bytes, stm32f1xx_hal_tim_ex.o(i.HAL_TIMEx_MasterConfigSynchronization))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> MX_TIM2_Init

  HAL_TIM_MspPostInit (Thumb, 50 bytes, Stack size 24 bytes, tim.o(i.HAL_TIM_MspPostInit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> MX_TIM2_Init

  HAL_TIM_PWM_ConfigChannel (Thumb, 208 bytes, Stack size 16 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_ConfigChannel))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_PWM_ConfigChannel ⇒ TIM_OC2_SetConfig
  [Calls]
  - >> TIM_OC2_SetConfig
  - >> TIM_OC4_SetConfig
  - >> TIM_OC3_SetConfig
  - >> TIM_OC1_SetConfig
  [Called By]
  - >> MX_TIM2_Init

  HAL_TIM_PWM_Init (Thumb, 54 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_Init))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_PWM_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> TIM_Base_SetConfig
  - >> HAL_TIM_PWM_MspInit
  [Called By]
  - >> MX_TIM2_Init

  HAL_TIM_PWM_MspInit (Thumb, 30 bytes, Stack size 8 bytes, tim.o(i.HAL_TIM_PWM_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_TIM_PWM_MspInit
  [Called By]
  - >> HAL_TIM_PWM_Init

  HAL_TIM_PWM_Start (Thumb, 42 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_Start))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_TIM_PWM_Start ⇒ TIM_CCxChannelCmd
  [Calls]
  - >> TIM_CCxChannelCmd
  [Called By]
  - >> main

  HAL_UART_Init (Thumb, 98 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  [Called By]
  - >> MX_USART2_UART_Init

  HAL_UART_MspInit (Thumb, 74 bytes, Stack size 32 bytes, usart.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_Init

  HAL_UART_Transmit (Thumb, 186 bytes, Stack size 32 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Transmit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> fputc

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  MX_GPIO_Init (Thumb, 78 bytes, Stack size 24 bytes, gpio.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 64
  - Call Chain = MX_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> main

  MX_I2C1_Init (Thumb, 54 bytes, Stack size 8 bytes, i2c.o(i.MX_I2C1_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = MX_I2C1_Init ⇒ HAL_I2C_Init ⇒ HAL_I2C_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_I2C_Init
  - >> _Error_Handler
  [Called By]
  - >> main

  MX_TIM2_Init (Thumb, 108 bytes, Stack size 48 bytes, tim.o(i.MX_TIM2_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = MX_TIM2_Init ⇒ HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_TIMEx_MasterConfigSynchronization
  - >> HAL_TIM_MspPostInit
  - >> _Error_Handler
  - >> HAL_TIM_PWM_Init
  - >> HAL_TIM_PWM_ConfigChannel
  [Called By]
  - >> main

  MX_USART2_UART_Init (Thumb, 52 bytes, Stack size 8 bytes, usart.o(i.MX_USART2_UART_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = MX_USART2_UART_Init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> _Error_Handler
  - >> HAL_UART_Init
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SysTick_Handler (Thumb, 14 bytes, Stack size 8 bytes, stm32f1xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_IRQHandler
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  SystemClock_Config (Thumb, 104 bytes, Stack size 72 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 136
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_SYSTICK_CLKSourceConfig
  - >> HAL_NVIC_SetPriority
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_RCC_ClockConfig
  [Called By]
  - >> main

  SystemInit (Thumb, 56 bytes, Stack size 0 bytes, system_stm32f1xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(.text)

  TCS34725_GetRGB565 (Thumb, 266 bytes, Stack size 32 bytes, tcs34725.o(i.TCS34725_GetRGB565))
  [Stack]

  - Max Depth = 40
  - Call Chain = TCS34725_GetRGB565 ⇒ __aeabi_fdiv
  [Calls]
  - >> __aeabi_ui2f
  - >> __aeabi_fdiv
  - >> __aeabi_f2uiz
  [Called By]
  - >> main

  TCS34725_GetRGB888 (Thumb, 266 bytes, Stack size 32 bytes, tcs34725.o(i.TCS34725_GetRGB888))
  [Stack]

  - Max Depth = 40
  - Call Chain = TCS34725_GetRGB888 ⇒ __aeabi_fdiv
  [Calls]
  - >> __aeabi_ui2f
  - >> __aeabi_fdiv
  - >> __aeabi_f2uiz
  [Called By]
  - >> main

  TCS34725_Get_RGBData (Thumb, 108 bytes, Stack size 16 bytes, tcs34725.o(i.TCS34725_Get_RGBData))
  [Stack]

  - Max Depth = 176
  - Call Chain = TCS34725_Get_RGBData ⇒ TCS34725_ReadWord ⇒ DEV_I2C_ReadWord ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_Delay
  - >> TCS34725_ReadWord
  [Called By]
  - >> main

  TCS34725_Init (Thumb, 116 bytes, Stack size 8 bytes, tcs34725.o(i.TCS34725_Init))
  [Stack]

  - Max Depth = 176
  - Call Chain = TCS34725_Init ⇒ TCS34725_Set_Interrupt_Threshold ⇒ TCS34725_WriteByte ⇒ DEV_I2C_WriteByte ⇒ HAL_I2C_Mem_Write ⇒ I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_Delay
  - >> TCS34725_Set_Integration_Time
  - >> TCS34725_Set_Gain
  - >> TCS34725_SetLight
  - >> TCS34725_WriteByte
  - >> TCS34725_Set_Interrupt_Threshold
  - >> TCS34725_Set_Interrupt_Persistence_Reg
  - >> TCS34725_ReadByte
  - >> DEV_Set_I2CAddress
  [Called By]
  - >> main

  TCS34725_SetLight (Thumb, 24 bytes, Stack size 0 bytes, tcs34725.o(i.TCS34725_SetLight))
  [Called By]

  - >> TCS34725_Init

  TCS34725_Set_Gain (Thumb, 18 bytes, Stack size 8 bytes, tcs34725.o(i.TCS34725_Set_Gain))
  [Stack]

  - Max Depth = 160
  - Call Chain = TCS34725_Set_Gain ⇒ TCS34725_WriteByte ⇒ DEV_I2C_WriteByte ⇒ HAL_I2C_Mem_Write ⇒ I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> TCS34725_WriteByte
  [Called By]
  - >> TCS34725_Init

  TCS34725_Set_Integration_Time (Thumb, 18 bytes, Stack size 8 bytes, tcs34725.o(i.TCS34725_Set_Integration_Time))
  [Stack]

  - Max Depth = 160
  - Call Chain = TCS34725_Set_Integration_Time ⇒ TCS34725_WriteByte ⇒ DEV_I2C_WriteByte ⇒ HAL_I2C_Mem_Write ⇒ I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> TCS34725_WriteByte
  [Called By]
  - >> TCS34725_Init

  TIM_Base_SetConfig (Thumb, 94 bytes, Stack size 20 bytes, stm32f1xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_Init

  TIM_CCxChannelCmd (Thumb, 22 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_CCxChannelCmd))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_CCxChannelCmd
  [Called By]
  - >> HAL_TIM_PWM_Start

  TIM_OC2_SetConfig (Thumb, 84 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC2_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC2_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  _Error_Handler (Thumb, 2 bytes, Stack size 0 bytes, main.o(i._Error_Handler))
  [Calls]

  - >> _Error_Handler
  [Called By]
  - >> MX_TIM2_Init
  - >> MX_I2C1_Init
  - >> _Error_Handler
  - >> MX_USART2_UART_Init

  __0printf$5 (Thumb, 22 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$5 (Thumb, 0 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> main

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  fputc (Thumb, 20 bytes, Stack size 16 bytes, dev_config.o(i.fputc))
  [Stack]

  - Max Depth = 72
  - Call Chain = fputc ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  [Address Reference Count : 1]
  - printf5.o(i.__0printf$5)

  main (Thumb, 114 bytes, Stack size 24 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 200
  - Call Chain = main ⇒ TCS34725_Init ⇒ TCS34725_Set_Interrupt_Threshold ⇒ TCS34725_WriteByte ⇒ DEV_I2C_WriteByte ⇒ HAL_I2C_Mem_Write ⇒ I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> TCS34725_Init
  - >> TCS34725_Get_RGBData
  - >> TCS34725_GetRGB888
  - >> TCS34725_GetRGB565
  - >> MX_TIM2_Init
  - >> SystemClock_Config
  - >> MX_I2C1_Init
  - >> MX_GPIO_Init
  - >> MX_USART2_UART_Init
  - >> HAL_Init
  - >> HAL_TIM_PWM_Start
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  TCS34725_ReadByte (Thumb, 8 bytes, Stack size 0 bytes, tcs34725.o(i.TCS34725_ReadByte))
  [Stack]

  - Max Depth = 160
  - Call Chain = TCS34725_ReadByte ⇒ DEV_I2C_ReadByte ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> DEV_I2C_ReadByte
  [Called By]
  - >> TCS34725_Init

  TCS34725_ReadWord (Thumb, 8 bytes, Stack size 0 bytes, tcs34725.o(i.TCS34725_ReadWord))
  [Stack]

  - Max Depth = 160
  - Call Chain = TCS34725_ReadWord ⇒ DEV_I2C_ReadWord ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> DEV_I2C_ReadWord
  [Called By]
  - >> TCS34725_Get_RGBData

  TCS34725_Set_Interrupt_Persistence_Reg (Thumb, 16 bytes, Stack size 0 bytes, tcs34725.o(i.TCS34725_Set_Interrupt_Persistence_Reg))
  [Stack]

  - Max Depth = 152
  - Call Chain = TCS34725_Set_Interrupt_Persistence_Reg ⇒ TCS34725_WriteByte ⇒ DEV_I2C_WriteByte ⇒ HAL_I2C_Mem_Write ⇒ I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> TCS34725_WriteByte
  [Called By]
  - >> TCS34725_Init

  TCS34725_Set_Interrupt_Threshold (Thumb, 42 bytes, Stack size 16 bytes, tcs34725.o(i.TCS34725_Set_Interrupt_Threshold))
  [Stack]

  - Max Depth = 168
  - Call Chain = TCS34725_Set_Interrupt_Threshold ⇒ TCS34725_WriteByte ⇒ DEV_I2C_WriteByte ⇒ HAL_I2C_Mem_Write ⇒ I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> TCS34725_WriteByte
  [Called By]
  - >> TCS34725_Init

  TCS34725_WriteByte (Thumb, 8 bytes, Stack size 0 bytes, tcs34725.o(i.TCS34725_WriteByte))
  [Stack]

  - Max Depth = 152
  - Call Chain = TCS34725_WriteByte ⇒ DEV_I2C_WriteByte ⇒ HAL_I2C_Mem_Write ⇒ I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> DEV_I2C_WriteByte
  [Called By]
  - >> TCS34725_Set_Integration_Time
  - >> TCS34725_Set_Gain
  - >> TCS34725_Init
  - >> TCS34725_Set_Interrupt_Threshold
  - >> TCS34725_Set_Interrupt_Persistence_Reg

  I2C_IsAcknowledgeFailed (Thumb, 40 bytes, Stack size 0 bytes, stm32f1xx_hal_i2c.o(i.I2C_IsAcknowledgeFailed))
  [Called By]

  - >> I2C_WaitOnTXEFlagUntilTimeout
  - >> I2C_WaitOnBTFFlagUntilTimeout

  I2C_RequestMemoryRead (Thumb, 240 bytes, Stack size 40 bytes, stm32f1xx_hal_i2c.o(i.I2C_RequestMemoryRead))
  [Stack]

  - Max Depth = 72
  - Call Chain = I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> I2C_WaitOnTXEFlagUntilTimeout
  - >> I2C_WaitOnMasterAddressFlagUntilTimeout
  - >> I2C_WaitOnFlagUntilTimeout
  [Called By]
  - >> HAL_I2C_Mem_Read

  I2C_RequestMemoryWrite (Thumb, 156 bytes, Stack size 32 bytes, stm32f1xx_hal_i2c.o(i.I2C_RequestMemoryWrite))
  [Stack]

  - Max Depth = 64
  - Call Chain = I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> I2C_WaitOnTXEFlagUntilTimeout
  - >> I2C_WaitOnMasterAddressFlagUntilTimeout
  - >> I2C_WaitOnFlagUntilTimeout
  [Called By]
  - >> HAL_I2C_Mem_Write

  I2C_WaitOnBTFFlagUntilTimeout (Thumb, 78 bytes, Stack size 16 bytes, stm32f1xx_hal_i2c.o(i.I2C_WaitOnBTFFlagUntilTimeout))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_WaitOnBTFFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> I2C_IsAcknowledgeFailed
  [Called By]
  - >> HAL_I2C_Mem_Write

  I2C_WaitOnFlagUntilTimeout (Thumb, 96 bytes, Stack size 32 bytes, stm32f1xx_hal_i2c.o(i.I2C_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 32
  - Call Chain = I2C_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> I2C_RequestMemoryWrite
  - >> I2C_RequestMemoryRead
  - >> HAL_I2C_Mem_Write
  - >> HAL_I2C_Mem_Read

  I2C_WaitOnMasterAddressFlagUntilTimeout (Thumb, 136 bytes, Stack size 32 bytes, stm32f1xx_hal_i2c.o(i.I2C_WaitOnMasterAddressFlagUntilTimeout))
  [Stack]

  - Max Depth = 32
  - Call Chain = I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> I2C_RequestMemoryWrite
  - >> I2C_RequestMemoryRead

  I2C_WaitOnRXNEFlagUntilTimeout (Thumb, 98 bytes, Stack size 24 bytes, stm32f1xx_hal_i2c.o(i.I2C_WaitOnRXNEFlagUntilTimeout))
  [Stack]

  - Max Depth = 24
  - Call Chain = I2C_WaitOnRXNEFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_I2C_Mem_Read

  I2C_WaitOnTXEFlagUntilTimeout (Thumb, 78 bytes, Stack size 16 bytes, stm32f1xx_hal_i2c.o(i.I2C_WaitOnTXEFlagUntilTimeout))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_WaitOnTXEFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> I2C_IsAcknowledgeFailed
  [Called By]
  - >> I2C_RequestMemoryWrite
  - >> I2C_RequestMemoryRead
  - >> HAL_I2C_Mem_Write

  NVIC_SetPriority (Thumb, 32 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.NVIC_SetPriority))
  [Called By]

  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority

  TIM_OC1_SetConfig (Thumb, 74 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC1_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC1_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  TIM_OC3_SetConfig (Thumb, 82 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC3_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC3_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  TIM_OC4_SetConfig (Thumb, 64 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC4_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC4_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  UART_SetConfig (Thumb, 364 bytes, Stack size 24 bytes, stm32f1xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_SetConfig
  [Calls]
  - >> HAL_RCC_GetPCLK1Freq
  - >> HAL_RCC_GetPCLK2Freq
  [Called By]
  - >> HAL_UART_Init

  UART_WaitOnFlagUntilTimeout (Thumb, 100 bytes, Stack size 24 bytes, stm32f1xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_UART_Transmit

  _printf_core (Thumb, 660 bytes, Stack size 104 bytes, printf5.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  [Called By]
  - >> __0printf$5

  ### Undefined Global Symbols