#,0# rev, program, local device, distant device, status
#,1# (to sort easily: sort -k2 -t, manual-test-results.txt)
#,2######################################################
r736, nfc-anticol, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, DESfire, OK
r736, nfc-anticol, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, MFC, OK
r736, nfc-anticol, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, UL, OK
r846, nfc-anticol, ARYGON 00V5.1 (/dev/ttyUSB0) - PN532 v1.4 (APDB2UA33), MFC, OK
r736, nfc-anticol, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, DESfire, OK
r736, nfc-anticol, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, MFC, OK
r736, nfc-anticol, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, UL, OK
r1013, nfc-anticol, ASK / LoGO - PN533 v2.7, DESfire, OK
r1013, nfc-anticol, ASK / LoGO - PN533 v2.7, MFC, OK
r1013, nfc-anticol, ASK / LoGO - PN533 v2.7, UL, OK
r1013, nfc-anticol, ASK / LoGO - PN533 v2.7, ULC, OK
r736, nfc-dep-initiator, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, ACS ACR 38U-CCID 00 00 / ACR122U102 - PN532 v1.4, OK
r1036, nfc-dep-initiator, ASK / LoGO - PN533 v2.7, Nokia 6212 Classic, OK
r736, nfc-dep-target, ACS ACR 38U-CCID 00 00 / ACR122U102 - PN532 v1.4, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, OK
r1036, nfc-dep-target, ASK / LoGO - PN533 v2.7, Nokia 6212 Classic, OK but USB device is not reacheable after that
r736, nfc-emulate-forum-tag4, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, ctrl-c & use, FAIL
r744, nfc-emulate-forum-tag4, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, Nokia 6131 NFC, OK
r736, nfc-emulate-forum-tag4, ACS ACR 38U-CCID 00 00 / ACR122U102 - PN532 v1.4, Nokia 6212 Classic, OK
r744, nfc-emulate-tag, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, Cardman 5321, OK
r744, nfc-emulate-tag, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, CardMan 5321, OK
r736, nfc-emulate-tag, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, ctrl-c & use, FAIL
r736, nfc-emulate-tag, ACS ACR 38U-CCID 00 00 / ACR122U102 - PN532 v1.4, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, OK
r736, nfc-emulate-tag, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, ACS ACR 38U-CCID 00 00 / ACR122U102 - PN532 v1.4, OK
r736, nfc-emulate-tag, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, ctrl-c & use, OK
r736, nfc-emulate-uid, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, ctrl-c & use, FAIL
r744, nfc-emulate-uid, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, emulate + ctrl-c & use, FAIL
r736, nfc-emulate-uid, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4 + nfc-anticol 2x, OK
r736, nfc-emulate-uid, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, ctrl-c & use, OK
r736, nfc-list, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, 2 DESfire, OK
r736, nfc-list, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, 2 UL, OK
r736, nfc-list, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, JCOP, OK
r736, nfc-list, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, MFC, OK
r736, nfc-list, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, topaz, OK
r736, nfc-list, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, typeB Calypso, OK
r736, nfc-list, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, ULC, OK
r736, nfc-list, ACS ACR 38U-CCID 00 00 / ACR122U102 - PN532 v1.4, DESFire, OK
r846, nfc-list, ARYGON 00V5.1 (/dev/ttyUSB0) - PN532 v1.4 (APDB2UA33), MFC, OK
r736, nfc-list, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, 2 DESfire, OK
r736, nfc-list, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, 2 UL, OK
r736, nfc-list, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, DESFire, OK
r736, nfc-list, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, JCOP, OK
r736, nfc-list, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, MFC, OK
r736, nfc-list, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, topaz, OK
r736, nfc-list, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, typeB Calypso, OK
r736, nfc-list, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, ULC, OK
r1013, nfc-list, ASK / LoGO - PN533 v2.7, DESfire, OK
r1013, nfc-list, ASK / LoGO - PN533 v2.7, MFC, OK
r1013, nfc-list, ASK / LoGO - PN533 v2.7, UL, OK
r1013, nfc-list, ASK / LoGO - PN533 v2.7, ULC, OK 
r1036, nfc-list, ASK / LoGO - PN533 v2.7, DESFire, OK 
r736, nfc-mfclassic r a foo, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, MFC, OK
r846, nfc-mfclassic r a foo, ARYGON 00V5.1 (/dev/ttyUSB0) - PN532 v1.4 (APDB2UA33), MFC, OK
r736, nfc-mfclassic r a foo, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, MFC, OK
r1013, nfc-mfclassic r a foo, ASK / LoGO - PN533 v2.7, MFC, OK
r736, nfc-mfultralight r foo, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, UL, OK
r736, nfc-mfultralight r foo, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, UL, OK
r1013, nfc-mfultralight r foo, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, UL, OK
r739, nfc-poll, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, 2 DESfire, OK
r739, nfc-poll, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, 2 UL, OK
r739, nfc-poll, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, JCOP, OK
r739, nfc-poll, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, MFC, OK
r739, nfc-poll, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, topaz, OK
r739, nfc-poll, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, typeB Calypso, OK
r739, nfc-poll, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, ULC, OK
r846, nfc-poll, ARYGON 00V5.1 (/dev/ttyUSB0) - PN532 v1.4 (APDB2UA33), MFC, FAIL
r849, nfc-poll, ARYGON 00V5.1 (/dev/ttyUSB0) - PN532 v1.4 (APDB2UA33), MFC, OK
r736, pn53x-diagnose, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, N/A, OK
r736, pn53x-diagnose, ACS ACR 38U-CCID 00 00 / ACR122U102 - PN532 v1.4, N/A, OK
r846, pn53x-diagnose, ARYGON 00V5.1 (/dev/ttyUSB0) - PN532 v1.4 (APDB2UA33), N/A, FAIL
r849, pn53x-diagnose, ARYGON 00V5.1 (/dev/ttyUSB0) - PN532 v1.4 (APDB2UA33), N/A, OK
r736, pn53x-diagnose, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, N/A, OK
r891, pn53x-diagnose, ACS ACR 38U-CCID 00 00 / ACR122U102 - PN532 v1.4, N/A, OK
r891, pn53x-diagnose, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, N/A, OK
r891, pn53x-diagnose, ASK / LoGO - PN533 v2.7, N/A, OK
r1013, pn53x-diagnose, ACS ACR 38U-CCID 00 00 / ACR122U102 - PN532 v1.4, N/A, FAIL
r1013, pn53x-diagnose, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, N/A, FAIL
r1013, pn53x-diagnose, NXP / PN533 - PN533 v2.7, N/A, FAIL
r1013, pn53x-diagnose, ASK / LoGO - PN533 v2.7, N/A, FAIL
r1015, pn53x-diagnose, ASK / LoGO - PN533 v2.7, N/A, OK
r1015, pn53x-diagnose, ACS ACR 38U-CCID 00 00 / ACR122U102 - PN532 v1.4, N/A, OK
r1015, pn53x-diagnose, NXP / PN533 - PN533 v2.7, N/A, OK
r1015, pn53x-diagnose, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, N/A, OK
r744, pn53x-sam (mode 1), Philips / PN531 - PN531 v4.2 + SAM, CardMan 5321, OK
r736, pn53x-tamashell < pn53x-tamashell-scripts/UltraLightRead.cmd, ACS ACR122U PICC Interface 00 00 / ACR122U102 - PN532 v1.4, ultralight, OK
r736, pn53x-tamashell < pn53x-tamashell-scripts/UltraLightRead.cmd, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, UL, OK
r1013, pn53x-tamashell < pn53x-tamashell-scripts/UltraLightRead.cmd, ACS ACR 38U-CCID 00 00 / ACR122U102 - PN532 v1.4,UL, OK
r1013, pn53x-tamashell < pn53x-tamashell-scripts/UltraLightRead.cmd, SCM Micro / SCL3711-NFC&RW - PN533 v2.7, UL, OK
r1013, pn53x-tamashell < pn53x-tamashell-scripts/UltraLightRead.cmd, NXP / PN533 - PN533 v2.7, UL, OK
r1013, pn53x-tamashell < pn53x-tamashell-scripts/UltraLightRead.cmd, ASK / LoGO - PN533 v2.7, UL, FAIL

